-------------------------------------------------------------------------------------------------------------
Release Notice ORION DAQ Driver v2.3.1.0
2018-07-13

* Version:	2.3.1.0

* Components:
** 32-bit DAQ driver 
** 64-bit DAQ driver

* New Features:
** supports Win10 64-bit systems (Winx64)
** supports Win7 32-/64-Bit systems

* Bugfixes:
** FW version number indication fixed for Orion 0816-1000N and Orion 1616-1000 (correct "101", wrong "901")
** ORION co-installer fixed to support Win10x64
** external clocking with DEWE-Clock fixed

* Known Limitation:
** At all times only one instance of the DAQ driver is allowed.
** Installing the driver without Administrator privileges will result in an incorrect installation
** When Orion 1616-50x, Orion 0816-100x or Orion 1616-100x are used in the system, the DMA buffer size has to be adjusted manually in order to support all channels of the cards. For the detailed descritpion please refer to <<Application_Note_64 Bit Driver.pdf>>
** Measurement start: If no CAN frames are received before the internal 24-bit counter overflows (~3 minutes @100 Hz), the overflow is not considered and the CAN timestamps are wrong. Workaround: add a CAN channel that always sends data.  (problem @ BOSCH, will be fixed for ORION and Oxygen, was already fixed for TRION, won´t be fixed for ORION and DS => DS issue)



-------------------------------------------------------------------------------------------------------------
Release Notice ORION DAQ Driver v2.3.0.0
2018-07-09

* Version:	2.3.0.0

* Components:
** 32-bit DAQ driver 
** 64-bit DAQ driver

* New Features:
** supports Win10 64-bit systems (Winx64)
** supports Win7 32-/64-Bit systems

* Bugfixes:
** ORION co-installer fixed to support Win10x64
** external clocking with DEWE-Clock fixed

* Known Limitation:
** At all times only one instance of the DAQ driver is allowed.
** Installing the driver without Administrator privileges will result in an incorrect installation
** When Orion 1616-50x, Orion 0816-100x or Orion 1616-100x are used in the system, the DMA buffer size has to be adjusted manually in order to support all channels of the cards. For the detailed descritpion please refer to <<Application_Note_64 Bit Driver.pdf>>
** Measurement start: If no CAN frames are received before the internal 24-bit counter overflows (~3 minutes @100 Hz), the overflow is not considered and the CAN timestamps are wrong. Workaround: add a CAN channel that always sends data.  (problem @ BOSCH, will be fixed for ORION and Oxygen, was already fixed for TRION, won´t be fixed for ORION and DS => DS issue)



-------------------------------------------------------------------------------------------------------------

Release Notice ORION DAQ Driver v2.1.0.0
2016-11-18

* Version: 2.1.0.0

* Components:
** 32-bit DAQ driver 
** 64-bit DAQ driver

* New Features:
** supports Win7 32-/64-Bit systems

* Bugfixes (Soo-Hong):
** #3624: Win10: installer fails the first time when started without admin rights
** #3623: Win10: driver not uninstalled completely
=> but no Win10 supports due to co-installer issues!!

* Known Limitation:
** At all times only one instance of the DAQ driver is allowed.
** Installing the driver without Administrator privileges will result in an incorrect installation
** When Orion 1616-50x, Orion 0816-100x or Orion 1616-100x are used in the system, the DMA buffer size has to be adjusted manually in order to support all channels of the cards. For the detailed descritpion please refer to <<Application_Note_64 Bit Driver.pdf>>
** Measurement start: If no CAN frames are received before the internal 24-bit counter overflows (~3 minutes @100 Hz), the overflow is not considered and the CAN timestamps are wrong. Workaround: add a CAN channel that always sends data.  (problem @ BOSCH, will be fixed for ORION and Oxygen, was already fixed for TRION, won´t be fixed for ORION and DS => DS issue)

-------------------------------------------------------------------------------------------------------------

Info ORION DAQ Drivers v2.0.0.900 to v2.0.0.904 test versions => not released

ver 2.0.0.900:	<a> A wrong "Over Count" problem still happened after ver2.0.0.11.
				-> So, I seriously considered the main reason why happened and solution how to solve. 
				And I started to try to find any kind of another method, and I changed the test version number as 900.

ver 2.0.0.901:	<a> Found a solution about a wrong "Over Count" problem.
				-> Fixed this problem by changing the management method of "Over Count" and Write Index for DMA.
				Until now, this method works normally. (Actually, I have tested for more than two months…)

ver 2.0.0.902:	<a> Found a wrong channel counter and size for Super Counter channel. 
				It happened only in case of 0816-5M/10M.
				-> Fixed it.

ver 2.0.0.903:	<a> When use the external clock in Dewesoft, it was not working correctly.
				-> The reason is because when use external clock, Dewesoft set the block count to big number, 1472.
				So, changed this block count to fit to Dewesoft.

ver 2.0.0.904:	<a> Found a bug in the Data Read function only for single mode.
				-> Missed to handle the NULL pointer as parameter. So changed it.

-------------------------------------------------------------------------------------------------------------

Release Notice ORION DAQ Driver v2.0.0.12

* Version: 2.0.0.12

	<a> Andreas requested a CAN read function for LabView.
		-> Young-Man added a CAN read function for LabView, RtReadCANLV().

-------------------------------------------------------------------------------------------------------------

Release Notice ORION DAQ Drivers v2.0.0.11

* Version: 2.0.0.11

	<a> Found a wrong "Over Count" behavior of write index for DMA operation in the kernel.
		-> Added some complement codes in the read function and ISR.

	<b> When use CAN and Rs485 concurrently and repeat the acquisition start and stop, 
		frequently CAN data are not transferred correctly.
		-> Fixed by changing the RS485 read method.

-------------------------------------------------------------------------------------------------------------

Info ORION DAQ Drivers v2.0.0.10 => not released

-------------------------------------------------------------------------------------------------------------

Release Notice ORION DAQ Drivers V2.0.0.9

* Version: 2.0.0.9

* Components:
** 32-bit DAQ driver 
** 64-bit DAQ driver

*New Features:
** Issue #396 solved: sometimes DAQ-board with CAN enabled stops to provide data (Rtdaq3 error), when switching between setup and measure screen. Only a reboot solves the issue.

* Known Limitations: 
** At all times only one instance of the DAQ driver is allowed.
** Installing the driver without Administrator privileges will result in an incorrect installation
** When Orion 1616-50x, Orion 0816-100x or Orion 1616-100x are used in the system, the DMA buffer size has to be adjusted manually in order to support all channels of the cards. For the detailed descritpion please refer to <<Application_Note_64 Bit Driver.pdf>>

-------------------------------------------------------------------------------------------------------------

Release Notice ORION DAQ Drivers V2.0.0.8

* Version: 2.0.0.8

* Components:
** 32-bit DAQ driver 
** 64-bit DAQ driver

*New Features:
** Limitation "Orion Cards with CNT expansion and DEWESoft ..." has been resolved

* Known Limitations: 
** At all times only one instance of the DAQ driver is allowed.
** Installing the driver without Administrator privileges will result in an incorrect installation
** When Orion 1616-50x, Orion 0816-100x or Orion 1616-100x are used in the system, the DMA buffer size has to be adjusted manually in order to support all channels of the cards. For the detailed descritpion please refer to <<Application_Note_64 Bit Driver.pdf>>

-------------------------------------------------------------------------------------------------------------

Release Notice ORION DAQ Drivers V2.0.0.7

* Version: 2.0.0.7

* Components:
** 32-bit DAQ driver 
** 64-bit DAQ driver

*New Features:
**none, only re-compiled with correct version info

* Known Limitations: 
** At all times only one instance of the DAQ driver is allowed.
** Installing the driver without Administrator privileges will result in an incorrect installation
** When Orion 1616-50x, Orion 0816-100x or Orion 1616-100x are used in the system, the DMA buffer size has to be adjusted manually in order to support all channels of the cards. For the detailed descritpion please refer to <<Application_Note_64 Bit Driver.pdf>>
** Orion Cards with CNT expansion will cause an ACCESS VIOLATION in Dewesoft.exe if the two Counter of the the "base" Orion Card are disabled whilst the CNT of the Expansion are enabled

-------------------------------------------------------------------------------------------------------------