+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2018-12-20 Release Notice DEWETRON TRION API R2.5.2 Legacy

* Version: 	2.5.48441.00 (Rev.: d6246370f569765bb764b063a172e3aa84a6ec70)

* Components:
** DEWE2 Explorer                       2.5.48441.00
** DEWE-TRION application library       2.5.48441.00
** DEWE-TRION system driver             2.5.48441.00
** DEWE2 enclosure access               2.5.48441.00
** DEWE-TRION board information         $Revision: 1507299269
** DEWE2 enclosure information          $Revision: 1502272020
** DEWE-TRION firmware revisions        $Revision: 1508496979
** DEWE-TRION TEDS default data			$Revision: 1500988820

* Files:
** DEWETRON-TRION-Applications-x64.exe
** DEWETRON-TRION-Applications-x86.exe

* New Features and most important bugfixes:
** Fixed: #6242 PPS sync mode - async timestamping startup-behaviour (DS only)

* Requirements:
** Use this package if x86 architecture (32bit) or DEWESoft is required
** In all other cases use latest TRION API (R3.x)
** Update all Trion modules to the firmware included in this release
** Use DEWESoft 7.1.3 b408
** Windows 10 64-Bit or Windows 7 64/32-Bit

* Installation procedure:
** Uninstall any previous TRION version via system uninstall (control panel - TRION Applications)
** Reboot system
** Install TRION applications
** Reboot system
** Start DEWE2Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
** Power-cycle TRION boards (Power down system, then restart)

* Known Limitations:
** DS: #3584 temperature measurement with PT100 sensor only valid till < 300°C (above linearization problems)

* HW Support TRION modules:
** TRION-1620-ACC-6-BNC			FW: x0031
** TRION-1620-ACC-6-L1B			FW: x0031
** TRION-1620-LV-6-BNC			FW: x0031
** TRION-1620-LV-6-L1B			FW: x0031
** TRION-1603-LV-6-BNC			FW: x0A15
** TRION-1603-LV-6-L1B			FW: x0A15
** TRION-1603-LV-6-D25			FW: x0A15
** TRION-1600-dLV-16-D			FW: x187E
** TRION-1600-dLV-16-D-CAN		FW: x187E
** TRION-1600-dLV-32-D			FW: x187E
** TRION-1600-dLV-32-D-CAN		FW: x187E
** TRION-1802-dLV-16-D			FW: x187E
** TRION-1802-dLV-16-D-CAN		FW: x187E
** TRION-1802-dLV-32-D			FW: x187E
** TRION-1802-dLV-32-D-CAN		FW: x187E
** TRION-1820-POWER-8			FW: x0035
** TRION-1810M-POWER-8			FW: x0035
** TRION-2402-MULTI-4-D			FW: x0B18
** TRION-2402-MULTI-8-L0B		FW: x0A23
** TRION-2402-MULTI-S1			FW: x0034
** TRION-2402-dSTG-6-L1B		FW: x1120
** TRION-2402-dSTG-6-L1B-S1		FW: x1120
** TRION-2402-dSTG-8-D			FW: x1120
** TRION-2402-dSTG-8-L0B		FW: x1120
** TRION-2402-dSTG-8-RJ			FW: x1120
** TRION-2400-dSTG-8-L0B		FW: x1120
** TRION-2400-dSTG-OEM			FW: x1120
** TRION-2402-dACC-6-BNC		FW: x1119
** TRION-2402-dACC-8-SMB		FW: x1119
** TRION-2402-dACC-8-MD			FW: x1119
** TRION-2402-V-4-B				FW: x1017
** TRION-2402-V-8-B				FW: x1017
** TRION-CNT-6-L1B				FW: x1119
** TRION-BASE					FW: x1144
** TRION-TIMING					FW: x1144
** TRION-TIMING-V2				FW: x0002
** TRION-VGPS-20				FW: x1144
** TRION-VGPS-100				FW: x1144
** TRION-CAN-4					FW: x1121
** TRION-CAN-2					FW: x1121
** TRION-DI-48					FW: x1119
** TRION-DI-64-S1				FW: x0009

* HW Support DEWE2 chassis:
** DEWE2-PA7
** DEWE2-A4
** DEWE2-A4L
** DEWE2-A7
** DEWE2-A13
** DEWE2-M4
** DEWE2-M4s
** DEWE2-M7
** DEWE2-M7s
** DEWE2-M13
** DEWE2-M13s
** DEWE2-M18
** DEWE2-F4s
** DEWE2-F7s
** DEWE2-F13s
** DEWE2-F18
** DEWE2-F4-THUNDERBOLT
** DEWE2-F13-FIBRE
** TRIONet
** TrendCorder


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2017-10-25 Release Notice DEWETRON TRION API R2.5.1

* Version: 	2.5.38306.00 (Rev.: db23169e7385993b0c27e542c0508a8e60fe5da6)

* Components:
** DEWE2 Explorer                       2.5.38306.00
** DEWE-TRION application library       2.5.38306.00
** DEWE-TRION system driver             2.5.38306.00
** DEWE2 enclosure access               2.5.38306.00
** DEWE-TRION board information         $Revision: 1507299269
** DEWE2 enclosure information          $Revision: 1502272020
** DEWE-TRION firmware revisions        $Revision: 1508496979
** DEWE-TRION TEDS default data			$Revision: 1500988820

* Files:
** DEWETRON-TRION-Applications-x64.exe
** DEWETRON-TRION-Applications-x86.exe

* Requirements:
** Update all Trion modules to the latest firmware included in this release
** Use Oxygen R2.5.1
** Use DEWESoft 7.1.3_b408
** Windows 10 64-Bit or Windows 7 64/32-Bit

* Installation procedure:
** Uninstall any previous TRION version via system uninstall (control panel - TRION Applications)
** Reboot system
** Install TRION applications
** Reboot system
** Start DEWE2Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
** Power-cycle TRION boards (Power down system, then restart)

* New Features and most important bugfixes:
** basic support of TRION-1820-POWER-8 module for Oxygen (will not be supported in DEWESoft at all)
** basic support of TRION-1810M-POWER-8 module for Oxygen (will not be supported in DEWESoft at all)

* Known Limitations:
** Each enclosure must have a unique serial number, else Oxygen will not start.
** DS only: #3584 temperature measurement with PT100 sensor only valid till < 300°C (above linearization problems)

* HW Support TRION modules:
** TRION-1620-ACC-6-BNC			FW: x0031
** TRION-1620-ACC-6-L1B			FW: x0031
** TRION-1620-LV-6-BNC			FW: x0031
** TRION-1620-LV-6-L1B			FW: x0031
** TRION-1603-LV-6-BNC			FW: x0A15
** TRION-1603-LV-6-L1B			FW: x0A15
** TRION-1603-LV-6-D25			FW: x0A15
** TRION-1600-dLV-16-D			FW: x187E
** TRION-1600-dLV-16-D-CAN		FW: x187E
** TRION-1600-dLV-32-D			FW: x187E
** TRION-1600-dLV-32-D-CAN		FW: x187E
** TRION-1802-dLV-16-D			FW: x187E
** TRION-1802-dLV-16-D-CAN		FW: x187E
** TRION-1802-dLV-32-D			FW: x187E
** TRION-1802-dLV-32-D-CAN		FW: x187E
** TRION-1820-POWER-8			FW: x0035
** TRION-1810M-POWER-8			FW: x0035
** TRION-2402-MULTI-4-D			FW: x0B18
** TRION-2402-MULTI-8-L0B		FW: x0A23
** TRION-2402-MULTI-S1			FW: x0034
** TRION-2402-dSTG-6-L1B		FW: x1120
** TRION-2402-dSTG-6-L1B-S1		FW: x1120
** TRION-2402-dSTG-8-D			FW: x1120
** TRION-2402-dSTG-8-L0B		FW: x1120
** TRION-2402-dSTG-8-RJ			FW: x1120
** TRION-2400-dSTG-8-L0B		FW: x1120
** TRION-2400-dSTG-OEM			FW: x1120
** TRION-2402-dACC-6-BNC		FW: x1119
** TRION-2402-dACC-8-SMB		FW: x1119
** TRION-2402-dACC-8-MD			FW: x1119
** TRION-2402-V-4-B				FW: x1017
** TRION-2402-V-8-B				FW: x1017
** TRION-CNT-6-L1B				FW: x1119
** TRION-BASE					FW: x1144
** TRION-TIMING					FW: x1144
** TRION-TIMING-V2				FW: x0002
** TRION-VGPS-20				FW: x1144
** TRION-VGPS-100				FW: x1144
** TRION-CAN-4					FW: x1121
** TRION-CAN-2					FW: x1121
** TRION-DI-48					FW: x1119
** TRION-DI-64-S1				FW: x0009

* HW Support DEWE2 chassis:
** DEWE2-PA7
** DEWE2-A4
** DEWE2-A4L
** DEWE2-A7
** DEWE2-A13
** DEWE2-M4
** DEWE2-M4s
** DEWE2-M7
** DEWE2-M7s
** DEWE2-M13
** DEWE2-M13s
** DEWE2-M18
** DEWE2-F4s
** DEWE2-F7s
** DEWE2-F13s
** DEWE2-F18
** DEWE2-F4-THUNDERBOLT
** DEWE2-F13-FIBRE
** TRIONet
** TrendCorder


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2017-09-04 Release Notice DEWETRON TRION API R2.5

* Version: 	2.5.36942.00 (Rev.: 3e332bd0badcb8035a2c5d7f25ed15350d83cf80)

* Components:
** DEWE2 Explorer                       2.5.36942.00
** DEWE-TRION application library       2.5.36942.00
** DEWE-TRION system driver             2.5.36942.00
** DEWE2 enclosure access               2.5.36942.00
** DEWE-TRION board information         $Revision: 1504005430
** DEWE2 enclosure information          $Revision: 1502272020
** DEWE-TRION firmware revisions        $Revision: 1503497080
** DEWE-TRION TEDS default data			$Revision: 1500988820

* Files:
** DEWETRON-TRION-Applications-x64.exe

* Requirements:
** Update all Trion modules to the latest firmware included in this release
** Use Oxygen R2.5
** Use DEWESoft 7.1.3_b408 or later
** Windows 10 64-Bit or Windows 7 64-Bit (32-Bit only on special demand)

* Installation procedure:
** Uninstall any previous TRION version via system uninstall (control panel)
** Reboot system
** Install TRION applications
** Reboot system
** Start DEWE2Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
** Power-cycle TRION boards (Power down system, then restart)

* New Features and most important bugfixes:
** support of TRION-1600-dLV module
** support of TRION-1802-dLV module
** support of TRION-TIMING V2 module
** support of DEWE2-PA7 chassis
** DEWE2Explorer: added channel configuration for TRION-1802-dLV / TRION-1600-dLV module (16 diff or 32 SE)
** DEWE2Explorer: improved internal configuration possibilities for new TRION modules
** TRION-CAL server: re-factured to fully support TRION module series
** new TRION board driver supporting AVALON platform
** fixed scan descripter (v2)
** improved internal overall test coverage
** enhanced debug information for new TRION board driver for easier support
** TRION-MULTI-2402-x: #4567 RTD measurement 3-wire connection shows wrong values - fixed

* Known Limitations:
** Each enclosure must have a unique serial number, else Oxygen will not start.
** DS only: #3584 temperature measurement with PT100 sensor only valid till < 300°C (above linearization problems)

* HW Support TRION modules:
** TRION-1620-ACC-6-BNC			FW: x0031
** TRION-1620-ACC-6-L1B			FW: x0031
** TRION-1620-LV-6-BNC			FW: x0031
** TRION-1620-LV-6-L1B			FW: x0031
** TRION-1603-LV-6-BNC			FW: x0A15
** TRION-1603-LV-6-L1B			FW: x0A15
** TRION-1603-LV-6-D25			FW: x0A15
** TRION-1600-dLV-16-D			FW: x187E
** TRION-1600-dLV-16-D-CAN		FW: x187E
** TRION-1600-dLV-32-D			FW: x187E
** TRION-1600-dLV-32-D-CAN		FW: x187E
** TRION-1802-dLV-16-D			FW: x187E
** TRION-1802-dLV-16-D-CAN		FW: x187E
** TRION-1802-dLV-32-D			FW: x187E
** TRION-1802-dLV-32-D-CAN		FW: x187E
** TRION-2402-MULTI-4-D			FW: x0B18
** TRION-2402-MULTI-8-L0B		FW: x0A23
** TRION-2402-MULTI-S1			FW: x0034
** TRION-2402-dSTG-6-L1B		FW: x1120
** TRION-2402-dSTG-8-D			FW: x1120
** TRION-2402-dSTG-8-L0B		FW: x1120
** TRION-2402-dSTG-8-RJ			FW: x1120
** TRION-2400-dSTG-8-L0B		FW: x1120
** TRION-2400-dSTG-OEM			FW: x1120
** TRION-2402-dACC-6-BNC		FW: x1119
** TRION-2402-dACC-8-SMB		FW: x1119
** TRION-2402-dACC-8-MD			FW: x1119
** TRION-2402-V-4-B				FW: x1017
** TRION-2402-V-8-B				FW: x1017
** TRION-CNT-6-L1B				FW: x1119
** TRION-BASE					FW: x1144
** TRION-TIMING					FW: x1144
** TRION-TIMING-V2				FW: x0002
** TRION-VGPS-20				FW: x1144
** TRION-VGPS-100				FW: x1144
** TRION-CAN-4					FW: x1121
** TRION-CAN-2					FW: x1121
** TRION-DI-48					FW: x1119
** TRION-DI-64-S1				FW: x0009

* HW Support DEWE2 chassis:
** DEWE2-PA7
** DEWE2-A4
** DEWE2-A4L
** DEWE2-A7
** DEWE2-A13
** DEWE2-M4
** DEWE2-M4s
** DEWE2-M7
** DEWE2-M7s
** DEWE2-M13
** DEWE2-M13s
** DEWE2-M18
** DEWE2-F4s
** DEWE2-F7s
** DEWE2-F13s
** DEWE2-F18
** DEWE2-F4-THUNDERBOLT
** DEWE2-F13-FIBRE
** TRIONet
** TrendCorder


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2017-05-17 Release Notice DEWETRON TRION API R2.4.4

* Version: 	2.4.33703.00 (Rev.: b1dafcb956c117bbd69d1571a584cf2e5844e879)

* Components:
** DEWE2 Explorer                       2.4.33703.00
** DEWE-TRION application library       2.4.33703.00
** DEWE-TRION system driver             2.4.33703.00
** DEWE2 enclosure access               2.4.33703.00
** DEWE-TRION board information         $Revision: 1481707729
** DEWE2 enclosure information          $Revision: 1470912035
** DEWE-TRION firmware revisions        $Revision: 1488196624

* Files:
** DEWETRON-TRION-Applications-x64.exe
** DEWETRON-TRION-Applications-x86.exe

* Requirements:
** Update all Trion modules to the latest firmware included in this release
** Use Oxygen R2.4 (2.4.0.33520)
** Use DEWESoft 7.1.3_b408 or later
** Windows 10 64-Bit or Windows 7 64-/32-Bit

* Installation procedure:
** Uninstall any previous TRION version via system uninstall (control panel)
** Reboot system
** Install TRION applications
** Reboot system
** Start DEWE2Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
** Power-cycle TRION boards (Power down system, then restart)

* New Features and most important bugfixes:
** TRION-Installer: TRION SDK is now included and selectable as individual package
** TRION-Installer: CPAD3 plugin is now selectable as individual package
** TRION API: Improved internal handling of TRION Digital-Out channels for OXYGEN 2.4
** DEWE2Explorer: Show correct icon in startmenu

* Known Limitations:
** DS only: temperature measurement with PT100 sensor only valid till < 300°C (above linearization problems)
** TRION-MULTI-2402-x: RTD measurement 3-wire connection shows wrong values

* HW Support TRION modules:
** TRION-1620-ACC-6-BNC			FW: x0031
** TRION-1620-ACC-6-L1B			FW: x0031
** TRION-1620-LV-6-BNC			FW: x0031
** TRION-1620-LV-6-L1B			FW: x0031
** TRION-1603-LV-6-BNC			FW: x0A15
** TRION-1603-LV-6-L1B			FW: x0A15
** TRION-1603-LV-6-D25			FW: x0A15
** TRION-2402-MULTI-4-D			FW: x0B18
** TRION-2402-MULTI-8-L0B		FW: x0A23
** TRION-2402-MULTI-S1			FW: x0034
** TRION-2402-dSTG-6-L1B		FW: x1120
** TRION-2402-dSTG-8-D			FW: x1120
** TRION-2402-dSTG-8-L0B		FW: x1120
** TRION-2402-dSTG-8-RJ			FW: x1120
** TRION-2400-dSTG-8-L0B		FW: x1120
** TRION-2400-dSTG-OEM			FW: x1120
** TRION-2402-dACC-6-BNC		FW: x1119
** TRION-2402-dACC-8-SMB		FW: x1119
** TRION-2402-dACC-8-MD			FW: x1119
** TRION-2402-V-4-B				FW: x1017
** TRION-2402-V-8-B				FW: x1017
** TRION-CNT-6-L1B				FW: x1119
** TRION-BASE					FW: x1144
** TRION-TIMING					FW: x1144
** TRION-VGPS-20				FW: x1144
** TRION-VGPS-100				FW: x1144
** TRION-CAN-4					FW: x1121
** TRION-CAN-2					FW: x1121
** TRION-DI-48					FW: x1119
** TRION-DI-64-S1				FW: x0009

* HW Support DEWE2 chassis:
** DEWE2-A4
** DEWE2-A4L
** DEWE2-A7
** DEWE2-A13
** DEWE2-M4
** DEWE2-M4s
** DEWE2-M7
** DEWE2-M7s
** DEWE2-M13
** DEWE2-M13s
** DEWE2-M18
** DEWE2-F4s
** DEWE2-F7s
** DEWE2-F13s
** DEWE2-F18
** DEWE2-F4-THUNDERBOLT
** DEWE2-F13-FIBRE
** TRIONet
** TrendCorder


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2017-03-02 Release Notice DEWETRON TRION API R2.4.3

* Version: 	2.4.31194.00 (Rev.: 73a92c99f38b02f6662273f2a57d06f2d2a302c1)

* Components:
** DEWE2 Explorer                       2.4.31194.00
** DEWE-TRION application library       2.4.31194.00
** DEWE-TRION system driver             2.4.31194.00
** DEWE2 enclosure access               2.4.31194.00
** DEWE-TRION board information         $Revision: 1479981955
** DEWE2 enclosure information          $Revision: 1470912035
** DEWE-TRION firmware revisions        $Revision: 1488196624

* Files:
** DEWETRON-TRION-Applications-x64.exe
** DEWETRON-TRION-Applications-x86.exe

* Requirements:
** Update all Trion modules to the latest firmware included in this release
** Use Oxygen R2.3.2 (2.3.2.30754)
** Use DEWESoft 7.1.3_b408 or later
** Windows 10 64-Bit or Windows 7 64-/32-Bit

* Installation procedure:
** Uninstall any previous TRION version via system uninstall (control panel)
** Reboot system
** Install TRION applications
** Reboot system
** Start DEWE2Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
** Power-cycle TRION boards (Power down system, then restart)

* New Features and most important bugfixes:
** TRION-1603-LV-6-BNC/L1B: update of firmware to xA015 due to stabilization of high channel-count systems
** TRION-2402-V-4/8-B: update of firmware to x1017 due to stabilization of high channel-count systems

* Known Limitations:
** DS only: temperature measurement with PT100 sensor only valid till < 300°C (above linearization problems)
** TRION-MULTI-2402-x: RTD measurement 3-wire connection shows wrong values

* HW Support TRION modules:
** TRION-1620-ACC-6-BNC			FW: x0031
** TRION-1620-ACC-6-L1B			FW: x0031
** TRION-1620-LV-6-BNC			FW: x0031
** TRION-1620-LV-6-L1B			FW: x0031
** TRION-1603-LV-6-BNC			FW: x0A15
** TRION-1603-LV-6-L1B			FW: x0A15
** TRION-1603-LV-6-D25			FW: x0A15
** TRION-2402-MULTI-4-D			FW: x0B18
** TRION-2402-MULTI-8-L0B		FW: x0A23
** TRION-2402-MULTI-S1			FW: x0034
** TRION-2402-dSTG-6-L1B		FW: x1120
** TRION-2402-dSTG-8-D			FW: x1120
** TRION-2402-dSTG-8-L0B		FW: x1120
** TRION-2402-dSTG-8-RJ			FW: x1120
** TRION-2400-dSTG-8-L0B		FW: x1120
** TRION-2400-dSTG-OEM			FW: x1120
** TRION-2402-dACC-6-BNC		FW: x1119
** TRION-2402-dACC-8-SMB		FW: x1119
** TRION-2402-dACC-8-MD			FW: x1119
** TRION-2402-V-4-B				FW: x1017
** TRION-2402-V-8-B				FW: x1017
** TRION-CNT-6-L1B				FW: x1119
** TRION-BASE					FW: x1144
** TRION-TIMING					FW: x1144
** TRION-VGPS-20				FW: x1144
** TRION-VGPS-100				FW: x1144
** TRION-CAN-4					FW: x1121
** TRION-CAN-2					FW: x1121
** TRION-DI-48					FW: x1119
** TRION-DI-64-S1				FW: x0009

* HW Support DEWE2 chassis:
** DEWE2-A4
** DEWE2-A4L
** DEWE2-A7
** DEWE2-A13
** DEWE2-M4
** DEWE2-M4s
** DEWE2-M7
** DEWE2-M7s
** DEWE2-M13
** DEWE2-M13s
** DEWE2-M18
** DEWE2-F4s
** DEWE2-F7s
** DEWE2-F13s
** DEWE2-F18
** DEWE2-F4-THUNDERBOLT
** DEWE2-F13-FIBRE
** TRIONet
** TrendCorder


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2017-02-13 Release Notice DEWETRON TRION API R2.4.2

* Version: 	2.4.30647.00 (Rev.: 1240d78d3b142c7a96e0b8e998bd358dc4259bc7)

* Components:
** DEWE2 Explorer                       2.4.30647.00
** DEWE-TRION application library       2.4.30647.00
** DEWE-TRION system driver             2.4.30647.00
** DEWE2 enclosure access               2.4.30647.00
** DEWE-TRION board information         $Revision: 1479981955
** DEWE2 enclosure information          $Revision: 1470912035
** DEWE-TRION firmware revisions        $Revision: 1486724309

* Files:
** DEWETRON-TRION-Applications-x64.exe
** DEWETRON-TRION-Applications-x86.exe

* Requirements:
** Update all Trion modules to the latest firmware included in this release
** Use Oxygen R2.3.1 (2.3.1.30189)
** Use DEWESoft 7.1.3_b408 or later
** Windows 10 64-Bit or Windows 7 64-/32-Bit

* Installation procedure:
** Uninstall any previous TRION version via system uninstall (control panel)
** Reboot system
** Install TRION applications
** Reboot system
** Start DEWE2Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
** Power-cycle TRION boards (Power down system, then restart)

* New Features and most important bugfixes:
** TRION-2402-MULTI-8-L0B: update of firmware to x0A23 due to measurement start issues
** DEWE2Explorer: update of icon
** DEWE2Explorer: fixed a crash when using older demo configuration files
** DEWE2Explorer: display correct demo system even when connected to real DEWE2-hardware

* Known Limitations:
** DS only: temperature measurement with PT100 sensor only valid till < 300°C (above linearization problems)
** TRION-MULTI-2402-x: RTD measurement 3-wire connection shows wrong values

* HW Support TRION modules:
** TRION-1620-ACC-6-BNC			FW: x0031
** TRION-1620-ACC-6-L1B			FW: x0031
** TRION-1620-LV-6-BNC			FW: x0031
** TRION-1620-LV-6-L1B			FW: x0031
** TRION-1603-LV-6-BNC			FW: x0A14
** TRION-1603-LV-6-L1B			FW: x0A14
** TRION-1603-LV-6-D25			FW: x0A14
** TRION-2402-MULTI-4-D			FW: x0B18
** TRION-2402-MULTI-8-L0B		FW: x0A23
** TRION-2402-MULTI-S1			FW: x0034
** TRION-2402-dSTG-6-L1B		FW: x1120
** TRION-2402-dSTG-8-D			FW: x1120
** TRION-2402-dSTG-8-L0B		FW: x1120
** TRION-2402-dSTG-8-RJ			FW: x1120
** TRION-2400-dSTG-8-L0B		FW: x1120
** TRION-2400-dSTG-OEM			FW: x1120
** TRION-2402-dACC-6-BNC		FW: x1119
** TRION-2402-dACC-8-SMB		FW: x1119
** TRION-2402-dACC-8-MD			FW: x1119
** TRION-2402-V-4-B				FW: x1016
** TRION-2402-V-8-B				FW: x1016
** TRION-CNT-6-L1B				FW: x1119
** TRION-BASE					FW: x1144
** TRION-TIMING					FW: x1144
** TRION-VGPS-20				FW: x1144
** TRION-VGPS-100				FW: x1144
** TRION-CAN-4					FW: x1121
** TRION-CAN-2					FW: x1121
** TRION-DI-48					FW: x1119
** TRION-DI-64-S1				FW: x0009

* HW Support DEWE2 chassis:
** DEWE2-A4
** DEWE2-A4L
** DEWE2-A7
** DEWE2-A13
** DEWE2-M4
** DEWE2-M4s
** DEWE2-M7
** DEWE2-M7s
** DEWE2-M13
** DEWE2-M13s
** DEWE2-M18
** DEWE2-F4s
** DEWE2-F7s
** DEWE2-F13s
** DEWE2-F18
** DEWE2-F4-THUNDERBOLT
** DEWE2-F13-FIBRE
** TRIONet
** TrendCorder


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2017-02-01 Release Notice DEWETRON TRION API R2.4.1

* Version: 	2.4.30182.00 (Rev.: eb9b52fe2a3a00ec79437519b196d0557816cdf6)

* Components:
** DEWE2 Explorer                       2.4.30182.00
** DEWE-TRION application library       2.4.30182.00
** DEWE-TRION system driver             2.4.30182.00
** DEWE2 enclosure access               2.4.30182.00
** DEWE-TRION board information         $Revision: 1479981955
** DEWE2 enclosure information          $Revision: 1470912035
** DEWE-TRION firmware revisions        $Revision: 1484822981
** TRION SDK OCX						1.0.0.7

* Files:
** DEWETRON-TRION-Applications-x64.exe
** DEWETRON-TRION-Applications-x86.exe

* TRION SDK: OCX package only
** trion_oxc.ocx (v1.0.0.7, Rev.: a155e335016c89583cb8a1fc3cd500995369b1c0)
** use with TRION R2.4.1 or higher, only 32-Bit (x86) supported

* Requirements:
** Update all Trion modules to the latest firmware included in this release
** Use Oxygen R2.3.1 (2.3.1.30189)
** Use DEWESoft 7.1.3_b408 or later
** Windows 10 64-Bit or Windows 7 64-/32-Bit

* Installation procedure:
** Uninstall any previous TRION version via system uninstall (control panel)
** Reboot system
** Install TRION applications
** Reboot system
** Start DEWE2Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
** Power-cycle TRION boards (Power down system, then restart)

* New Features and most important bugfixes:
** TRION SDK OCX-package updated
** DS only: explicit "filter off" setting for IIR-filters
** TRIONCAL: boost_regex-vc120-mt-1_57.dll was missing in TRIONCAL folder C:\Program Files\DEWETRON\TRIONCAL 

* Known Limitations:
** DS only: temperature measurement with PT100 sensor only valid till < 300°C (above linearization problems)
** TRION-MULTI-2402-x: RTD measurement 3-wire connection shows wrong values

* HW Support TRION modules:
** TRION-1620-ACC-6-BNC			FW: x0031
** TRION-1620-ACC-6-L1B			FW: x0031
** TRION-1620-LV-6-BNC			FW: x0031
** TRION-1620-LV-6-L1B			FW: x0031
** TRION-1603-LV-6-BNC			FW: x0A14
** TRION-1603-LV-6-L1B			FW: x0A14
** TRION-1603-LV-6-D25			FW: x0A14
** TRION-2402-MULTI-4-D			FW: x0B18
** TRION-2402-MULTI-8-L0B		FW: x0A22
** TRION-2402-MULTI-S1			FW: x0034
** TRION-2402-dSTG-6-L1B		FW: x1120
** TRION-2402-dSTG-8-D			FW: x1120
** TRION-2402-dSTG-8-L0B		FW: x1120
** TRION-2402-dSTG-8-RJ			FW: x1120
** TRION-2400-dSTG-8-L0B		FW: x1120
** TRION-2400-dSTG-OEM			FW: x1120
** TRION-2402-dACC-6-BNC		FW: x1119
** TRION-2402-dACC-8-SMB		FW: x1119
** TRION-2402-dACC-8-MD			FW: x1119
** TRION-2402-V-4-B				FW: x1016
** TRION-2402-V-8-B				FW: x1016
** TRION-CNT-6-L1B				FW: x1119
** TRION-BASE					FW: x1144
** TRION-TIMING					FW: x1144
** TRION-VGPS-20				FW: x1144
** TRION-VGPS-100				FW: x1144
** TRION-CAN-4					FW: x1121
** TRION-CAN-2					FW: x1121
** TRION-DI-48					FW: x1119
** TRION-DI-64-S1				FW: x0009

* HW Support DEWE2 chassis:
** DEWE2-A4
** DEWE2-A4L
** DEWE2-A7
** DEWE2-A13
** DEWE2-M4
** DEWE2-M4s
** DEWE2-M7
** DEWE2-M7s
** DEWE2-M13
** DEWE2-M13s
** DEWE2-M18
** DEWE2-F4s
** DEWE2-F7s
** DEWE2-F13s
** DEWE2-F18
** DEWE2-F4-THUNDERBOLT
** DEWE2-F13-FIBRE
** TRIONet
** TrendCorder


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2016-12-07 Release Notice DEWETRON TRION API R2.4

* Version: 	2.4.28624.00 (Rev.: df87d3c1f4e3f43cbbd8992d6a7782acf6f7532d)

* Components:
** DEWE2 Explorer                       2.4.28624.00
** DEWE-TRION application library       2.4.28624.00
** DEWE-TRION system driver             2.4.28624.00
** DEWE2 enclosure access               2.4.28624.00
** DEWE-TRION board information         $Revision: 1479981955
** DEWE2 enclosure information          $Revision: 1470912035
** DEWE-TRION firmware revisions        $Revision: 1476265207

* Files:
** DEWETRON-TRION-Applications-x64.exe
** DEWETRON-TRION-Applications-x86.exe

* Requirements:
** Update all Trion modules to the latest firmware included in this release
** Use Oxygen R2.3 (2.3.0.28628)
** Use DEWESoft 7.1.3_b408 or later
** Windows 10 64-Bit or Windows 7 64-/32-Bit

* Installation procedure:
** Uninstall any previous TRION version via system uninstall (control panel)
** Reboot system
** Install TRION applications
** Reboot system
** Start DEWE2Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
** Power-cycle TRION boards (Power down system, then restart)

* New Features and most important bugfixes:
** support of Windows 10 64-Bit 
** support of TRION-1620-ACC-6-L1B
** support of DEWE2-A4L
** support of zeroconf for TRIONet
** improved self-test functionalities of DEWE2Explorer
** improved CAN data transfer
** installation of all 4 CPAD3 plugin instances to DS-Addons folder (CPAD3_A.dll, CPAD3_B.dll, CPAD3_C.dll, CPAD3_D.dll) and removal of CPAD2 plugin
** exchanged the XML-parser with big performance improvement and lower memory consumption
** default setting of TRION input filters changed to characteristic "Bessel"

* Known Limitations:
** DS only: temperature measurement with PT100 sensor only valid till < 300°C (above linearization problems)
** TRION-MULTI-2402-x: RTD measurement 3-wire connection shows wrong values
** TRIONCAL: boost_regex-vc120-mt-1_57.dll is missing in TRIONCAL folder C:\Program Files\DEWETRON\TRIONCAL (solution: copy from DEWE2explorer folder)

* HW Support TRION modules:
** TRION-1620-ACC-6-BNC			FW: x0031
** TRION-1620-ACC-6-L1B			FW: x0031
** TRION-1620-LV-6-BNC			FW: x0031
** TRION-1620-LV-6-L1B			FW: x0031
** TRION-1603-LV-6-BNC			FW: x0A14
** TRION-1603-LV-6-L1B			FW: x0A14
** TRION-1603-LV-6-D25			FW: x0A14
** TRION-2402-MULTI-4-D			FW: x0B18
** TRION-2402-MULTI-8-L0B		FW: x0A22
** TRION-2402-MULTI-S1			FW: x0034
** TRION-2402-dSTG-6-L1B		FW: x1120
** TRION-2402-dSTG-8-D			FW: x1120
** TRION-2402-dSTG-8-L0B		FW: x1120
** TRION-2402-dSTG-8-RJ			FW: x1120
** TRION-2400-dSTG-8-L0B		FW: x1120
** TRION-2400-dSTG-OEM			FW: x1120
** TRION-2402-dACC-6-BNC		FW: x1119
** TRION-2402-dACC-8-SMB		FW: x1119
** TRION-2402-dACC-8-MD			FW: x1119
** TRION-2402-V-4-B				FW: x1016
** TRION-2402-V-8-B				FW: x1016
** TRION-CNT-6-L1B				FW: x1119
** TRION-BASE					FW: x1144
** TRION-TIMING					FW: x1144
** TRION-VGPS-20				FW: x1144
** TRION-VGPS-100				FW: x1144
** TRION-CAN-4					FW: x1121
** TRION-CAN-2					FW: x1121
** TRION-DI-48					FW: x1119
** TRION-DI-64-S1				FW: x0009

* HW Support DEWE2 chassis:
** DEWE2-A4
** DEWE2-A4L
** DEWE2-A7
** DEWE2-A13
** DEWE2-M4
** DEWE2-M4s
** DEWE2-M7
** DEWE2-M7s
** DEWE2-M13
** DEWE2-M13s
** DEWE2-M18
** DEWE2-F4s
** DEWE2-F7s
** DEWE2-F13s
** DEWE2-F18
** DEWE2-F4-THUNDERBOLT
** DEWE2-F13-FIBRE
** TRIONet
** TrendCorder


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2016-09-27 Release Notice DEWETRON TRION Software R2.3.3 (VW only)

* Version: 2.3.26121.00 (Rev.: d7f77521a0a25709ea8216a20c1f52acd3f8af6e)

* Components:
** DEWE2 Explorer                       2.3.26121.00
** DEWE-TRION application library       2.3.26121.00
** DEWE-TRION system driver             2.3.26121.00
** DEWE2 enclosure access               2.3.26121.00
** DEWE-TRION board information         $Revision: 1467109435
** DEWE2 enclosure information          $Revision: 1470912035
** DEWE-TRION firmware revisions        $Revision: 1465913615

* Requirements:
** Update all Trion modules to the latest firmware included in this release
** Use Oxygen R2.2
** Use DEWESoft 7.1.3_b408 or later
** Windows 7 64-/32-Bit

* Fixes:
** #3457 Fixed: DeweSoft - sensor-offset not loaded reliably when loading setup (issue reported from VW)


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2016-07-19 Release Notice DEWETRON TRION Software R2.3.2

* Version: 2.3.23834.00 (Rev.: c2751fc7ef0cf31d59a67b3c6ae218f4565f588f)

* Components:
** DEWE2 Explorer                       2.3.23834.00
** DEWE-TRION application library       2.3.23834.00
** DEWE-TRION system driver             2.3.23834.00
** DEWE2 enclosure access               2.3.23834.00
** DEWE-TRION board information         $Revision: 1467109435
** DEWE2 enclosure information          $Revision: 1454673046
** DEWE-TRION firmware revisions        $Revision: 1465913615

* Requirements:
** Update all Trion modules to the latest firmware included in this release
** Use Oxygen R2.1 (2.1.0.22505)
** Use DEWESoft 7.1.3_b408 or later
** Windows 7 64-/32-Bit

* New Features:
** TRIONet: enhanced IP config troubleshooting in DEWE2Explorer
** TRIONet: access empty TRIONet enclosures

* Fixes:
** #3175 Fixed: TRION CAL does not store xml-files
** #3227 Fixed: TRION CAL error when running CMD_DRIVER_LOAD

* Known Limitations:
**none


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2016-07-12 Release Notice DEWETRON TRION Software R2.1.2 Amergint 1.0.10 (Customer A)

Software Update Package delivered to AMERGINT - TRION R2.1.2 Amergint 1.0.10

Buildserver Tag:				TRION 2.1.2 Amergint 1.0.10

TRION API LINUX CentOS 6.4: 	2.1.23429.00
(TRION API WINDOWS 32-Bit:		2.1.23429.0)
(TRION API WINDOWS 64-Bit:		2.1.23429.0)

TRION-2402-MULTI-S1 FW:			0034
TRION-DI-64-S1 FW:				0008

* New Features:
** TRION CAL server included in package
** CR04: change the lower limit of the digital low pass filter from 10Hz to 1Hz
** TRION-MULTI resistance mode: EXC current adjustable up to max. 4mA
** TRION-MULTI input mode 3-wire type2: 
	implemented additional internal offset (module) to improve measurement accuracy  
	for the internal offset a special 3-wire-short-connector has to be connected to the module
	Factory calibration now also supports internal offset calibration for input mode 3-wire type2
** DEWE2Explorer: new functionality to manualy trigger the internal offset function (special 3-wire-short-connector required)


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2016-06-21 Release Notice DEWETRON TRION Software R2.3.1

* Version: 2.3.22727.00

* Components:
** DEWE2 Explorer                       2.3.22727.00
** DEWE-TRION application library       2.3.22727.00
** DEWE-TRION system driver             2.3.22727.00
** DEWE2 enclosure access               2.3.22727.00
** DEWE-TRION board information         $Revision: 1464773604
** DEWE2 enclosure information          $Revision: 1454673046
** DEWE-TRION firmware revisions        $Revision: 1465913615

* Requirements:
** Update all Trion modules to the latest firmware included in this release
** Use Oxygen R2.1 (2.1.0.22505)
** Use DEWESoft 7.1.3_b408 or later
** Windows 7 64-/32-Bit

* New Features:
** Support of TRIONet device (LAN or USB connection) 
** TRION Module IIR-Filter: lower cut-off frequency changed from 10Hz to 1Hz, for TRION-1620-LV/ACC
** TRION-BASE, TRION-TIMING, TRION-VGPS modules: added IRIG_B_TTL option, that allows better accuracy when using IRIG-sources providing TTL-compatible levels compared to IRIG_DC
** TRION-BASE, TRION-TIMING, TRION-VGPS modules: Straight-binary-Seconds (SBS) added to IRIG_B_DC output stream  

* Fixes:
** apps/dewe2explorer: RemoteSettingsDialog: disable IP & MASK text boxes in case of DHCP
** #3031 fixed TRION-2402-dSTG Quarter Bridge mode - no measured values, if AC-coupling >= 0,5 Hz is selected
** #2091 fixed TRION-2402-dSTG Bridge mode: Selecting an Excitation <= 0 V would lead to an application-crash

* Known Limitations:
** When changing AUX Output in Hardware Setup of DeweSoft directly from ACQ_CLK or Frequency / Continuous Out to any other AUX Output Option the Trion Boards will not start
   => Workaround: Open Hardware Setup again, click Cancel Button 


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2016-06-16 Release Notice DEWETRON TRION Software R2.3

* Version: 2.3.22662.00

* Components:
** DEWE2 Explorer                       2.3.22662.00
** DEWE-TRION application library       2.3.22662.00
** DEWE-TRION system driver             2.3.22662.00
** DEWE2 enclosure access               2.3.22662.00
** DEWE-TRION board information         $Revision: 1464773604
** DEWE2 enclosure information          $Revision: 1454673046
** DEWE-TRION firmware revisions        $Revision: 1465913615

* Requirements:
** Update all Trion modules to the latest firmware included in this release
** Use Oxygen R2.1 (2.1.0.22505)
** Use DEWESoft 7.1.3_b408 or later
** Windows 7 64-/32-Bit

* New Features:
** Support of TRIONet device (LAN or USB connection) 
** TRION Module IIR-Filter: lower cut-off frequency changed from 10Hz to 1Hz, for TRION-1620-LV/ACC
** TRION-BASE, TRION-TIMING, TRION-VGPS modules: added IRIG_B_TTL option, that allows better accuracy when using IRIG-sources providing TTL-compatible levels compared to IRIG_DC
** TRION-BASE, TRION-TIMING, TRION-VGPS modules: Straight-binary-Seconds (SBS) added to IRIG_B_DC output stream  

* Fixes:
** #3031 fixed TRION-2402-dSTG Quarter Bridge mode - no measured values, if AC-coupling >= 0,5 Hz is selected
** #2091 fixed TRION-2402-dSTG Bridge mode: Selecting an Excitation <= 0 V would lead to an application-crash

* Known Limitations:
** When changing AUX Output in Hardware Setup of DeweSoft directly from ACQ_CLK or Frequency / Continuous Out to any other AUX Output Option the Trion Boards will not start
   => Workaround: Open Hardware Setup again, click Cancel Button 


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2016-04-21 Release Notice DEWETRON TRION Software R2.2.6

* Version: 2.2.21036.00

* Components:
** DEWE2 Explorer                       2.2.21036.00
** DEWE-TRION application library       2.2.21036.00
** DEWE-TRION system driver             2.2.21036.00
** DEWE2 enclosure access               2.2.21036.00
** DEWE-TRION board information         $Revision: 1457081665
** DEWE2 enclosure information          $Revision: 1444215375
** DEWE-TRION firmware revisions        $Revision: 1446458150

* Requirements:
** Update all Trion modules to the latest firmware included in this release
** Use DEWESoft 7.1.3_b408 or later
** Windows 7 64-/32-Bit

* Fixes:
** #2719 Fixed: Bride mode - Range is set to not allowed range when highest range and 10V excitation is selected and sensor balance is done (VW)

+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2016-03-25 Release Notice DEWETRON TRION Software R2.2.5

* Version: 2.2.20313.00

* Components:
** DEWE2 Explorer                       2.2.20313.00
** DEWE-TRION application library       2.2.20313.00
** DEWE-TRION system driver             2.2.20313.00
** DEWE2 enclosure access				2.2.20313.00
** DEWE-TRION board information         $Revision: 1457081665
** DEWE2 enclosure information          $Revision: 1444215375
** DEWE-TRION firmware revisions        $Revision: 1446458150

* Requirements:
** Update all Trion modules to the latest firmware included in this release
** Use DEWESoft 7.1.3_b408 or later
** Windows 7 64-/32-Bit

* New Features:
** Size of SetupScreenBuffer is now adjustable in DEWESoft HW-setup, set to higher value if scan of TRION-boards lasts too long (default 10sec, adjustable 5-50 sec) - Caution: consider memory consumption of DEWESoft


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2016-03-10 Release Notice DEWETRON TRION Software R2.2.4

* Version: 2.2.19888.00

* Components:
** DEWE2 Explorer                       2.2.19888.00
** DEWE-TRION application library       2.2.19888.00
** DEWE-TRION system driver             2.2.19888.00
** DEWE2 enclosure access				2.2.19888.00
** DEWE-TRION board information         $Revision: 1457081665
** DEWE2 enclosure information          $Revision: 1444215375
** DEWE-TRION firmware revisions        $Revision: 1446458150

* Requirements:
** Update all Trion modules to the latest firmware included in this release
** Use DEWESoft 7.1.3_b408 or later
** Windows 7 64-/32-Bit

* Fixes:
** #2720 Fixed: QuarterBridge mode missing in TRION-2400-dSTG-8-L0B 


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2016-02-16 Release Notice DEWETRON TRION Software R2.2.3

* Version: 2.2.19234.00

* Components:
** DEWE2 Explorer                       2.2.19234.00
** DEWE-TRION application library       2.2.19234.00
** DEWE-TRION system driver             2.2.19234.00
** DEWE2 enclosure access				2.2.19234.00
** DEWE-TRION board information         $Revision: 1455013357
** DEWE2 enclosure information          $Revision: 1444215375
** DEWE-TRION firmware revisions        $Revision: 1446458150

* Requirements:
** Update all Trion modules to the latest firmware included in this release
** Use DEWESoft 7.1.3_b408 or later
** Windows 7 64-/32-Bit

* New supported Modules:
** TRION-1603-LV-6-D25

* Fixes:
** #2622 Fixed: Lowered Memory-consumption on TRION.DAQ 


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2015-12-11 Release Notice DEWETRON TRION Software R2.2.2

* Version: 2.2.17821.00

* Components:
** DEWE2 Explorer                       2.2.17821.00
** DEWE-TRION application library       2.2.17821.00
** DEWE-TRION system driver             2.2.17821.00
** DEWE2 enclosure access				2.2.17821.00
** DEWE-TRION board information         $Revision: 1449749478
** DEWE2 enclosure information          $Revision: 1444215375
** DEWE-TRION firmware revisions        $Revision: 1446458150

* Requirements:
** Update all Trion modules to the latest firmware included in this release
** Use DEWESoft 7.1.3_b408 or later
** Windows 7 64-/32-Bit

* Fixes:
** TRION-2402-MULTI-8-L0B/TRION-2402-MULTI-4-D: self-test functionality improved


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2015-11-13 Release Notice DEWETRON TRION Software R2.2.1

* Version: 2.2.17086.00

* Components:
** DEWE2 Explorer                       2.2.17086.00
** DEWE-TRION application library       2.2.17086.00
** DEWE-TRION system driver             2.2.17086.00
** DEWE2 enclosure access				2.2.17086.00
** DEWE-TRION board information         $Revision: 1446722136
** DEWE2 enclosure information          $Revision: 1444215375
** DEWE-TRION firmware revisions        $Revision: 1446458150

* Requirements:
** Update all Trion modules to the latest firmware included in this release
** Use DEWESoft 7.1.3_b408 or later
** Windows 7 64-/32-Bit

* New supported Modules:
** TRION-2402-MULTI-8-L0B
** TRION-2402-MULTI-4-D
** TRION-1620-LV-6-L1B
** TRION-1603-LV-6-L1B
** TRION-2400-dSTG-8-L0B

* New Features:
** MSI SDK-Support for TRION-2402-MULTI implementation done
** TimeSync PlugIn (Honeywell): added year information to time stamp, configureable and per default "off"
** TRION Module IIR-Filter: lower cut-off frequency changed from 10Hz to 1Hz, exception: TRION-1620-LV/ACC
** TRION installer with new CI and DEWETRON logo

* Fixes:
** #2241 CAN: Fixed measurement start when using SMOTION sensor (Kistler Wheel)
** #2103 CAN: re-worked stop and start of CAN measurement to ensure correct time stamps
** #2193 TRION-VGPS: correction of Counter Channel reporting, only 1 Counter Channel available on the module 
** #2104 Fixed: When EPADs are enabled in DeweSoft a restart is required
** #1834 Fixed: TRION-1620-xx: max shown LP-filter was set to 600kHz (before 500kHz)

* Known Limitations:
** Insertion of a TRION-2402-MULTI module prior to the TRION software update will cause a blue screen due to wrong kernel driver version
** #961 TRION-DI48 only runs up to 2MS/s
** #2064 Video trigger only working on TRION module in Star-Slot
** #1842 Trion-1620-ACC channel indicator LED function (IEPE mode) not implemented. 
** TRION-VGPS: differential GPS not supported
** When disabling CAN in DEWESoft Hardware Setup Screen, a restart of DEWESoft might be necessary.
** #2313 When disabling CAN in DEWESoft, the setup sampling rate might change and will need manual reconfiguration.
** If DEWESoft has been used with old Trion.DAQ and Trion.CAN plugins, it is necessary to delete DEWESoft Default Project File (...\DEWESoft7\System\V7_0\Default.d7p).
** DEWESoft-Licenses that hold too many Plugin-Licenses might be too large, to be stored to the E2Prom within a Dewe2-Chassis. The Errormessage will be a missleading "EEPROM WRITE FAILED", instead of "FILESIZE EXCEEDS E2PROMSIZE". In these cases it is necessary to store the DEWESoft-License file in the filesystem of the system.
** When using SYNC I/O in a NET-System, statusmessages regarding the sync-connection are shown on NET-Slave instead of NET-Master
** Selecting a Dynamic Samplingrate in DEWESoft that equals Setup(Preview)-Sampling-Rate on Systems with "slow" and fast cards, may show undesired behavior regarding the automatically determinded Samplingrate-Divider and the automatically determined Lowpass-Filter.
** Timing: Setup GPS-In, IRIG-Out basically applies 21000ns between Master and Slave. Same behaviour with GPS-In PPS-Out. RESOLUTION: Consideration of the 21000ns within the missmatch value between Master and Slave with this specific configuration. In Sync-Configuration it is possible, to enter  21000ns into the cable length compensation on the slave system.


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2015-10-19 Release Notice DEWETRON TRION Software R2.2 - TRENDCORDER BUNDLE ONLY

* Version: 2.2.15013.0 

 Components:
** DEWE2 Explorer                       2.2.15013.00
** DEWE-TRION application library       2.2.15013.00
** DEWE-TRION system driver             2.2.15013.00
** DEWE2 enclosure access				2.2.15013.00
** DEWE-TRION board information         $Revision: 1441104660
** DEWE2 enclosure information          $Revision: 1437049260
** DEWE-TRION firmware revisions        $Revision: 1440761646

* New supported Modules:
** TRION-2402-MULTI-8-L0B
** TRION-2402-MULTI-4-D
** TRION-1620-LV-6-L1B                                  


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2015-10-16 Release Notice DEWETRON TRION Software R2.1.3.2

* Version: 2.1.15729.0

 Components:
** DEWE2 Explorer                       2.1.15729.00
** DEWE-TRION application library       2.1.15729.00
** DEWE-TRION system driver             2.1.15729.00
** DEWE2 enclosure access				2.1.15729.0
** DEWE-TRION board information         $Revision: 1442560019
** DEWE2 enclosure information          $Revision: 1437049260
** DEWE-TRION firmware revisions        $Revision: 1434525193

* Hotfix:
** #2097 Wrong module assignment in DEWE2 Explorer fixed (only when daisy chaining DEWE2-chassis)

* Known Limitations:
** #2241 CAN: Problem with measurement start when using SMOTION sensor (Kistler Wheel)


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2015-08-07 Release Notice DEWETRON TRION Software R2.1.3.1

* Version: 2.1.14172.0

 Components:
** DEWE2 Explorer                       2.1.14172.00
** DEWE-TRION application library       2.1.14172.00
** DEWE-TRION system driver             2.1.14172.00
** DEWE2 enclosure access				2.1.14172.0
** DEWE-TRION board information         $Revision: 1437567639
** DEWE2 enclosure information          $Revision: 1437049260
** DEWE-TRION firmware revisions        $Revision: 1434525193

* Hotfix:
** CAN bus stability issue fixed
 

+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2015-07-29 Release Notice DEWETRON TRION Software R2.1.3

* Version: 2.1.13961.0

* Components:
** DEWE2 Explorer                       2.1.13961.00
** DEWE-TRION application library       2.1.13961.00
** DEWE-TRION system driver             2.1.13961.00
** DEWE2 enclosure access				2.1.13961.0
** DEWE-TRION board information         $Revision: 1437567639
** DEWE2 enclosure information          $Revision: 1437049260
** DEWE-TRION firmware revisions        $Revision: 1434525193

* Requirements:
** Update all Trion modules to the latest firmware included in this release
** Use DEWESoft 7.1.3b397 or later
** Windows 7 64-/32-Bit

* New Features:
** Windows 7 64-/32-Bit support 
** Self tests enhanced (gain cal...)
** support of IIR-filter on TRION-2402-V hardware
** new supported chassis : DEWE2-M7, DEWE2-F4-THUNDERBOLT

* Fixes:
** TRION-board initalization problems fixed
** Enclosure initalization problems fixed
** fixed: possible Start-Acquisition-Issues using a DeweSoft NET configuration in conjunction with SYNC I/O-synchronisation:
    - possible start issue on some systems, when SMU holds more than 5 TRION-modules
    - possible start issue, when mixing slow and fast TRION-modules, and MMU holds only slow modules (TRION-24XX).
** CAN bus message time-stamping improved

* New supported Modules:
** TRION-1620-LV-6-L1B
** Any board supported by TRION Release 1.3.3

* Changes
** TRION-boards naming in device-manager changed to TRION Module

* Known Limitations:
** #1834 TRION-1620-xx - max shown LP-filter is 500kHz instead of 600kHz
** #961 TRION-DI48 only runs up to 2Ms
** #2064 Video trigger only working on TRION module in Star-slot
** When EPADs are enabled in DeweSoft a restart is required
** When disabling CAN in DeweSoft Hardware Setup Screen a restart of DeweSoft might be necessary.
** If DeweSoft has been used with old Trion.DAQ and Trion.CAN plugins, it is necessary to delete DeweSoft Default Project File (...\DEWESoft7\System\V7_0\Default.d7p).
** Dewesoft-Licenses that hold too many Plugin-Licenses might be too large, to be stored to the E2Prom within a Dewe2-Chassis. The Errormessage will be a missleading "EEPROM WRITE FAILED", instead of "FILESIZE EXCEEDS E2PROMSIZE". In these cases it is necessary to store the Dewesoft-License file in the filesystem of the system.
** When using SYNC I/O in a NET-System, statusmessages regarding the sync-connection are shown on NET-Slave instead of NET-Master
** Selecting a Dynamic Samplingrate in Dewesoft that equals Setup(Preview)-Sampling-Rate on Systems with "slow" and fast cards, may show undesired behavior regarding the automatically determinded Samplingrate-Divider and the automatically determined Lowpass-Filter.
** Timing: Setup GPS-In, IRIG-Out basically applies 21000ns between Master and Slave. Same behaviour with GPS-In PPS-Out. RESOLUTION: Consideration of the 21000ns within the missmatch value between Master and Slave with this specific configuration. In Sync-Configuration it is possible, to enter  21000ns into the cable length compensation on the slave system.
** Trion-1620-ACC channel indicator LED function (IEPE mode) not implemented. 
** TRION-VGPS: differential GPS not supported!


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2015-07-08 Release Notice DEWETRON TRION Software R2.1.2 Amergint 1.0.7 (Customer A)

Software Update Package delivered to AMERGINT - TRION R2.1.2 Amergint 1.0.7

Buildserver Tag:				2.1 Amergint 1.0.7

TRION API LINUX CentOS 6.4: 	2.1.13291.00
(TRION API WINDOWS 32-Bit:		2.1.13291.0)
(TRION API WINDOWS 64-Bit:		2.1.13291.0)

TRION-2402-MULTI-S1 FW:			0034


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2015-06-10 Release Notice DEWETRON TRION Software R2.1.1 (TrendCorder only)

* Version: 2.1.12689.0 (TrendCorder ONLY)
Per intention not published on install server


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2015-03-06 Release Notice DEWETRON TRION Software R2.0.1 (TrendCorder only)

* Version: 2.0.1 (TrendCorder ONLY)
Per intention not published on install server


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2015-01-21 Release Notice DEWETRON TRION Software R1.3.3 (Calibration only)

* Version: 1.3.9847.00

* Components:
** DEWE2 Explorer                       1.3.9847.00
** DEWE-TRION application library       1.3.9847.00
** DEWE-TRION system driver             0.0.0.35
** DEWE2 enclosure access				00.01.9847.00
** DEWE-TRION board information         $Revision: 5000 $
** DEWE2 enclosure information          $Revision: 5000 $
** DEWE-TRION firmware revisions        $Revision: 5000 $

* Requirements:
** Update all Trion modules to the latest firmware included in this release
** Use DEWESoft 7.1.1 Release or later

* New Features:
** none

* Fixes:
** TRION-API: Fixed an issue with calibration of TRION-16xx modules (e.g. TRION-1620-ACC) and all 24-Bit modules.
 
* New supported Modules:
** Any board supported by TRION Release 1.3.

* Known Limitations:
** TRION-VGPS: differential GPS not supported!


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2014-12-18 Release Notice DEWETRON TRION Software R1.3.2. RC1 (VGPS only)

* Version: 1.3.9629.00

* Components:
** DEWE2 Explorer                       1.3.9629.00
** DEWE-TRION application library       1.3.9629.00
** DEWE-TRION system driver             0.0.0.35
** DEWE2 enclosure access				00.01.9629.00
** DEWE-TRION board information         $Revision: 5000 $
** DEWE2 enclosure information          $Revision: 5000 $
** DEWE-TRION firmware revisions        $Revision: 5000 $

* Requirements:
** Update all Trion modules to the latest firmware included in this release
** Use DEWESoft 7.1.1 Release or later

* New Features:
** DEWESoft: VGPS-Configuration GPS update rate selectable (drop down list with predefined values)

* Fixes:
** TRION-VGPS: improvement of performance due to fix in baudrate-test
** TRION-VGPS: display port fixed and working
** TRION-VGPS: digital out (DO) fixed and working
** TRION-VGPS: baudrate changed from 115k to 460k

* New supported Modules:
** Any board supported by TRION Release 1.3.

* Known Limitations:
** TRION-VGPS: differential GPS not supported!


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2014-10-22 Release Notice DEWETRON TRION Software R1.3.1 (VGPS only)

* Version: 1.3.7876.00

* Components:
** DEWE2 Explorer                       1.3.7876.00
** DEWE-TRION application library       1.3.7876.00
** DEWE-TRION system driver             0.0.0.35
** DEWE2 enclosure access				00.01.7876.00
** DEWE-TRION board information         $Revision: 5000 $
** DEWE2 enclosure information          $Revision: 5000 $
** DEWE-TRION firmware revisions        $Revision: 5000 $

* Requirements:
** Update all Trion modules to the latest firmware included in this release
** Use DEWESoft 7.1.1 Release or later

* New Features:
** All features of TRION Release 1.3.

* Fixes:
** Fixed two issues with the TRION-VGPS: Update of GPS receiver INIT-string to activate 5V antenna supply, Update of XML schematics so IRIG B-DC is selectable again as input type

* New supported Modules:
** Any board supported by TRION Release 1.3.

* Known Limitations:
** TRION-VGPS: display port not supported
** please also refer to TRION Release 1.3.


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2014-09-10 Release Notice DEWETRON TRION Software R1.3

* Version: 1.3.4230.00

* Components:
** DEWE2 Explorer                       1.3.4230.00
** DEWE-TRION application library       1.3.4230.00
** DEWE-TRION system driver             0.0.0.35
** DEWE2 enclosure access				00.01.4230.00
** DEWE-TRION board information         $Revision: 5000 $
** DEWE2 enclosure information          $Revision: 5000 $
** DEWE-TRION firmware revisions        $Revision: 5000 $

* Requirements:
** Update all Trion modules to the latest firmware included in this release
** Use DEWESoft 7.1.1b309 or later

* New Features:
** Added support for TRION-2402-dSTG.8A.LE
** Added support for TRION-1603-LV.6.BN
** Added support for TRION-1620-LV.6.BN
** Added support for TRION-1620-ACC.6.BN
** Added support for TRION-VGPS.20 and TRION-VGPS.100
** Increased maximum possible Samplingrate for most Non-Analogue TRION-Modules
***	2000 kS/sec: TRION-BASE, TRION-TIMING, TRION-VGPS, TRION-CAN, TRION-CNT
*** 3251 kS/sec: TRION-DI-48
** Added support to make TRION-TIMING or TRION-VGPS.XX VGPS information like distance and acceleration available through "Virtual GPS" in Dewesoft.
** Added possiblity to perform "cold-reset" on TRION-GPS receivers, if necessary.
** Added support for Digital-Out on DO capable Boards in Dewesoft, using Alarms
** Added automatic support to allow mixing slower AD-cards with faster ones, and utilize the faster sampling-rate as dynamic-samplingrate
   The slower cards will be used with a automatically determined samplingrate-divider
** The TRION-Driver will now prevent multiple simultaneous application-accesses to TRION-HW to prevent rare cases, where calibration and/or hardware-
   identification data would become corrupted.
   If a second application is trying to initialize TRION-hardware for access, the Driver will report an errorcode indicating, that the application
   cannot take ownership over the TRION-hardware. The final user-representation for this state is application-depending.

* Fixes:
** Fixed a problem, where async TRION-Channels like Timechannel or GPS-data might show a live-data-delay of 1 sec. when no async-consuming plugin is activated.
   The stored data was not affected by this problem.
** Fixed a problem, where the timestamp of GigE-Cams would be wrong by up to 300ms in the first 5 seconds of measurement
** Fixed a problem on TRION-2402-dSTG, where selecting "BridgeMode" would lead to an application-crash, if the module was previsouly in "IEPE"-Mode
** Fixed Dewe2Explorer reporting a wrong File-Version 
** Fixed a problem, where NET-Systems synced via SYNC I/O would not start reliably in Dewesoft-Setup-Screen, when changing Counter or DI configurations

* New supported Modules:
** TRION-2402-dSTG.8A.LE
** TRION-1603-LV.6.BN
** TRION-1620-LV.6.BN
** TRION-1620-ACC.6.BN
** TRION-VGPS.20 and TRION-VGPS.100
** Any board supported by TRION Release 1.2.3

* Changes
** The syncoption "EncSync" has been relabled to "SYNC I/O" to be in line with labling on the Dewe2Unit.

* Known Limitations:
** In rare cases the installer terminates unexpectedly at the end of the installation process. Since all components are already installed at his stage, this behavior has no further impact, and the system can be used as intended.
** After changing a TRION module, the name of the initially installed modules still shows up in Windows Device Manager.
** When disabling CAN in DeweSoft Hardware Setup Screen a restart of DeweSoft might be necessary.
** If DeweSoft has been used with old Trion.DAQ and Trion.CAN plugins, it is necessary to delete DeweSoft Default Project File (...\DEWESoft7\System\V7_0\Default.d7p).
** Dewesoft-Licenses that hold too many Pluginin-Licenses might be too large, to be stored to the E2Prom within a Dewe2-Chassis. The Errormessage will be a missleading "EEPROM WRITE FAILED", instead of "FILESIZE EXCEEDS E2PROMSIZE"
   In these cases it is necessary to store the Dewesoft-License file in the filesystem of the system.
** When using SYNC I/O in a NET-System, statusmessages regarding the sync-connection are shown on NET-Slave instead of NET-Master
** Selecting a Dynamic Samplingrate in Dewesoft that equals Setup(Preview)-Sampling-Rate on Systems with "slow" and fast cards, may show undesired behavior regarding the automatically determinded Samplingrate-Divider and the
   automatically determined Lowpass-Filter.
** possible Start-Acquisition-Issues using a DeweSoft NET configuration in conjunction with SYNC I/O-synchronisation:
    - possible start issue on some systems, when SMU holds more than 5 TRION-modules
    - possible start issue, when mixing slow and fast TRION-modules, and MMU holds only slow modules (TRION-24XX).
** Timing: Setup GPS-In, IRIG-Out basically applies 21000ns between Master and Slave. Same behaviour with GPS-In PPS-Out.
   RESOLUTION: Consideration of the 21000ns within the missmatch value between Master and Slave with this specific configuration. In Sync-Configuration it is possible, to enter 21000ns into the cable length compensation on the slave system.
** Trion-1620-ACC channel indicator LED function (IEPE mode) not implemented. 

  
+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2014-03-03 Release Notice DEWETRON TRION Software R1.2.3

* Version: 0.2014.226.2712

* Components:
** DEWE2 Explorer                       0.2.2712.00
** DEWE-TRION application library       1.2.2712.00
** DEWE-TRION system driver             0.0.0.35
** DEWE-TRION board information         $Revision: 4412 $
** DEWE2 enclosure information          $Revision: 3776 $
** DEWE-TRION firmware revisions        $Revision: 3733 $

* New Features:
** Added support for TRION-2402-dACC.8A.MD
** Added possibility to mount a time-channel in DeweSoft, when synchronizing via GPS or IRIG

* Fixes:
** No fixes.

* New supported Modules:
** TRION-2402-dACC.8A.MD
** Any board supported by TRION Release 1.2.2

* Known Limitations:
** In rare cases the installer terminates unexpectedly at the end of the installation process. Since all components are already installed at his stage, this behavior has no further impact, and the system can be used as intended.
** After changing a TRION module, the name of the initially installed modules still shows up in Windows Device Manager.
** When disabling CAN in DeweSoft Hardware Setup Screen a restart of DeweSoft might be necessary.
** If DeweSoft has been used with old Trion.DAQ and Trion.CAN plugins, it is necessary to delete DeweSoft Default Project File (...\DEWESoft7\System\V7_0\Default.d7p).
** The SYNC I/O hardware interfaces on the TRION TIMING board are currently not supported.
** Timing: Setup GPS-In, IRIG-Out basically applies 21000ns between Master and Slave. Same behaviour with GPS-In PPS-Out.
   RESOLUTION: Consideration of the 21000ns within the missmatch value between Master and Slave with this specific configuration. In Sync-Configuration it is possible, to enter 21000ns into the cable length compensation on the slave system.

   
+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2014-02-12 Release Notice DEWETRON TRION Software R1.2.2

* Version: 0.2014.211.2707

* Components:
** DEWE2 Explorer                       0.2.2707.00
** DEWE-TRION application library       1.2.2707.00
** DEWE-TRION system driver             0.0.0.35
** DEWE-TRION board information         $Revision: 4412 $
** DEWE2 enclosure information          $Revision: 3776 $
** DEWE-TRION firmware revisions        $Revision: 3733 $

* New Features:
** Extended auto restore functionality for TRION modules to prevent loss of calibration data from only base board to connector panel.

* Fixes:
** Some valid sample rates could not be set before R1.2.2
** Some TEDS sensors could not be read.

* New supported Modules:
** Any board supported by TRION Release 1.2.

* Known Limitations:
** In rare cases the installer terminates unexpectedly at the end of the installation process. Since all components are already installed at his stage, this behavior has no further impact, and the system can be used as intended.
** After changing a TRION module, the name of the initially installed modules still shows up in Windows Device Manager.
** When disabling CAN in DeweSoft Hardware Setup Screen a restart of DeweSoft might be necessary.
** If DeweSoft has been used with old Trion.DAQ and Trion.CAN plugins, it is necessary to delete DeweSoft Default Project File (...\DEWESoft7\System\V7_0\Default.d7p).
** The SYNC I/O hardware interfaces on the TRION TIMING board are currently not supported.
** Timing: Setup GPS-In, IRIG-Out basically applies 21000ns between Master and Slave. Same behaviour with GPS-In PPS-Out.
   RESOLUTION: Consideration of the 21000ns within the missmatch value between Master and Slave with this specific configuration. In Sync-Configuration it is possible, to enter 21000ns into the cable length compensation on the slave system.


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2013-xx-yy Release Notice DEWETRON TRION Software R1.2.1

does not exits


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2013-12-09 Release Notice DEWETRON TRION Software R1.2

* Version: 0.2013.1209.2665

* Components:
** DEWE2 Explorer                 		0.2.2665.00
** DEWE-TRION application library       0.36.2665.00
** DEWE-TRION system driver             0.0.0.35
** DEWE-TRION board information         $Revision: 4412 $
** DEWE2 enclosure information          $Revision: 3776 $
** DEWE-TRION firmware revisions        $Revision: 3733 $

* New Features:
** Full featured GPS functionality on TRION Timing
** TRION Installer supports multiple DEWESoft installations 

* New supported Modules:
** Any board supported by Trion Release 1.1.1

* Known Limitations:
** In rare cases the installer terminates unexpectedly at the end of the installation process. Since all components are already installed at his stage, this behavior has no further impact, and the system can be used as intended.
** After changing a TRION module, the name of the initially installed modules still shows up in Windows Device Manager.
** When disabling CAN in DeweSoft Hardware Setup Screen a restart of DeweSoft might be necessary.
** If DeweSoft has been used with old Trion.DAQ and Trion.CAN plugins, it is necessary to delete DeweSoft Default Project File (...\DEWESoft7\System\V7_0\Default.d7p).
** The SYNC I/O hardware interfaces on the TRION TIMING board are currently not supported.
** Timing: Setup GPS-In, IRIG-Out basically applies 21000ns between Master and Slave. Same behaviour with GPS-In PPS-Out.
   RESOLUTION: Consideration of the 21000ns within the missmatch value between Master and Slave with this specific configuration. In Sync-Configuration it is possible, to enter 21000ns into the cable length compensation on the slave system.


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2013-11-06 Release Notice DEWETRON TRION Software R1.1.1 - Teledyne

* Version: 0.2013.1106.1876 for Teledyne

* New Features:
** Added auto restore functionality to prevent loss of calibration data.
** TRION-2400-dSTG-OEM (CON-TRION-dSTG-8.HD)


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2013-11-06 Release Notice DEWETRON TRION Software R1.1.1

* Version: 0.2013.1105.1858

* Components:
** DEWE2 Explorer                   	0.2.1858.00
** DEWE-TRION application library       0.36.1858.00
** DEWE-TRION system driver             0.0.0.35
** DEWE2 enclosure application library  0.2.1858.00
** DEWE2 enclosure system driver        0.01.1858.00
** DEWE-TRION board information         $Revision: 4412 $
** DEWE2 enclosure information          $Revision: 3776 $
** DEWE-TRION firmware revisions        $Revision: 3733 $
** TRION.DAQ (DeweSoft Plugin)          1.1.1858.00
** TRION.CAN (DeweSoft Plugin)          1.1.1858.00

* New Features:
** Added auto restore functionality to prevent loss of calibration data.

* New supported Modules:
** Any board supported by Trion Release 1.1

* Known Limitations:
** In rare cases the installer terminates unexpectedly at the end of the installation process. Since all components are already installed at his stage, this behavior has no further impact, and the system can be used as intended.
** After changing a TRION module, the name of the initially installed modules still shows up in Windows Device Manager.
** When disabling CAN in DeweSoft Hardware Setup Screen a restart of DeweSoft might be necessary.
** If DeweSoft has been used with old Trion.DAQ and Trion.CAN plugins, it is necessary to delete DeweSoft Default Project File (...\DEWESoft7\System\V7_0\Default.d7p).
** The SYNC I/O hardware interfaces on the TRION TIMING board are currently not supported.
** Timing: Setup GPS-In, IRIG-Out basically applies 21000ns between Master and Slave. Same behaviour with GPS-In PPS-Out.
   RESOLUTION: Consideration of the 21000ns within the missmatch value between Master and Slave with this specific configuration. In Sync-Configuration it is possible, to enter 21000ns into the cable length compensation on the slave system.
** DEWE2Explorer shows wrong attributes for some enclosures (e.g. power range).
** When having multiple DEWESoft versions installed, Trion.daq and Trion.can won't be replaced in all DEWESoft versions, only within the last opened version. Please check the version numbers of Trion.daq and Trion.can within DEWESoft Hardware Setup.


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2013-10-23 Release Notice DEWETRON TRION Software R1.1

* Version: 0.2013.1023.1843

* Components:
** DEWE2 Explorer                   	0.2.1843.00
** DEWE-TRION application library       0.36.1843.00
** DEWE-TRION system driver             0.0.0.35
** DEWE2 enclosure application library  0.2.1843.00
** DEWE2 enclosure system driver        0.01.1843.00
** DEWE-TRION board information         $Revision: 4412 $
** DEWE2 enclosure information          $Revision: 3776 $
** DEWE-TRION firmware revisions        $Revision: 3733 $
** TRION.DAQ (DeweSoft Plugin)          1.1.1843.00
** TRION.CAN (DeweSoft Plugin)          1.1.1843.00

* New supported Modules:
** Any board supported by Trion Release 1.0.1
** TRION-TIMING
** TRION-2402-dSTG.6.LE-S1

* Known Limitations:
** In rare cases the installer terminates unexpectedly at the end of the installation process. Since all components are already installed at his stage, this behavior has no further impact, and the system can be used as intended.
** After changing a TRION module, the name of the initially installed modules still shows up in Windows Device Manager.
** When disabling CAN in DeweSoft Hardware Setup Screen a restart of DeweSoft might be necessary.
** If DeweSoft has been used with old Trion.DAQ and Trion.CAN plugins, it is necessary to delete DeweSoft Default Project File (...\DEWESoft7\System\V7_0\Default.d7p).
** The SYNC I/O hardware interfaces on the TRION TIMING board are currently not supported.
** Timing: Setup GPS-In, IRIG-Out basically applies 21000ns between Master and Slave. Same behaviour with GPS-In PPS-Out.
   RESOLUTION: Consideration of the 21000ns within the missmatch value between Master and Slave with this specific configuration. In Sync-Configuration it is possible, to enter 21000ns into the cable length compensation on the slave system.
** DEWE2Explorer shows wrong attributes for some enclosures (e.g. power range).


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2013-07-23 Release Notice DEWETRON TRION Software R1.0.1

* Version: 0.2013.0722.4462

* Components:
** DEWE2 System Explorer                0.1.4393.00
** DewePXI API configuration library    0.1.4393.00
** DEWE-TRION application library       0.35.4390.00
** DEWE-TRION system driver             0.0.0.35
** DEWE2 enclosure application library  0.1.4345.00
** DEWE2 enclosure system driver        00.01.4344.00
** DEWE-TRION board information         $Revision: 4379 $
** DEWE2 enclosure information          $Revision: 3776 $
** DEWE-TRION firmware revisions        $Revision: 4387 $
** TRION.DAQ (DeweSoft Plugin)          4398
** TRION.CAN (DeweSoft Plugin)          4331

* New supported Modules:
** Any board supported by Trion Release 1
** TRION-CAN-.2.DB

* Known Limitations:
** In rare cases the installer terminates unexpectedly at the end of the installation process. Since all components are already installed at his stage, this behavior has no further impact, and the system can be used as intended.
** After changing a TRION module, the name of the initially installed modules still shows up in Windows Device Manager.
** When disabling CAN in DeweSoft Hardware Setup Screen a restart of DeweSoft might be necessary.
** If DeweSoft has been used with old Trion.DAQ and Trion.CAN plugins, it is necessary to delete DeweSoft Default Project File (...\DEWESoft7\System\V7_0\Default.d7p).


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2013-05-06 Release Notice DEWETRON TRION Software R1

* Version:  0.2013.0426.4390

* Components:
** DEWE2 System Explorer                0.1.4389.00
** DewePXI API configuration library    0.1.4389.00
** DEWE-TRION application library       0.35.4390.00
** DEWE-TRION system driver             0.0.0.35
** DEWE2 enclosure application library  0.1.4345.00
** DEWE2 enclosure system driver        00.01.4344.00
** DEWE-TRION board information         $Revision: 4379 $
** DEWE2 enclosure information          $Revision: 3776 $
** DEWE-TRION firmware revisions        $Revision: 4387 $
** TRION.DAQ (DeweSoft Plugin)          4371
** TRION.CAN (DeweSoft Plugin)          4331

* Supported Modules:
** TRION-2402-dACC.6.BN
** TRION-2402-dACC.8A.SB
** TRION-2402-dSTG.4.DB
** TRION-2402-dSTG.6.LE
** TRION-2402-dSTG.8.DB
** TRION-2402-dSTG.8.RJ
** TRION-2402-V.4.BA
** TRION-2402-V.4.BN
** TRION-2402-V.8.BA
** TRION-2402-V.8.BN
** TRION-BASE
** TRION-CAN-.22A.DB
** TRION-CAN-.4.DB
** TRION-CNT.6.LE
** TRION-CNT.6.LE
** TRION-DIO.3200A.MU
** TRION-DIO.4800.MU
(** TRION-CAN-.2.DB)

* Known Limitations:
** In rare cases the installer terminates unexpectedly at the end of the installation process. Since all components are already installed at his stage, this behavior has no further impact, and the system can be used as intended.
** After changing a TRION module, the name of the initially installed modules still shows up in Windows Device Manager.
** When disabling CAN in DeweSoft Hardware Setup Screen a restart of DeweSoft might be necessary.              
** If DeweSoft has been used with old Trion.DAQ and Trion.CAN plugins, it is necessary to delete DeweSoft Default Project File (...\DEWESoft7\System\V7_0\Default.d7p).
** Disabling DIO channels in Dewesoft Hardware Setup may corrupt digital measurement.
** TRION-CAN-.2.DB is not supported by this release.

