+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2020-06-29 Release Notice DEWETRON Oxygen R5.2.0 x64

* Components:
** DEWETRON Oxygen      R5.2.0   (5.2.0.55324)   (7fdcd54fb5a17fbe813c830d08a6a86a89efe987)

* Files:
** DEWETRON_Oxygen_Setup_R5.2.0_x64.exe
** DEWETRON_DMDReader_R5.2.0.zip

* Requirements:
** 5.x Software License required!
** OS: Windows 10 64bit, Windows 7 64bit
** CPU: Intel i5 3rd gen. or better
** RAM: 8 GB
** DAQ Hardware:
    * DEWETRON TRION and TRION3 (DEWETRON TRION Software R5.2.0)
    * DEWETRON ORION DAQ (ORION DAQ Driver V2.3.1.0)
    * DEWETRON ORION DSA (ORION DSA Driver V5.0.1.0)

* Installation procedure:
** TRION:
** Install TRION applications
** Reboot system (if requested by the installer)
** Start DEWETRON Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
** Power-cycle TRION boards (Power down system, then restart)
** Start DEWETRON Explorer and check for a successful firmware upgrade
** OXYGEN:
** Install Oxygen
** Verify HW settings in system menu on first startup

* New Features Oxygen:
** Channel-wise sample rate selector
   - Set individual sampling rates on the same board
   - Auto-Adjust of AAF
** Advanced storing modes
   - individual storing settings per channel
   - including skip mode for sample rate switch emulation
   - show "Statistics" data in all instruments
** Efficiency Map (Matrix Sampler)
   - Calculation Module for matrix sampling (X-Y -> Z)
   - used for efficiency map creation (matrix channel)
   - including interpolation in intensity diagram
   - requires OXY-OPT-POW-ADV
** Soundlevel Meter
   - Calculation module for sound level determination
   - A/B/C/D/Z frequency weighting
   - slow, fast, impulse time weighting
   - interval and continous mode
* Fixes:
** Export:
   - Fixed Acquisition Problems after AUTO-Export
   - Lower the MATLAB Compressed Export duration by 80%
   - MDF4: Export did not contain any data, if a CAN Message was selected
** CAN:
   - Fixed Problems with CAN-OUT at high data rate
   - DBC-Parser now can move on with DLC mismatch
   - J1939: Ignore priority and source address (if defined as 0xFE) in message id
** OXYGEN NET:
   - Fixed Memory increase in case of deactivating the statistics storage


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2020-05-04 Release Notice DEWETRON Oxygen R5.1.1 x64

* Components:
** DEWETRON Oxygen      R5.1.1	(5.1.1.54768)   (89a86d505f09155520a64b46b36ba53cf2ef6b86)

* Files:
** DEWETRON_Oxygen_Setup_R5.1.1_x64.exe

* Requirements:
** 5.x Software License required!
** OS: Windows 10 64bit, Windows 7 64bit
** CPU: Intel i5 3rd gen. or better
** RAM: 8 GB
** DAQ Hardware:
    * DEWETRON TRION and TRION3 (DEWETRON TRION Software R5.1.0)
    * DEWETRON ORION DAQ (ORION DAQ Driver V2.3.1.0)
    * DEWETRON ORION DSA (ORION DSA Driver V5.0.1.0)

* Installation procedure:
** TRION:
** Install TRION applications
** Reboot system (if requested by the installer)
** Start DEWETRON Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
** Power-cycle TRION boards (Power down system, then restart)
** Start DEWETRON Explorer and check for a successful firmware upgrade
** OXYGEN:
** Install Oxygen
** Verify HW settings in system menu on first startup

* New Features Oxygen:
** CAN-FD
   - Set Samplepoint and advanced timing parameter

* Fixes:
** Common:
   - OXYGEN crashes when switching AI to CAN
** Export:
   - XLSX-Export have wrong output format (text instead of value)
** MSI:
   - MSI2-STG, no balance action possible on CB16
   - MSI2-STG, bridge factor missing in settings
** Intensity Diagram:
   - Scaling broken after changes of channel settings
** Spectrum Analyzer:
   - Phase channel is not rendered correctly
** Snapshot Channels:
   - Sporadic NaN values when using aggregation (e.g. AVG)
** TRION-POWER:
    - SUB-Modules have ranges with wrong scaling
** SCPI:
   - Command STORE:FILE:NAME not applicable
   - Command :NUM:DIMS? does not report the right sample dimension
** XCP:
   - Use of same Oxygen setup leads to different A2L-file
   - A2L-file contains non usable channels (e.g. Power Group Channel)
   - Connect/Disconnect sometimes lead to deadlock of Oxygen
   - adapt visible names in A2L for better compatiblity with CANoe
   - Improved stability

* Changes:
** Power:
   - channel's samplerate for mechanical power must be less or equal to U/I channels
** FFT:
   - FFT-Group channel (complex) is not stored by default


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2020-03-30 Release Notice DEWETRON Oxygen R5.1.0 x64

* Components:
** DEWETRON Oxygen      R5.1.0	(5.1.0.54560)   (813c00d657afde62743a6ce131ae1608f2a8b4bc)

* Files:
** DEWETRON_Oxygen_Setup_R5.1.0_x64.exe
** DEWETRON_DMDReader_R5.1.0.zip

* Requirements:
** 5.x Software License required!
** OS: Windows 10 64bit, Windows 7 64bit
** CPU: Intel i5 3rd gen. or better
** RAM: 8 GB
** DAQ Hardware:
    * DEWETRON TRION and TRION3 (DEWETRON TRION Software R5.1.0)
    * DEWETRON ORION DAQ (ORION DAQ Driver V2.3.1.0)
    * DEWETRON ORION DSA (ORION DSA Driver V5.0.1.0)

* Installation procedure:
** TRION:
** Install TRION applications
** Reboot system (if requested by the installer)
** Start DEWETRON Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
** Power-cycle TRION boards (Power down system, then restart)
** Start DEWETRON Explorer and check for a successful firmware upgrade
** OXYGEN:
** Install Oxygen
** Verify HW settings in system menu on first startup

* New Features Oxygen:
** Vector FlexRay support
   - Supports Fibex 2.0 to 4.1.2
   - Decoding to individual signals with offline support
   - Intuitive channel picker
** CAN-Offline decoding
   - Intuitive channel picker
** File Browser
   - Oxygen file browser is able to create new folders
   - Oxygen file browser is able to use standard file explorer ("Browse..." button)
** Filesplit by absolute time
   - Allows filesplits on rounded absolute time
** Array access in formula
   - Access single array elements
** OXYGEN Viewer
   - Review data files in parallel to a running Oxygen.
** Update of 6-Phase Calculation (Power)
   - Changed 6P6W schematic to 2x3P3W.
** Oxygen SDK
   - Improvements due to first reviews. More on GitHub (https://github.com/DEWETRON/OXYGEN-SDK)
** Oxygen GUI Improvements
   - Channel list: Unused channel groups are automatically folded
   - Channel list: Math formula editor now supports multiline edit
   - Channel list: Simple channel type filter
   - Improved tooltips
   - Cursors can now be renamed (A/B cursor)
   - Text instrument: Can display measurement time

* Fixes:
** Actions: Zero and Bridge Balance action on large systems
** Power:Crash with power group in special combinations with XCP
** Power: Crash when deleting power group on a special customer setup
** Trigger: Triggered recording: recording does not restart after resync
** Oxygen Net: High memory consumption when using Pause mode
** FFT: Fixed an invalid sign jump in the phase calculation
** EPAD/DAQP: Crash that may happens on module scans with invalid module addresses
** MSI: Fixed a scaling issue with MSI2-STG-5V, added missing Bridge Factor input field


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2020-03-05 Release Notice DEWETRON Oxygen R5.0.3 x64

* Components:
** DEWETRON Oxygen      R5.0.3	(5.0.3.54295)   (5cfbb19288f85929d38e68795382aca08c382fbe)

* Files:
** DEWETRON_Oxygen_Setup_R5.0.3_x64.exe

* Requirements:
** 5.x Software License required!
** OS: Windows 10 64bit, Windows 7 64bit
** CPU: Intel i5 3rd gen. or better
** RAM: 8 GB
** DAQ Hardware:
    * DEWETRON TRION and TRION3 (DEWETRON TRION Software R5.0.0)
    * DEWETRON ORION DAQ (ORION DAQ Driver V2.3.1.0)
    * DEWETRON ORION DSA (ORION DSA Driver V5.0.1.0)

* Installation procedure:
** TRION:
** Install TRION applications
** Reboot system (if requested by the installer)
** Start DEWETRON Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
** Power-cycle TRION boards (Power down system, then restart)
** Start DEWETRON Explorer and check for a successful firmware upgrade
** OXYGEN:
** Install Oxygen
** Verify HW settings in system menu on first startup

* Fixes:
** GUI: Rendering of the channel mapping dialog took a long time.
** GUI: Cancelling the channel mapping dialog took a long time.
** GUI: Creation and adding a lot of channels to digital instruments was slow.
** Oxygen Net: High memory consumption on master and remote node.
** Oxygen Net: High cpu load with enabled gps channels.
** DAQP: DAQP modules could not be configured after loading a setup.


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2020-01-20 Release Notice DEWETRON Oxygen R5.0.1 x64

* Components:
** DEWETRON Oxygen      R5.0.1	(5.0.1.53790)   (1342c33387a7abfeeb8b40b9b10ab1a6f39a3033)

* Files:
** DEWETRON_Oxygen_Setup_R5.0.1_x64.exe

* Requirements:
** 5.x Software License required!
** OS: Windows 10 64bit, Windows 7 64bit
** CPU: Intel i5 3rd gen. or better
** RAM: 8 GB
** DAQ Hardware:
    * DEWETRON TRION and TRION3 (DEWETRON TRION Software R5.0.0)
    * DEWETRON ORION DAQ (ORION DAQ Driver V2.3.1.0)
    * DEWETRON ORION DSA (ORION DSA Driver V5.0.1.0)

* Installation procedure:
** TRION:
** Install TRION applications
** Reboot system (if requested by the installer)
** Start DEWETRON Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
** Power-cycle TRION boards (Power down system, then restart)
** Start DEWETRON Explorer and check for a successful firmware upgrade
** OXYGEN:
** Install Oxygen
** Verify HW settings in system menu on first startup

* Fixes:
** Fixed: Unresponsive UI interface issue


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2019-12-20 Release Notice DEWETRON Oxygen R5.0.0 x64

* Components:
** DEWETRON Oxygen      R5.0.0	(5.0.0.53695)   (92af9018aedf6425c0b19ec86f38a2ed9b071745)
** DEWETRON DMDReader   R5.0.0	(5.0.0.53690)   (83f10f6cc8f7f6f9b893372a2c8c8a75aa8bba99)

* Files:
** DEWETRON_Oxygen_Setup_R5.0.0_x64.exe
** DEWETRON_DMDReader_R5.0.0.zip

* Requirements:
** 5.x Software License required!
** OS: Windows 10 64bit, Windows 7 64bit
** CPU: Intel i5 3rd gen. or better
** RAM: 8 GB
** DAQ Hardware:
    * DEWETRON TRION and TRION3 (DEWETRON TRION Software R5.0.0)
    * DEWETRON ORION DAQ (ORION DAQ Driver V2.3.1.0)
    * DEWETRON ORION DSA (ORION DSA Driver V5.0.1.0)

* Installation procedure:
** TRION:
** Install TRION applications
** Reboot system (if requested by the installer)
** Start DEWETRON Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
** Power-cycle TRION boards (Power down system, then restart)
** Start DEWETRON Explorer and check for a successful firmware upgrade
** OXYGEN:
** Install Oxygen
** Verify HW settings in system menu on first startup

* New Features Oxygen:
** Mechanical Power Analysis
   - Mechanical power efficiency measurement synchronized to electrical power calculation
** Order Analysis
   - Noise and vibration analysis in rotating machines
   - Spectrogram instrument
** CAN J1939
   - decoding of J1939 Messages defined by a DBC file
** Oxygen SDK
   - Calculation & data interface plugin for Oxygen
   - Math extensions
   - Data interfaces
** Ethernet Sender Plugin
   - send Oxygen channel data via Ethernet (UDP)

* Fixes:
** Fixed: EPAD-data with snapshots resulted in very large files
** Fixed: Crash when changing the channel color in replay mode
** Fixed: Support for PAD-CB8-UNI-P2 added
** Fixed: CAN-FD, not all signals can be received if DLC does not cover all signals
** Fixed: Oxygen stops working with EtherCAT, acquisition didn't start
** Fixed: Non-consistent column order in text based exports; now using system topology
** Fixed: Auto-Export with file split only exports last split; corrected misleading export file name
** Fixed: Problems receiving CAN-Messages faster than than set samplerate

* Known Limitations, general (additional to Oxygen 3.7.0):


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2020-03-05 Release Notice DEWETRON Oxygen R3.7.1 x64

* Components:
** DEWETRON Oxygen      R3.7.1	(3.7.1.54298)   (4b37f08fa8f3c9dc677d70bfc643b69957046738)

* Requirements:
** 3.x Software License required!
** OS: Windows 10 64bit, Windows 7 64bit
** CPU: Intel i5 3rd gen. or better
** RAM: 8 GB
** DAQ Hardware:
    * DEWETRON TRION (DEWETRON TRION Software R3.7.0)
    * DEWETRON ORION DAQ (ORION DAQ Driver V2.3.1.0)
    * DEWETRON ORION DSA (ORION DSA Driver V5.0.1.0)

* Installation procedure:
** Uninstall previous Oxygen version
** Uninstall any previous TRION version via system uninstall (control panel).
** Reboot system
** Install TRION applications
** Reboot system
** Start DEWETRON Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
** Power-cycle TRION boards (Power down system, then restart)
** Install Oxygen
** Verify HW settings in system menu on first startup

* Fixes:
** GUI: Improved German translation
** DMD-Export: Fixed writing invalid data in source dmd file when saving after dmd export
** Oxygen Net: Fixed spurious instabilities on Windows Nodes (zmq upgrade to 4.3.2)
** Oxygen Net: Fixed an issue concerning high memory consumption.
** DAQP: Fixed an issue when DAQP modules could not be configured after loading a setup.


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2019-09-27 Release Notice DEWETRON Oxygen R3.7.0 x64

* Components:
** DEWETRON Oxygen      R3.7.0	(3.7.0.52578)   (ab62f024664ad23dd1f3c94e33d6c31c6b5bbf17)
** DEWETRON DMDReader   R3.7.0	(3.7.0.52578)   (ab62f024664ad23dd1f3c94e33d6c31c6b5bbf17)

* Files:
** DEWETRON_Oxygen_Setup_R3.7.0_x64.exe
** DEWETRON_DMDReader_R3.7.0.zip

* Requirements:
** 3.x Software License required!
** OS: Windows 10 64bit, Windows 7 64bit
** CPU: Intel i5 3rd gen. or better
** RAM: 8 GB
** DAQ Hardware:
    * DEWETRON TRION (DEWETRON TRION Software R3.7.0)
    * DEWETRON ORION DAQ (ORION DAQ Driver V2.3.1.0)
    * DEWETRON ORION DSA (ORION DSA Driver V5.0.1.0)

* Installation procedure:
***TRION:
** Uninstall previous Oxygen version
** Uninstall any previous TRION version via system uninstall (control panel).
** Reboot system
** Install TRION applications
** Reboot system
** Start DEWETRON Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
** Power-cycle TRION boards (Power down system, then restart)
** Install Oxygen
** Verify HW settings in system menu on first startup

* New Features Oxygen:
** HW support:
   -MSI-RTD adapter
   -MSI2 adapters
   -TRION[3]-18xx-POWER-4 Delay Compensation (phase-align current input)
** Sensor Database
   -choose sensor scaling/amplifier settings from editable database
** Table Scaling
** IIR Filter:
   -Bandpass and Bandstop filter
** Usability:
   -dark measurement screen
   -enter filename at recording start
   -export to DMD
   -export between cursors

* Support of MSI2-Adapters:
** MSI2-TH-x
** MSI2-250R-20mA
** MSI2-LVDT
** MSI2-STG-5V
** MSI2-STG-10V
** MSI2-CH-5
** MSI2-CH-100

* Fixes:
** GUI: now ready for HDPI-Screens, automatic setting of scaling for better compatibility on 4k+ Displays
** CAN-OUT: much faster response in channel list when switching to transmit, fixed possible crash when using many transmit-messages
** dmd reader: correct behaviour when reading multifile-parts
** Oxygen Net: correct behaviour when using IRIG with no DIOs enabled
** Matlab-Export: Fixed problems with export of long-term measurements
** FFT: better performance of big FFT-calculations which lead to "High math load" warning
** Highspeed: Fixed problems using fast TRION3-Modules which caused "Unable to read data" Error

* Known Limitations, general (additional to Oxygen 3.6):
** DMD-Export: May not work correctly with multifile-parts and offline calculated channels
** DMD-Export: Changes in setup will only be exported when saved before to origin file
** DMD-Export: Offline created channels will only be exported when saved before to origin file
** DMD-Export: Orange cursor in reporting pages will not be moved to exported area


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
Release Notice DEWETRON Oxygen R3.6.2 x64

* Components:
** DEWETRON Oxygen	R3.6.2	(3.6.2.52069)    	(52df705a52293001a167bbe6af3ac28749fcad3d)
** DEWETRON DMDReader	R3.6.2	(3.6.2.52078)   (3063d6e712244463046e617045397fd721f52a2b)

* Files:
** DEWETRON_Oxygen_Setup_R3.6.2_x64.exe
** DEWETRON_DMDReader_R3.6.2.zip

* Requirements:
** 3.x Software License required!
** OS: Windows 7 64bit, Windows 10 64bit
** CPU: Intel i5 3rd gen. or better
** RAM: 8 GB
** DAQ Hardware:
    * DEWETRON TRION (DEWETRON TRION Software R3.6.2)
    * DEWETRON ORION DAQ (ORION DAQ Driver V2.3.1.0)
    * DEWETRON ORION DSA (ORION DSA Driver V5.0.1.0)

* Installation procedure:
***TRION:
** Uninstall previous Oxygen version
** Uninstall any previous TRION version via system uninstall (control panel).
** Reboot system
** Install TRION applications
** Reboot system
** Start DEWETRON Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
** Power-cycle TRION boards (Power down system, then restart)
** Install Oxygen
** Verify HW settings in system menu on first startup

* Fixes:
** Fix for TRIONET IRIG Sync issue
** dmd reader: skip periods where sync channel data cannot be loaded from file


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
Release Notice DEWETRON Oxygen R3.6.1 x64

* Components:
** DEWETRON Oxygen	R3.6.1	(3.6.1.51676)    (e01a7680af16)
** DEWETRON DMDReader	R3.6	(3.6.0.51621)    (50d68b8a6678)

* Files:
** DEWETRON_Oxygen_Setup_R3.6.1_x64.exe
** DEWETRON_DMDReader_R3.6.zip

* Requirements:
** 3.x Software License required!
** OS: Windows 7 64bit, Windows 10 64bit
** CPU: Intel i5 3rd gen. or better
** RAM: 8 GB
** DAQ Hardware:
    * DEWETRON TRION (DEWETRON TRION Software R3.6.0)
    * DEWETRON ORION DAQ (ORION DAQ Driver V2.3.1.0)
    * DEWETRON ORION DSA (ORION DSA Driver V5.0.1.0)

* Installation procedure:
***TRION:
** Uninstall previous Oxygen version
** Uninstall any previous TRION version via system uninstall (control panel).
** Reboot system
** Install TRION applications
** Reboot system
** Start Dewe2Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
** Power-cycle TRION boards (Power down system, then restart)
** Install Oxygen
** Verify HW settings in system menu on first startup

* Fixes:
Installer does not end after successful installation


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
Release Notice DEWETRON Oxygen R3.6 x64

* Components:
** DEWETRON Oxygen	R3.6	(3.6.0.51634)    (bd159c1a85ad)
** DEWETRON DMDReader	R3.6	(3.6.0.51621)    (50d68b8a6678)

* Files:
** DEWETRON_Oxygen_Setup_R3.6_x64.exe
** DEWETRON_DMDReader_R3.6.zip

* Requirements:
** 3.x Software License required!
** OS: Windows 7 64bit, Windows 10 64bit
** CPU: Intel i5 3rd gen. or better
** RAM: 8 GB
** DAQ Hardware:
    * DEWETRON TRION (DEWETRON TRION Software R3.6.0)
    * DEWETRON ORION DAQ (ORION DAQ Driver V2.3.1.0)
    * DEWETRON ORION DSA (ORION DSA Driver V5.0.1.0)

* Installation procedure:
***TRION:
** Uninstall previous Oxygen version
** Uninstall any previous TRION version via system uninstall (control panel).
** Reboot system
** Install TRION applications
** Reboot system
** Start Dewe2Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
** Power-cycle TRION boards (Power down system, then restart)
** Install Oxygen
** Verify HW settings in system menu on first startup

* New Features Oxygen:
** HW support:
   -MSI adapters
   -TRION-18xx-MULTI
   -Vector CAN/CAN-FD USB interfaces
** Swept Sine Analysis
** Power: Rolling calculation pt.2
** SCPI+XCP simultaneous operation
** Ethernet Receiver time-sync option
** Automatic Export
** Math Formula additions
** Usability:
   -lock timebase for multiple recorders

* New Features Oxygen NET: 		
-


* HW Support:
***TRION - all supported modules	(Supported Measurement mode):
** TRION-1620-ACC-6-BNC			(Voltage, SW Current, IEPE, Simple CNT)
** TRION-1620-LV-6-BNC			(Voltage, SW Current)
** TRION-1620-LV-6-L1B			(Voltage, Current)
** TRION-1603-LV-6-BNC			(Voltage, SW Current)
** TRION-1603-LV-6-L1B			(Voltage, SW Current)
** TRION-1603-LV-6-D25			(Voltage, SW Current)
** TRION-2402-MULTI-4-D			(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE, CAN, MSI(%1))
** TRION-2402-MULTI-8-L0B		(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE, CAN, MSI(%1))
** TRION-2402-dSTG-6-L1B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-D			(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-L0B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-RJ			(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2400-dSTG-8-L0B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dACC-6-BNC		(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-dACC-8-SMB		(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-dACC-8-MD			(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-V-4-B			(Voltage, SW Current)
** TRION-2402-V-8-B			(Voltage, SW Current)
** TRION-CNT-6-L1B			(Simple CNT, Frequency)
** TRION-BASE				(IRIG B DC synchronization, PPS sync, Simple CNT, Frequency, DI, DO)
** TRION-TIMING				(IRIG A AC or DC, IRIG B AC or DC, PPS sync, GPS time sync + position, DI, DO)
** TRION-TIMING-V2			(IRIG A AC or DC, IRIG B AC or DC, PPS sync, GPS time sync + position, DI, DO)
** TRION-TIMING-V3			(PTP, IRIG A AC or DC, IRIG B AC or DC, PPS sync, GPS time sync + position, DI, DO)
** TRION-VGPS-20			(PPS sync, GPS time sync + position, Simple CNT, Frequency, DI, DO)
** TRION-VGPS-100			(PPS sync, GPS time sync + position, Simple CNT, Frequency, DI, DO)
** TRION-VGPS-20-V3			(PTP, IRIG A AC or DC, IRIG B AC or DC, PPS sync, GPS time sync + position, DI, DO)
** TRION-VGPS-100-V3			(PTP, IRIG A AC or DC, IRIG B AC or DC, PPS sync, GPS time sync + position, DI, DO)
** TRION-CAN-4				(CAN)
** TRION-CAN-2				(CAN)
** TRION-DI48				(DI)
** TRION-1802				(Voltage, SW Current)	[RS-485 + DAQP support]	[CB16 + MSI(%2) support]
** TRION-1600				(Voltage, SW Current)	[RS-485 + DAQP support]	[CB16 + MSI(%2) support]
** TRION-1820-POWER-4			(Voltage, Current($))
** TRION-1810-HV-4			(Voltage)
** TRION-1810M-POWER-4			(Voltage, Current($))
** TRION3-1810M-POWER-4			(Voltage, Current($))
** TRION-1820-MULTI-4-D			(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE, CAN, MSI(%1))
** TRION3-1820-MULTI-4-D		(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE, CAN, MSI(%1))
** TRION3-1820-MULTI-8-L0B		(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE, CAN, MSI(%1))
** TRION3-1850-MULTI-4-D		(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE, CAN, MSI(%1))
** TRION3-1850-MULTI-8-L0B		(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE, CAN, MSI(%1))

(%1) MSI on TRION-x-MULTI series
MSI-BR-TH-x				(Temperature)
MSI-BR-TH-x-V2				(Temperature)
MSI-BR-V-200				(Voltage)
MSI-BR-CH-x				(Charge)
MSI-BR-CH-x-V2				(Charge)
MSI-BR-LVDT				(LVDT)

(%2) MSI on CB16 connector box
MSI-BR-TH-x-V2				(Temperature)
MSI-BR-ACC-x				(IEPE)
MSI-BR-V-200				(Voltage)
MSI-BR-CH-x				(Charge)
MSI-BR-CH-x-V2				(Charge)
MSI-BR-LA-250R-20mA			(Current)
MSI-BR-LVDT				(LVDT)
MSI-BR-STG-5V				(Bridge)
MSI-BR-STG-10V				(Bridge)
Do not use MSI-BR-TH-x MSI types (very noisy)!


($) Current module required for Current mode:
* SUB-dLV-1				(Current)
* SUB-CUR-20A-1				(Current)
* SUB-CUR-2A-1				(Current)
* SUB-CUR-02A-1				(Current)
* SUB-CUR-1A-1				(Current)


***EPAD - all supported modules		(Supported Measurement mode):
** EPAD2-TH8-x				(Temperature, Voltage)
** EPAD2-TH8-UNIVERSAL			(Temperature, Voltage)
** EPAD2-V8				(Voltage)
** EPAD2-RTD8				(Temperature, Resistance)
** EPAD2-TH8-P				(Temperature(�), Voltage)
** EPAD2-LA8				(Current)
** EPAD -V8				(Voltage)
** EPAD -TH8-P				(Temperature(�), Voltage)

***PAD - all supported modules		(Supported Measurement mode):
** PAD-TH8-P				(Temperature(�), Voltage)
** PAD-V8-P				(Voltage)
** PAD-DO7				(DO)

(�) Connector block required for Temperature mode:
* PAD-CB8-x-P2				(Temperature)
* PAD-CB8-x-M				(Temperature)
* PAD-CB8-RTD-S3			(Temperature)


***ORION - all supported boards		(Supported Input type):
*  ORION DAQ Series (16 bit):
** ORION-0816-10M(%)			(Analog in, CAN)
** ORION-0816-5M (%)			(Analog in, CAN)
** ORION-0816-1000			(Analog in, CAN)
** ORION-0816-500			(Analog in, CAN)
** ORION-1616-10x			(Analog in, CAN)
** ORION-1616-100x			(Analog in, CAN)
** ORION-3216-10x			(Analog in, CAN)
*  ORION DSA Series (24 bit):
** ORION-1624-20x			(Analog in, CAN)
(%)data storing speed depends on hardware configuration
CAN only available on CAN enabled boards


***HSI/DAQP - all supported modules	(Supported Measurement mode):
** HSI-HV				(Voltage, SW Current)
** HSI-LV				(Voltage, SW Current)
** DAQP-HV				(Voltage, SW Current)
** DAQP-LV				(Voltage, SW Current)
** DAQP-STG				(Voltage, SW Current, Resistance, Bridge)
** HSI-STG				(Voltage, SW Current, Resistance, Bridge)
** DAQP-BRIDGE-A			(Voltage, SW Current, Bridge)
** DAQP-BRIDGE-B			(Voltage, SW Current, Bridge)
** DAQP-FREQ-A				(Frequency)
** DAQP-CFB2				(Bridge, Capacitance)
** DAQP-CHARGE-B			(Charge)
** DAQP-CHARGE-A			(Charge)
** DAQP-MULTI				(Voltage, SW Current, Resistance, Bridge, Temperature)
** DAQP-THERM				(Temperature)
** DAQP-ACC-A				(IEPE)
** DAQP-LA				(Current)
** DAQP-V				(Voltage, SW Current)
** DAQP-V-A				(Voltage, SW Current)
** DAQP-V-B				(Voltage, SW Current)
!All other modules not tested!

DI = Digital in
DO = Digital out


* Known Limitations, general:
** Single value channel export (Swept sine analysis) may not work for MATLAB and MDF4
** Statistics window may be adjusted automatically, to prevent drifting on rounded values
** Total number of DAQP/HSI/PAD/EPAD modules on each serial port is limited to 32 (scan range 0-31)
** Slow data is used as an export option and can only be viewed in recorder instruments within Oxygen
** dejaVIEW may experience degrading performance on long slow async data recordings
** DMD recovery may lead to non perfect results, depending on filesize, sampling rate, no. of channels and channel type
** Only a reduced number of triggers is shown in recorder instruments
** PCI bus overload may lead to Oxygen fault

* Known Limitations, Oxygen NET:
** Swept sine analysis calculation on net slaves not recommended, transfer data to master and calculate there instead
** TRION-SYNC-BUS on DEWE3 enclosures only updated in GUI after manual acquisition restart
** With TRION-TIMING/VGPS V3 in DEWE3 installed, TRION-SYNC-BUS out not working
** When using an Oxygen NET master without TRION HW in a NET system with IRIG/PTP/GPS sync, the TRION DAQ plugin on the master must be disabled for the system to start
** Oxygen NET slave node not starting, if TRION-SYNC-BUS is used, and TRION-TIMING-V3 module is installed and no channels are active
** results of global actions can be bad when using MSIs
** Setup on Slaves containing statistic, filter or FFT channels, may not be loaded if "load last setup" option on Slaves is active
   (Recommendation: do not use "load last setup" on Oxygen NET Slaves)
** Recording-trigger settings only valid on Master node, Slave recording-triggers are ignored (other triggers on Slave are still valid)
** PC Master with manual sync settings set to "internal" leads to free-running measurement (unsynchronized)
** on Master node the last sample of async channels may not be transferred
** claiming nodes takes a long time with active ADMA plugin
** auto-sync settings recommended (Master: Internal (no absolute time-sync), Slaves: TRION-SYNC-bus only), manual sync mode is only used under special circumstances
** TRIONet: dynamic connect/disconnect not supported

* Known Limitations with TRION:
-

* Known Limitations with ORION:
** ORION-CNT not supported
** ORION-DI, DO not supported
** DAQ AD-boards: fixed AIRef set to Sense
** DSA AD-boards: only 5V AI range available (AIRef set to GND)
                  10V range for DAQP racks not supported (but is selectable in SW)


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
Release Notice DEWETRON Oxygen R3.5.2 x64

* Components:
** DEWETRON Oxygen	R3.5.2	(3.5.2.51070)    (afac96bb75b7)
** DEWETRON DMDReader	R3.5	(3.5.50091.0)    (513462417f78)

* Files:
** DEWETRON_Oxygen_Setup_R3.5.2_x64.exe
** DEWETRON_DMDReader_R3.5.zip

* Requirements:
** 3.x Software License required!
** OS: Windows 7 64bit, Windows 10 64bit
** CPU: Intel i5 3rd gen. or better
** RAM: 8 GB
** DAQ Hardware:
    * DEWETRON TRION (DEWETRON TRION Software R3.5.2)
    * DEWETRON ORION DAQ (ORION DAQ Driver V2.3.1.0)
    * DEWETRON ORION DSA (ORION DSA Driver V5.0.1.0)

* Installation procedure:
***TRION:
** Uninstall previous Oxygen version
** Uninstall any previous TRION version via system uninstall (control panel).
** Reboot system
** Install TRION applications
** Reboot system
** Start Dewe2Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
** Power-cycle TRION boards (Power down system, then restart)
** Install Oxygen
** Verify HW settings in system menu on first startup

* New Features Oxygen:
-

* New Features Oxygen NET: 		
-

* Fixes:
** IRIG synchronization accuracy
** Instruments in live mode now show data of non-recorded channels


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
Release Notice DEWETRON Oxygen R3.5.1 x64

* Components:
** DEWETRON Oxygen	R3.5.1	(3.5.1.50716)    (6684dea98430)
** DEWETRON DMDReader	R3.5	(3.5.50091.0)    (513462417f78)

* Files:
** DEWETRON_Oxygen_Setup_R3.5.1_x64.exe
** DEWETRON_DMDReader_R3.5.zip

* Requirements:
** 3.x Software License required!
** OS: Windows 7 64bit, Windows 10 64bit
** CPU: Intel i5 3rd gen. or better
** RAM: 8 GB
** DAQ Hardware:
    * DEWETRON TRION (DEWETRON TRION Software R3.5.0)
    * DEWETRON ORION DAQ (ORION DAQ Driver V2.3.1.0)
    * DEWETRON ORION DSA (ORION DSA Driver V5.0.1.0)

* Installation procedure:
***TRION:
** Uninstall previous Oxygen version
** Uninstall any previous TRION version via system uninstall (control panel).
** Reboot system
** Install TRION applications
** Reboot system
** Start Dewe2Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
** Power-cycle TRION boards (Power down system, then restart)
** Install Oxygen
** Verify HW settings in system menu on first startup

* New Features Oxygen:
** Automated Export during recording
** Psopometer calculation Plugin	[License required]

* New Features Oxygen NET: 		
-


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
Release Notice DEWETRON Oxygen R3.5 x64

* Components:
** DEWETRON Oxygen	R3.5	(3.5.0.50470)    (cc0275d4a8c5)
** DEWETRON DMDReader	R3.5	(3.5.50091.0)    (513462417f78)

* Files:
** DEWETRON_Oxygen_Setup_R3.5_x64.exe
** DEWETRON_DMDReader_R3.5.zip

* Requirements:
** 3.x Software License required!
** OS: Windows 7 64bit, Windows 10 64bit
** CPU: Intel i5 3rd gen. or better
** RAM: 8 GB
** DAQ Hardware:
    * DEWETRON TRION (DEWETRON TRION Software R3.5.0)
    * DEWETRON ORION DAQ (ORION DAQ Driver V2.3.1.0)
    * DEWETRON ORION DSA (ORION DSA Driver V5.0.1.0)

* Installation procedure:
***TRION:
** Uninstall previous Oxygen version
** Uninstall any previous TRION version via system uninstall (control panel).
** Reboot system
** Install TRION applications
** Reboot system
** Start Dewe2Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
** Power-cycle TRION boards (Power down system, then restart)
** Install Oxygen
** Verify HW settings in system menu on first startup

* New Features Oxygen:
** HW support:
   -PA8
   -CB16
   -TRION-18xx-MULTI DEMO support (not all features finalized)
** Power: Rolling calculation
** TB-CAN out
** Bird�s Eye Arc object
** Usability:
   -Reset to defaults (�New setup�)
   -Auto-start recording
   -CAN, set timebase option

* New Features Oxygen NET: 		
** Oxygen NET, external sync (IRIG, GPS, PTP)


* HW Support:
***TRION - all supported modules	(Supported Measurement mode):
** TRION-1620-ACC-6-BNC			(Voltage, SW Current, IEPE, Simple CNT)
** TRION-1620-LV-6-BNC			(Voltage, SW Current)
** TRION-1620-LV-6-L1B			(Voltage, Current)
** TRION-1603-LV-6-BNC			(Voltage, SW Current)
** TRION-1603-LV-6-L1B			(Voltage, SW Current)
** TRION-1603-LV-6-D25			(Voltage, SW Current)
** TRION-2402-MULTI-4-D			(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE, CAN, MSI(%1))
** TRION-2402-MULTI-8-L0B		(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE, CAN, MSI(%1))
** TRION-2402-dSTG-6-L1B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-D			(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-L0B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-RJ			(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2400-dSTG-8-L0B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dACC-6-BNC		(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-dACC-8-SMB		(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-dACC-8-MD			(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-V-4-B			(Voltage, SW Current)
** TRION-2402-V-8-B			(Voltage, SW Current)
** TRION-CNT-6-L1B			(Simple CNT, Frequency)
** TRION-BASE				(IRIG B DC synchronization, PPS sync, Simple CNT, Frequency, DI, DO)
** TRION-TIMING				(IRIG A AC or DC, IRIG B AC or DC, PPS sync, GPS time sync + position, DI, DO)
** TRION-TIMING-V2			(IRIG A AC or DC, IRIG B AC or DC, PPS sync, GPS time sync + position, DI, DO)
** TRION-TIMING-V3			(PTP, IRIG A AC or DC, IRIG B AC or DC, PPS sync, GPS time sync + position, DI, DO)
** TRION-VGPS-20			(PPS sync, GPS time sync + position, Simple CNT, Frequency, DI, DO)
** TRION-VGPS-100			(PPS sync, GPS time sync + position, Simple CNT, Frequency, DI, DO)
** TRION-VGPS-20-V3			(PTP, IRIG A AC or DC, IRIG B AC or DC, PPS sync, GPS time sync + position, DI, DO)
** TRION-VGPS-100-V3			(PTP, IRIG A AC or DC, IRIG B AC or DC, PPS sync, GPS time sync + position, DI, DO)
** TRION-CAN-4				(CAN)
** TRION-CAN-2				(CAN)
** TRION-DI48				(DI)
** TRION-1802				(Voltage, SW Current)	[RS-485 + DAQP support]	[CB16 + MSI(%2) support]
** TRION-1600				(Voltage, SW Current)	[RS-485 + DAQP support]	[CB16 + MSI(%2) support]
** TRION-1820-POWER-4			(Voltage, Current($))
** TRION-1810-HV-4			(Voltage)
** TRION-1810M-POWER-4			(Voltage, Current($))
** TRION3-1810M-POWER-4			(Voltage, Current($))
** TRION-1820-MULTI-4-D�		(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE, CAN, MSI(%1))
** TRION-1850-MULTI-4-D�		(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE, CAN, MSI(%1))
** TRION3-1820-MULTI-4-D�		(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE, CAN, MSI(%1))
** TRION3-1820-MULTI-8-L0B�		(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE, CAN, MSI(%1))
** TRION3-1850-MULTI-4-D�		(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE, CAN, MSI(%1))
** TRION3-1850-MULTI-8-L0B�		(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE, CAN, MSI(%1))
� DEMO only, not all features finalized

(%1) MSI on TRION-x-MULTI series
MSI-BR-TH-x				(Temperature)
MSI-BR-ACC				(IEPE)
MSI-BR-V-200				(Voltage)
MSI-BR-RTD				(Temperature)
MSI-BR-CH-x				(Charge)

(%2) MSI on CB16 connector box
MSI-BR-TH-x-V2�				(Temperature)
MSI-BR-ACC��				(IEPE)
MSI-BR-V-200				(Voltage)
MSI-BR-RTD�				(Temperature)
MSI-BR-CH-x��				(Charge)
MSI-BR-LA-250R-20mA			(Current)
MSI-BR-LVDT				(LVDT)
MSI-BR-STG-5V				(Bridge)
MSI-BR-STG-10V				(Bridge)
�/�� DEMO only, linearization� and SoftHP�� not yet available

($) Current module required for Current mode:
* SUB-dLV-1				(Current)
* SUB-CUR-20A-1				(Current)
* SUB-CUR-2A-1				(Current)
* SUB-CUR-02A-1				(Current)

***EPAD - all supported modules		(Supported Measurement mode):
** EPAD2-TH8-x				(Temperature, Voltage)
** EPAD2-TH8-UNIVERSAL			(Temperature, Voltage)
** EPAD2-V8				(Voltage)
** EPAD2-RTD8				(Temperature, Resistance)
** EPAD2-TH8-P				(Temperature(�), Voltage)
** EPAD2-LA8				(Current)
** EPAD -V8				(Voltage)
** EPAD -TH8-P				(Temperature(�), Voltage)

***PAD - all supported modules		(Supported Measurement mode):
** PAD-TH8-P				(Temperature(�), Voltage)
** PAD-V8-P				(Voltage)
** PAD-DO7				(DO)

(�) Connector block required for Temperature mode:
* PAD-CB8-x-P2				(Temperature)
* PAD-CB8-x-M				(Temperature)
* PAD-CB8-RTD-S3			(Temperature)


***ORION - all supported boards		(Supported Input type):
*  ORION DAQ Series (16 bit):
** ORION-0816-10M(%)			(Analog in, CAN)
** ORION-0816-5M (%)			(Analog in, CAN)
** ORION-0816-1000			(Analog in, CAN)
** ORION-0816-500			(Analog in, CAN)
** ORION-1616-10x			(Analog in, CAN)
** ORION-1616-100x			(Analog in, CAN)
** ORION-3216-10x			(Analog in, CAN)
*  ORION DSA Series (24 bit):
** ORION-1624-20x			(Analog in, CAN)
(%)data storing speed depends on hardware configuration
CAN only available on CAN enabled boards


***HSI/DAQP - all supported modules	(Supported Measurement mode):
** HSI-HV				(Voltage, SW Current)
** HSI-LV				(Voltage, SW Current)
** DAQP-HV				(Voltage, SW Current)
** DAQP-LV				(Voltage, SW Current)
** DAQP-STG				(Voltage, SW Current, Resistance, Bridge)
** HSI-STG				(Voltage, SW Current, Resistance, Bridge)
** DAQP-BRIDGE-A			(Voltage, SW Current, Bridge)
** DAQP-BRIDGE-B			(Voltage, SW Current, Bridge)
** DAQP-FREQ-A				(Frequency)
** DAQP-CFB2				(Bridge, Capacitance)
** DAQP-CHARGE-B			(Charge)
** DAQP-CHARGE-A			(Charge)
** DAQP-MULTI				(Voltage, SW Current, Resistance, Bridge, Temperature)
** DAQP-THERM				(Temperature)
** DAQP-ACC-A				(IEPE)
** DAQP-LA				(Current)
** DAQP-V				(Voltage, SW Current)
** DAQP-V-A				(Voltage, SW Current)
** DAQP-V-B				(Voltage, SW Current)
!All other modules not tested!

DI = Digital in
DO = Digital out


* Known Limitations, general:
** Statistics window may be adjusted automatically, to prevent drifting on rounded values
** Total number of DAQP/HSI/PAD/EPAD modules on each serial port is limited to 32 (scan range 0-31)
** Slow data is used as an export option and can only be viewed in recorder instruments within Oxygen
** dejaVIEW may experience degrading performance on long slow async data recordings
** DMD recovery may lead to non perfect results, depending on filesize, sampling rate, no. of channels and channel type
** Only a reduced number of triggers is shown in recorder instruments
** PCI bus overload may lead to Oxygen fault

* Known Limitations, Oxygen NET:
** When using an Oxygen NET master without TRION HW in a NET system with IRIG/PTP/GPS sync, the TRION DAQ plugin on the master must be disabled for the system to start
** Oxygen NET slave node not starting, if TRION-SYNC-BUS is used, and TRION-TIMING-V3 module is installed and no channels are active
** results of global actions can be bad when using MSIs
** Setup on Slaves containing statistic, filter or FFT channels, may not be loaded if "load last setup" option on Slaves is active
   (Recommendation: do not use "load last setup" on Oxygen NET Slaves)
FIXED ** Absolute recording time between Master and Slave may not be synchronized - depending on sync settings
** Recording-trigger settings only valid on Master node, Slave recording-triggers are ignored (other triggers on Slave are still valid)
** PC Master with manual sync settings set to "internal" leads to free-running measurement (unsynchronized)
** on Master node the last sample of async channels may not be transferred
** claiming nodes takes a long time with active ADMA plugin
** auto-sync settings recommended (Master: Internal (no absolute time-sync), Slaves: TRION-SYNC-bus only), manual sync mode is only used under special circumstances
** TRIONet: dynamic connect/disconnect not supported

* Known Limitations with TRION:
-

* Known Limitations with ORION:
** ORION-CNT not supported
** ORION-DI, DO not supported
** DAQ AD-boards: fixed AIRef set to Sense
** DSA AD-boards: only 5V AI range available (AIRef set to GND)
                  10V range for DAQP racks not supported (but is selectable in SW)


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
Release Notice DEWETRON Oxygen R3.4.2 x64

* Components:
** DEWETRON Oxygen	R3.4.2	(3.4.2.49868)    (05c80087c4a9)
** DEWETRON DMDReader	R3.3	(3.3.47204.0)    (2dcf0e3ffa70)

* Files:
** DEWETRON_Oxygen_Setup_R3.4.2_x64.exe
** DEWETRON_DMDReader_R3.3.zip

* Requirements:
** 3.x Software License required!
** OS: Windows 7 64bit, Windows 10 64bit
** CPU: Intel i5 3rd gen. or better
** RAM: 8 GB
** DAQ Hardware:
    * DEWETRON TRION (DEWETRON TRION Software R3.4.0)
    * DEWETRON ORION DAQ (ORION DAQ Driver V2.3.1.0)
    * DEWETRON ORION DSA (ORION DSA Driver V5.0.1.0)

* Installation procedure:
***TRION:
** Uninstall previous Oxygen version
** Uninstall any previous TRION version via system uninstall (control panel).
** Reboot system
** Install TRION applications
** Reboot system
** Start Dewe2Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
** Power-cycle TRION boards (Power down system, then restart)
** Install Oxygen
** Verify HW settings in system menu on first startup

* New Features Oxygen:
** TRION-18xx-MULTI DEMO support
* New Features Oxygen NET: 		
-

* HW Support:
***TRION - all supported modules	(Supported Measurement mode):
** TRION-1620-ACC-6-BNC			(Voltage, SW Current, IEPE, Simple CNT)
** TRION-1620-LV-6-BNC			(Voltage, SW Current)
** TRION-1620-LV-6-L1B			(Voltage, Current)
** TRION-1603-LV-6-BNC			(Voltage, SW Current)
** TRION-1603-LV-6-L1B			(Voltage, SW Current)
** TRION-1603-LV-6-D25			(Voltage, SW Current)
** TRION-2402-MULTI-4-D			(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE, CAN, MSI(%))
** TRION-2402-MULTI-8-L0B		(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE, CAN, MSI(%))
** TRION-2402-dSTG-6-L1B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-D			(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-L0B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-RJ			(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2400-dSTG-8-L0B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dACC-6-BNC		(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-dACC-8-SMB		(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-dACC-8-MD			(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-V-4-B			(Voltage, SW Current)
** TRION-2402-V-8-B			(Voltage, SW Current)
** TRION-CNT-6-L1B			(Simple CNT, Frequency)
** TRION-BASE				(IRIG B DC synchronization, PPS sync, Simple CNT, Frequency, DI, DO)
** TRION-TIMING				(IRIG A AC or DC, IRIG B AC or DC, PPS sync, GPS time sync + position, DI, DO)
** TRION-TIMING-V2			(IRIG A AC or DC, IRIG B AC or DC, PPS sync, GPS time sync + position, DI, DO)
** TRION-TIMING-V3			(PTP, IRIG A AC or DC, IRIG B AC or DC, PPS sync, GPS time sync + position, DI, DO) [TRION R3.3]
** TRION-VGPS-x				(PPS sync, GPS time sync + position, Simple CNT, Frequency, DI, DO)
** TRION-CAN-4				(CAN)
** TRION-CAN-2				(CAN)
** TRION-DI48				(DI)
** TRION-1802				(Voltage, SW Current)	[incl. RS-485 + DAQP support]
** TRION-1600				(Voltage, SW Current)	[incl. RS-485 + DAQP support]
** TRION-1820-POWER-4			(Voltage, Current($))
** TRION-1810-HV-4			(Voltage)
** TRION3-1810M-POWER-4			(Voltage, Current($))
** TRION-1820-MULTI-4-D			(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE, CAN, MSI(%))
** TRION3-1820-MULTI-4-D		(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE, CAN, MSI(%))
** TRION3-1820-MULTI-8-L0B		(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE, CAN, MSI(%))
** TRION3-1850-MULTI-4-D		(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE, CAN, MSI(%))
** TRION3-1850-MULTI-8-L0B		(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE, CAN, MSI(%))

(%) MSI-BR-TH-x, MSI-BR-CH-x

($) Current module required for Current mode:
* SUB-dLV-1				(Current)
* SUB-CUR-20A-1				(Current)
* SUB-CUR-2A-1				(Current)
* SUB-CUR-02A-1				(Current)

***EPAD - all supported modules		(Supported Measurement mode):
** EPAD2-TH8-x				(Temperature, Voltage)
** EPAD2-TH8-UNIVERSAL			(Temperature, Voltage)
** EPAD2-V8				(Voltage)
** EPAD2-RTD8				(Temperature, Resistance)
** EPAD2-TH8-P				(Temperature(�), Voltage)
** EPAD2-LA8				(Current)
** EPAD -V8				(Voltage)
** EPAD -TH8-P				(Temperature(�), Voltage)

***PAD - all supported modules		(Supported Measurement mode):
** PAD-TH8-P				(Temperature(�), Voltage)
** PAD-V8-P				(Voltage)
** PAD-DO7				(DO)

(�) Connector block required for Temperature mode:
* PAD-CB8-x-P2				(Temperature)
* PAD-CB8-x-M				(Temperature)
* PAD-CB8-RTD-S3			(Temperature)


***ORION - all supported boards		(Supported Input type):
*  ORION DAQ Series (16 bit):
** ORION-0816-10M(%)			(Analog in, CAN)
** ORION-0816-5M (%)			(Analog in, CAN)
** ORION-0816-1000			(Analog in, CAN)
** ORION-0816-500			(Analog in, CAN)
** ORION-1616-10x			(Analog in, CAN)
** ORION-1616-100x			(Analog in, CAN)
** ORION-3216-10x			(Analog in, CAN)
*  ORION DSA Series (24 bit):
** ORION-1624-20x			(Analog in, CAN)
(%)data storing speed depends on hardware configuration
CAN only available on CAN enabled boards


***HSI/DAQP - all supported modules	(Supported Measurement mode):
** HSI-HV				(Voltage, SW Current)
** HSI-LV				(Voltage, SW Current)
** DAQP-HV				(Voltage, SW Current)
** DAQP-LV				(Voltage, SW Current)
** DAQP-STG				(Voltage, SW Current, Resistance, Bridge)
** HSI-STG				(Voltage, SW Current, Resistance, Bridge)
** DAQP-BRIDGE-A			(Voltage, SW Current, Bridge)
** DAQP-BRIDGE-B			(Voltage, SW Current, Bridge)
** DAQP-FREQ-A				(Frequency)
** DAQP-CFB2				(Bridge, Capacitance)
** DAQP-CHARGE-B			(Charge)
** DAQP-CHARGE-A			(Charge)
** DAQP-MULTI				(Voltage, SW Current, Resistance, Bridge, Temperature)
** DAQP-THERM				(Temperature)
** DAQP-ACC-A				(IEPE)
** DAQP-LA				(Current)
** DAQP-V				(Voltage, SW Current)
** DAQP-V-A				(Voltage, SW Current)
** DAQP-V-B				(Voltage, SW Current)
!All other modules not tested!

DI = Digital in
DO = Digital out


* Known Limitations, general:
** Statistics window may be adjusted automatically, to prevent drifting on rounded values
** Total number of DAQP/HSI/PAD/EPAD modules on each serial port is limited to 32 (scan range 0-31)
** Slow data is used as an export option and can only be viewed in recorder instruments within Oxygen
** dejaVIEW may experience degrading performance on long slow async data recordings
** DMD recovery may lead to non perfect results, depending on filesize, sampling rate, no. of channels and channel type
** Only a reduced number of triggers is shown in recorder instruments
** PCI bus overload may lead to Oxygen fault

* Known Limitations, Oxygen NET:
** Setup on Slaves containing statistic, filter or FFT channels, may not be loaded if "load last setup" option on Slaves is active
   (Recommendation: do not use "load last setup" on Oxygen NET Slaves)
** Absolute recording time between Master and Slave may not be synchronized - depending on sync settings
** Recording-trigger settings only valid on Master node, Slave recording-triggers are ignored (other triggers on Slave are still valid)
** PC Master with manual sync settings set to "internal" leads to free-running measurement (unsynchronized)
** on Master node the last sample of async channels may not be transferred
** claiming nodes takes a long time with active ADMA plugin
** auto-sync settings recommended (Master: Internal (no absolute time-sync), Slaves: TRION-SYNC-bus only), manual sync mode is only used under special circumstances
** TRIONet: dynamic connect/disconnect not supported

* Known Limitations with TRION:
FIXED ** TRION-Timing-V2/3 sometimes off by one second in case of 1Hz Samplerate (Solution: Set to 10Hz)

* Known Limitations with ORION:
** ORION-CNT not supported
** ORION-DI, DO not supported
** DAQ AD-boards: fixed AIRef set to Sense
** DSA AD-boards: only 5V AI range available (AIRef set to GND)
                  10V range for DAQP racks not supported (but is selectable in SW)


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
Release Notice DEWETRON Oxygen R3.4.1 x64

WARNING: Customer Release

* Components:
** DEWETRON Oxygen	R3.4.1	(3.4.1.49205)    (21d84ed0fd77)

* Files:
** DEWETRON_Oxygen_Setup_R3.4.1_x64.exe

* Bugfixes:
FIXED ** Oxygen NET connection loss during long-term tests


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
Release Notice DEWETRON Oxygen R3.4 x64

* Components:
** DEWETRON Oxygen	R3.4	(3.4.0.48732)    (63a468b76e5e)
** DEWETRON DMDReader	R3.3	(3.3.47204.0)    (2dcf0e3ffa70)

* Files:
** DEWETRON_Oxygen_Setup_R3.4_x64.exe
** DEWETRON_DMDReader_R3.3.zip

* Requirements:
** 3.x Software License required!
** OS: Windows 7 64bit, Windows 10 64bit
** CPU: Intel i5 3rd gen. or better
** RAM: 8 GB
** DAQ Hardware:
    * DEWETRON TRION (DEWETRON TRION Software R3.3.0)
    * DEWETRON ORION DAQ (ORION DAQ Driver V2.3.1.0)
    * DEWETRON ORION DSA (ORION DSA Driver V5.0.1.0)

* Installation procedure:
***TRION:
** Uninstall previous Oxygen version
** Uninstall any previous TRION version via system uninstall (control panel).
** Reboot system
** Install TRION applications
** Reboot system
** Start Dewe2Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
** Power-cycle TRION boards (Power down system, then restart)
** Install Oxygen
** Verify HW settings in system menu on first startup

* New Features Oxygen:
** SCPI External Data Logging (ELOG)
   gapless fetching of buffered data, ~50 S/s with 50 channels
** XY-Recorder Automatic Zoom
** EtherCAT Slave			 [optional, license required]
   Data Output via TRION-EtherCAT (Hilscher CIFX80-RE), ~400 S/s with 100 channels
** Data Stream Interface via TCP/IP	 [optional, license required]
   Full-speed data transfer, multiple streams, each one to multiple receivers,
   ~100 kS/s with 350 channels or ~2 MS/s with 12 channels on typical 1Gbit network
** Ethernet Receiver (UDP)		 [optional, license required]
   Generic receiver with XML configuration, listen-only
** Oxford Technical Solutions (OxTS) IMU [optional, license required]
   receive data from RT series IMUs, incl. HW-sync for mixed-signal operation
   (PPS negative edge w/ TRION-TIMING-V3 only)

* New Features Oxygen NET: 		
-

* HW Support:
***TRION - all supported modules	(Supported Measurement mode):
** TRION-1620-ACC-6-BNC			(Voltage, SW Current, IEPE, Simple CNT)
** TRION-1620-LV-6-BNC			(Voltage, SW Current)
** TRION-1620-LV-6-L1B			(Voltage, Current)
** TRION-1603-LV-6-BNC			(Voltage, SW Current)
** TRION-1603-LV-6-L1B			(Voltage, SW Current)
** TRION-1603-LV-6-D25			(Voltage, SW Current)
** TRION-2402-MULTI-4-D			(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE, CAN, MSI(%))
** TRION-2402-MULTI-8-L0B		(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE, CAN, MSI(%))
** TRION-2402-dSTG-6-L1B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-D			(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-L0B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-RJ			(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2400-dSTG-8-L0B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dACC-6-BNC		(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-dACC-8-SMB		(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-dACC-8-MD			(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-V-4-B			(Voltage, SW Current)
** TRION-2402-V-8-B			(Voltage, SW Current)
** TRION-CNT-6-L1B			(Simple CNT, Frequency)
** TRION-BASE				(IRIG B DC synchronization, PPS sync, Simple CNT, Frequency, DI, DO)
** TRION-TIMING				(IRIG A AC or DC, IRIG B AC or DC, PPS sync, GPS time sync + position, DI, DO)
** TRION-TIMING-V2			(IRIG A AC or DC, IRIG B AC or DC, PPS sync, GPS time sync + position, DI, DO)
** TRION-TIMING-V3			(PTP, IRIG A AC or DC, IRIG B AC or DC, PPS sync, GPS time sync + position, DI, DO) [TRION R3.3]
** TRION-VGPS-x				(PPS sync, GPS time sync + position, Simple CNT, Frequency, DI, DO)
** TRION-CAN-4				(CAN)
** TRION-CAN-2				(CAN)
** TRION-DI48				(DI)
** TRION-1802				(Voltage, SW Current)	[incl. RS-485 + DAQP support]
** TRION-1600				(Voltage, SW Current)	[incl. RS-485 + DAQP support]
** TRION-1820-POWER-4			(Voltage, Current($))
(%) MSI-BR-TH-x, MSI-BR-CH-x

($) Current module required for Current mode:
* SUB-dLV-1				(Current)
* SUB-CUR-20A-1				(Current)
* SUB-CUR-2A-1				(Current)
* SUB-CUR-02A-1				(Current)

***EPAD - all supported modules		(Supported Measurement mode):
** EPAD2-TH8-x				(Temperature, Voltage)
** EPAD2-TH8-UNIVERSAL			(Temperature, Voltage)
** EPAD2-V8				(Voltage)
** EPAD2-RTD8				(Temperature, Resistance)
** EPAD2-TH8-P				(Temperature(�), Voltage)
** EPAD2-LA8				(Current)
** EPAD -V8				(Voltage)
** EPAD -TH8-P				(Temperature(�), Voltage)

***PAD - all supported modules		(Supported Measurement mode):
** PAD-TH8-P				(Temperature(�), Voltage)
** PAD-V8-P				(Voltage)
** PAD-DO7				(DO)

(�) Connector block required for Temperature mode:
* PAD-CB8-x-P2				(Temperature)
* PAD-CB8-x-M				(Temperature)
* PAD-CB8-RTD-S3			(Temperature)


***ORION - all supported boards		(Supported Input type):
*  ORION DAQ Series (16 bit):
** ORION-0816-10M(%)			(Analog in, CAN)
** ORION-0816-5M (%)			(Analog in, CAN)
** ORION-0816-1000			(Analog in, CAN)
** ORION-0816-500			(Analog in, CAN)
** ORION-1616-10x			(Analog in, CAN)
** ORION-1616-100x			(Analog in, CAN)
** ORION-3216-10x			(Analog in, CAN)
*  ORION DSA Series (24 bit):
** ORION-1624-20x			(Analog in, CAN)
(%)data storing speed depends on hardware configuration
CAN only available on CAN enabled boards


***HSI/DAQP - all supported modules	(Supported Measurement mode):
** HSI-HV				(Voltage, SW Current)
** HSI-LV				(Voltage, SW Current)
** DAQP-HV				(Voltage, SW Current)
** DAQP-LV				(Voltage, SW Current)
** DAQP-STG				(Voltage, SW Current, Resistance, Bridge)
** HSI-STG				(Voltage, SW Current, Resistance, Bridge)
** DAQP-BRIDGE-A			(Voltage, SW Current, Bridge)
** DAQP-BRIDGE-B			(Voltage, SW Current, Bridge)
** DAQP-FREQ-A				(Frequency)
** DAQP-CFB2				(Bridge, Capacitance)
** DAQP-CHARGE-B			(Charge)
** DAQP-CHARGE-A			(Charge)
** DAQP-MULTI				(Voltage, SW Current, Resistance, Bridge, Temperature)
** DAQP-THERM				(Temperature)
** DAQP-ACC-A				(IEPE)
** DAQP-LA				(Current)
** DAQP-V				(Voltage, SW Current)
** DAQP-V-A				(Voltage, SW Current)
** DAQP-V-B				(Voltage, SW Current)
!All other modules not tested!

DI = Digital in
DO = Digital out

* Known Limitations, general:
** Statistics window may be adjusted automatically, to prevent drifting on rounded values
** Total number of DAQP/HSI/PAD/EPAD modules on each serial port is limited to 32 (scan range 0-31)
** Slow data is used as an export option and can only be viewed in recorder instruments within Oxygen
** dejaVIEW may experience degrading performance on long slow async data recordings
** DMD recovery may lead to non perfect results, depending on filesize, sampling rate, no. of channels and channel type
** Only a reduced number of triggers is shown in recorder instruments
** PCI bus overload may lead to Oxygen fault

* Known Limitations, Oxygen NET:
** Recording-trigger settings only valid on Master node, Slave recording-triggers are ignored (other triggers on Slave are still valid)
** PC Master with manual sync settings set to "internal" leads to free-running measurement (unsynchronized)
** on Master node the last sample of async channels may not be transferred
** claiming nodes takes a long time with active ADMA plugin
** auto-sync settings recommended (Master: Internal (no absolute time-sync), Slaves: TRION-SYNC-bus only), manual sync mode is only used under special circumstances
** TRIONet: dynamic connect/disconnect not supported

* Known Limitations with TRION:
** TRION-Timing-V2/3 sometimes off by one second in case of 1Hz Samplerate (Solution: Set to 10Hz)

* Known Limitations with ORION:
** ORION-CNT not supported
** ORION-DI, DO not supported
** DAQ AD-boards: fixed AIRef set to Sense
** DSA AD-boards: only 5V AI range available (AIRef set to GND)
                  10V range for DAQP racks not supported (but is selectable in SW)


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
Release Notice DEWETRON Oxygen R3.3.3 x64

WARNING: Customer Release

* Components:
** DEWETRON Oxygen	R3.3.3	(3.3.3.48226)    (f14cb1bfa250)

* Files:
** DEWETRON_Oxygen_Setup_R3.3.3_x64.exe

* New Features Oxygen:
** EtherCAT Data Output via TRION-EtherCAT (Hilscher CIFX80-RE)


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
Release Notice DEWETRON Oxygen R3.3.2 x64

* Components:
** DEWETRON Oxygen	R3.3.2	(3.3.2.47475)    (fa53deceb1cb)
** DEWETRON DMDReader	R3.3	(3.3.47204.0)    (2dcf0e3ffa70)

* Files:
** DEWETRON_Oxygen_Setup_R3.3.2_x64.exe
** DEWETRON_DMDReader_R3.3.zip

* Bugfixes:
FIXED ** ORION+DAQP HW issues (multiple boards, DAQP scan)
FIXED ** Network issues in evaluation mode (Oxygen NET is now OFF by default)


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
Release Notice DEWETRON Oxygen R3.3.1 x64

* Components:
** DEWETRON Oxygen	R3.3.1	(3.3.1.47236)    (fcb92cdca262)
** DEWETRON DMDReader	R3.3	(3.3.47204.0)    (2dcf0e3ffa70)

* Files:
** DEWETRON_Oxygen_Setup_R3.3.1_x64.exe
** DEWETRON_DMDReader_R3.3.zip

* Bugfixes:
FIXED ** ORION HW support


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
Release Notice DEWETRON Oxygen R3.3 x64

* Components:
** DEWETRON Oxygen	R3.3	(3.3.0.47209)    (414787e146f6)
** DEWETRON DMDReader	R3.3	(3.3.47204.0)    (2dcf0e3ffa70)

* Files:
** DEWETRON_Oxygen_Setup_R3.3_x64.exe
** DEWETRON_DMDReader_R3.3.zip

* Requirements:
** 3.x Software License required! (120 day Evaluation time-limit is removed)
** OS: Windows 7 64bit, Windows 10 64bit
** CPU: Intel i5 3rd gen. or better
** RAM: 8 GB
** DAQ Hardware:
    * DEWETRON TRION (DEWETRON TRION Software R3.1.0)
    * DEWETRON ORION DAQ (ORION DAQ Driver V2.3.1.0)
    * DEWETRON ORION DSA (ORION DSA Driver V5.0.1.0)

* Installation procedure:
***TRION:
** Uninstall previous Oxygen version
** Uninstall any previous TRION version via system uninstall (control panel).
** Reboot system
** Install TRION applications
** Reboot system
** Start Dewe2Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
** Power-cycle TRION boards (Power down system, then restart)
** Install Oxygen
** Verify HW settings in system menu on first startup

* New Features Oxygen:
** FFT Math channels
** Spectrogram display instrument
** Snapshot trigger (one value at trigger)
** Excel data export
** Math, Strain-gage Rosette calculation

* New Features Oxygen NET: 	[optional, license required]
** Data transfer
** Remote channel setup
** Triggered recording
** PC Master sync mode

* Plugin Support:
** XCP Plugin V1.3

* HW Support:
***TRION - all supported modules	(Supported Measurement mode):
** TRION-1620-ACC-6-BNC			(Voltage, SW Current, IEPE, Simple CNT)
** TRION-1620-LV-6-BNC			(Voltage, SW Current)
** TRION-1620-LV-6-L1B			(Voltage, Current)
** TRION-1603-LV-6-BNC			(Voltage, SW Current)
** TRION-1603-LV-6-L1B			(Voltage, SW Current)
** TRION-1603-LV-6-D25			(Voltage, SW Current)
** TRION-2402-MULTI-4-D			(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE, CAN, MSI(%))
** TRION-2402-MULTI-8-L0B		(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE, CAN, MSI(%))
** TRION-2402-dSTG-6-L1B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-D			(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-L0B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-RJ			(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2400-dSTG-8-L0B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dACC-6-BNC		(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-dACC-8-SMB		(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-dACC-8-MD			(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-V-4-B			(Voltage, SW Current)
** TRION-2402-V-8-B			(Voltage, SW Current)
** TRION-CNT-6-L1B			(Simple CNT, Frequency)
** TRION-BASE				(IRIG B DC synchronization, PPS sync, Simple CNT, Frequency, DI, DO)
** TRION-TIMING				(IRIG A AC or DC, IRIG B AC or DC, PPS sync, GPS time sync + position, DI, DO)
** TRION-TIMING-V2			(IRIG A AC or DC, IRIG B AC or DC, PPS sync, GPS time sync + position, DI, DO)
** TRION-TIMING-V3			(PTP, IRIG A AC or DC, IRIG B AC or DC, PPS sync, GPS time sync + position, DI, DO) [TRION R3.3]
** TRION-VGPS-x				(PPS sync, GPS time sync + position, Simple CNT, Frequency, DI, DO)
** TRION-CAN-4				(CAN)
** TRION-CAN-2				(CAN)
** TRION-DI48				(DI)
** TRION-1802				(Voltage, SW Current)	[incl. RS-485 + DAQP support]
** TRION-1600				(Voltage, SW Current)	[incl. RS-485 + DAQP support]
** TRION-1820-POWER-4			(Voltage, Current($))
(%) MSI-BR-TH-x, MSI-BR-CH-x

($) Current module required for Current mode:
* SUB-dLV-1				(Current)
* SUB-CUR-20A-1				(Current)
* SUB-CUR-2A-1				(Current)
* SUB-CUR-02A-1				(Current)

***EPAD - all supported modules		(Supported Measurement mode):
** EPAD2-TH8-x				(Temperature, Voltage)
** EPAD2-TH8-UNIVERSAL			(Temperature, Voltage)
** EPAD2-V8				(Voltage)
** EPAD2-RTD8				(Temperature, Resistance)
** EPAD2-TH8-P				(Temperature(�), Voltage)
** EPAD2-LA8				(Current)
** EPAD -V8				(Voltage)
** EPAD -TH8-P				(Temperature(�), Voltage)

***PAD - all supported modules		(Supported Measurement mode):
** PAD-TH8-P				(Temperature(�), Voltage)
** PAD-V8-P				(Voltage)
** PAD-DO7				(DO)

(�) Connector block required for Temperature mode:
* PAD-CB8-x-P2				(Temperature)
* PAD-CB8-x-M				(Temperature)
* PAD-CB8-RTD-S3			(Temperature)


***ORION - all supported boards		(Supported Input type):
*  ORION DAQ Series (16 bit):
** ORION-0816-10M(%)			(Analog in, CAN)
** ORION-0816-5M (%)			(Analog in, CAN)
** ORION-0816-1000			(Analog in, CAN)
** ORION-0816-500			(Analog in, CAN)
** ORION-1616-10x			(Analog in, CAN)
** ORION-1616-100x			(Analog in, CAN)
** ORION-3216-10x			(Analog in, CAN)
*  ORION DSA Series (24 bit):
** ORION-1624-20x			(Analog in, CAN)
(%)data storing speed depends on hardware configuration
CAN only available on CAN enabled boards


***HSI/DAQP - all supported modules	(Supported Measurement mode):
** HSI-HV				(Voltage, SW Current)
** HSI-LV				(Voltage, SW Current)
** DAQP-HV				(Voltage, SW Current)
** DAQP-LV				(Voltage, SW Current)
** DAQP-STG				(Voltage, SW Current, Resistance, Bridge)
** HSI-STG				(Voltage, SW Current, Resistance, Bridge)
** DAQP-BRIDGE-A			(Voltage, SW Current, Bridge)
** DAQP-BRIDGE-B			(Voltage, SW Current, Bridge)
** DAQP-FREQ-A				(Frequency)
** DAQP-CFB2				(Bridge, Capacitance)
** DAQP-CHARGE-B			(Charge)
** DAQP-CHARGE-A			(Charge)
** DAQP-MULTI				(Voltage, SW Current, Resistance, Bridge, Temperature)
** DAQP-THERM				(Temperature)
** DAQP-ACC-A				(IEPE)
** DAQP-LA				(Current)
** DAQP-V				(Voltage, SW Current)
** DAQP-V-A				(Voltage, SW Current)
** DAQP-V-B				(Voltage, SW Current)
!All other modules not tested!

DI = Digital in
DO = Digital out

* Known Limitations, general:
** Statistics window may be adjusted automatically, to prevent drifting on rounded values
** Total number of DAQP/HSI/PAD/EPAD modules on each serial port is limited to 32 (scan range 0-31)
** Slow data is used as an export option and can only be viewed in recorder instruments within Oxygen
** dejaVIEW may experience degrading performance on long slow async data recordings
** DMD recovery may lead to non perfect results, depending on filesize, sampling rate, no. of channels and channel type
** Only a reduced number of triggers is shown in recorder instruments
** PCI bus overload may lead to Oxygen fault

* Known Limitations, Oxygen NET:
** Recording-trigger settings only valid on Master node, Slave recording-triggers are ignored (other triggers on Slave are still valid)
** PC Master with manual sync settings set to "internal" leads to free-running measurement (unsynchronized)
** on Master node the last sample of async channels may not be transferred
** claiming nodes takes a long time with active ADMA plugin
** auto-sync settings recommended (Master: Internal (no absolute time-sync), Slaves: TRION-SYNC-bus only), manual sync mode is only used under special circumstances
FIXED ** Triggered measurement not possible
FIXED ** differing multi-samplerates between Master and Slaves may cause phase-offsets by 1 slow sample
** TRIONet: dynamic connect/disconnect not supported
FIXED ** Occasionally, claiming a remote node may not work at first try

* Known Limitations, Birds Eye Plugin:
FIXED ** when setting up moving objects (assigned position channel), all calculations are NaN as long as no actual position data is received
FIXED ** when 1 of multiple position sources has no data for n seconds, all live calculations are not updated for those n seconds (data file shows all available calculated values)

* Known Limitations with TRION:
-

* Known Limitations with ORION:
** ORION-CNT not supported
** ORION-DI, DO not supported
** DAQ AD-boards: fixed AIRef set to Sense
** DSA AD-boards: only 5V AI range available (AIRef set to GND)
                  10V range for DAQP racks not supported (but is selectable in SW)


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
Release Notice DEWETRON Oxygen R3.2 x64

* Components:
** DEWETRON Oxygen	R3.2	(3.2.0.45031)    (79f3d089de0f)
** DEWETRON DMDReader	R3.2	(3.2.44956.0)    (98a220fd09e1)

* Files:
** DEWETRON_Oxygen_Setup_R3.2_x64.exe
** DEWETRON_DMDReader_R3.2.zip

* Requirements:
** 3.x Software License required! (120 day Evaluation time-limit is removed)
** OS: Windows 7 64bit, Windows 10 64bit
** CPU: Intel i5 3rd gen. or better
** RAM: 8 GB
** DAQ Hardware:
    * DEWETRON TRION (DEWETRON TRION Software R3.1.0)
    * DEWETRON ORION DAQ (ORION DAQ Driver V2.1.0.0)
    * DEWETRON ORION DSA (ORION DSA Driver V4.1.0.0)

* Installation procedure:
***TRION:
** Uninstall previous Oxygen version
** Uninstall any previous TRION version via system uninstall (control panel).
** Reboot system
** Install TRION applications
** Reboot system
** Start Dewe2Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
** Power-cycle TRION boards (Power down system, then restart)
** Install Oxygen
** Verify HW settings in system menu on first startup

* New Features Oxygen:
***ADAS-Package:		[optional, license required]
** IMU - ADMA Plugin		
   up to 3 synchronized ADMA standard + delta streams via Ethernet
** BirdsEye Plugin
   distance calculation between up to n moving objects (POIs or contour), cones and tracks

* New Features Oxygen NET: 	[optional, license required]
-

* Plugin Support:
** XCP Plugin V1.1

* HW Support:
***TRION - all supported modules	(Supported Measurement mode):
** TRION-1620-ACC-6-BNC			(Voltage, SW Current, IEPE, Simple CNT)
** TRION-1620-LV-6-BNC			(Voltage, SW Current)
** TRION-1620-LV-6-L1B			(Voltage, Current)
** TRION-1603-LV-6-BNC			(Voltage, SW Current)
** TRION-1603-LV-6-L1B			(Voltage, SW Current)
** TRION-1603-LV-6-D25			(Voltage, SW Current)
** TRION-2402-MULTI-4-D			(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE, CAN, MSI(%))
** TRION-2402-MULTI-8-L0B		(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE, CAN, MSI(%))
** TRION-2402-dSTG-6-L1B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-D			(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-L0B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-RJ			(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2400-dSTG-8-L0B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dACC-6-BNC		(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-dACC-8-SMB		(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-dACC-8-MD			(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-V-4-B			(Voltage, SW Current)
** TRION-2402-V-8-B			(Voltage, SW Current)
** TRION-CNT-6-L1B			(Simple CNT, Frequency)
** TRION-BASE				(IRIG B DC synchronization, PPS sync, Simple CNT, Frequency, DI, DO)
** TRION-TIMING				(IRIG A AC or DC, IRIG B AC or DC, PPS sync, GPS time sync + position, DI, DO)
** TRION-TIMING-V2			(IRIG A AC or DC, IRIG B AC or DC, PPS sync, GPS time sync + position, DI, DO)
** TRION-VGPS-x				(PPS sync, GPS time sync + position, Simple CNT, Frequency, DI, DO)
** TRION-CAN-4				(CAN)
** TRION-CAN-2				(CAN)
** TRION-DI48				(DI)
** TRION-1802				(Voltage, SW Current)	[incl. RS-485 + DAQP support]
** TRION-1600				(Voltage, SW Current)	[incl. RS-485 + DAQP support]
** TRION-1820-POWER-4			(Voltage, Current($))
(%) MSI-BR-TH-x, MSI-BR-CH-x

($) Current module required for Current mode:
* SUB-dLV-1				(Current)
* SUB-CUR-20A-1				(Current)
* SUB-CUR-2A-1				(Current)
* SUB-CUR-02A-1				(Current)

***EPAD - all supported modules		(Supported Measurement mode):
** EPAD2-TH8-x				(Temperature, Voltage)
** EPAD2-TH8-UNIVERSAL			(Temperature, Voltage)
** EPAD2-V8				(Voltage)
** EPAD2-RTD8				(Temperature, Resistance)
** EPAD2-TH8-P				(Temperature(�), Voltage)
** EPAD2-LA8				(Current)
** EPAD -V8				(Voltage)
** EPAD -TH8-P				(Temperature(�), Voltage)

***PAD - all supported modules		(Supported Measurement mode):
** PAD-TH8-P				(Temperature(�), Voltage)
** PAD-V8-P				(Voltage)
** PAD-DO7				(DO)

(�) Connector block required for Temperature mode:
* PAD-CB8-x-P2				(Temperature)
* PAD-CB8-x-M				(Temperature)
* PAD-CB8-RTD-S3			(Temperature)


***ORION - all supported boards		(Supported Input type):
*  ORION DAQ Series (16 bit):
** ORION-0816-10M(%)			(Analog in, CAN)
** ORION-0816-5M (%)			(Analog in, CAN)
** ORION-0816-1000			(Analog in, CAN)
** ORION-0816-500			(Analog in, CAN)
** ORION-1616-10x			(Analog in, CAN)
** ORION-1616-100x			(Analog in, CAN)
** ORION-3216-10x			(Analog in, CAN)
*  ORION DSA Series (24 bit):
** ORION-1624-20x			(Analog in, CAN)
(%)data storing speed depends on hardware configuration
CAN only available on CAN enabled boards


***HSI/DAQP - all supported modules	(Supported Measurement mode):
** HSI-HV				(Voltage, SW Current)
** HSI-LV				(Voltage, SW Current)
** DAQP-HV				(Voltage, SW Current)
** DAQP-LV				(Voltage, SW Current)
** DAQP-STG				(Voltage, SW Current, Resistance, Bridge)
** HSI-STG				(Voltage, SW Current, Resistance, Bridge)
** DAQP-BRIDGE-A			(Voltage, SW Current, Bridge)
** DAQP-BRIDGE-B			(Voltage, SW Current, Bridge)
** DAQP-FREQ-A				(Frequency)
** DAQP-CFB2				(Bridge, Capacitance)
** DAQP-CHARGE-B			(Charge)
** DAQP-CHARGE-A			(Charge)
** DAQP-MULTI				(Voltage, SW Current, Resistance, Bridge, Temperature)
** DAQP-THERM				(Temperature)
** DAQP-ACC-A				(IEPE)
** DAQP-LA				(Current)
** DAQP-V				(Voltage, SW Current)
** DAQP-V-A				(Voltage, SW Current)
** DAQP-V-B				(Voltage, SW Current)
!All other modules not tested!

DI = Digital in
DO = Digital out

* Known Limitations, general:
** Statistics window may be adjusted automatically, to prevent drifting on rounded values
FIXED** Offline statistics may have possible shift of 1 sample under certain conditions
** Total number of DAQP/HSI/PAD/EPAD modules on each serial port is limited to 32 (scan range 0-31)
** Slow data is used as an export option and can only be viewed in recorder instruments within Oxygen
** dejaVIEW may experience degrading performance on long slow async data recordings
** DMD recovery may lead to non perfect results, depending on filesize, sampling rate, no. of channels and channel type
** Only a reduced number of triggers is shown in recorder instruments
** PCI bus overload may lead to Oxygen fault

* Known Limitations, Oxygen NET:
** claiming nodes takes a long time with active ADMA plugin
** Only auto-sync settings allowed (Master: Internal (no absolute time-sync), Slaves: TRION-SYNC-bus only) 
** Triggered measurement not possible
** differing multi-samplerates between Master and Slaves may cause phase-offsets by 1 slow sample
** TRIONet: dynamic connect/disconnect not supported
** Occasionally, claiming a remote node may not work at first try

* Known Limitations, Birds Eye Plugin:
** when setting up moving objects (assigned position channel), all calculations are NaN as long as no actual position data is received
** when 1 of multiple position sources has no data for n seconds, all live calculations are not updated for those n seconds (data file shows all available calculated values)

* Known Limitations with TRION:
-

* Known Limitations with ORION:
** ORION-CNT not supported
** ORION-DI, DO not supported
** DAQ AD-boards: fixed AIRef set to Sense
** DSA AD-boards: only 5V AI range available (AIRef set to GND)
                  10V range for DAQP racks not supported (but is selectable in SW)


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
Release Notice DEWETRON Oxygen R3.1 x64

* Components:
** DEWETRON Oxygen	R3.1	(3.1.0.44194)    (6055d07b223c)
** DEWETRON DMDReader	R3.0	(3.0.42798.0)    (c170aa40bb9f)

* Files:
** DEWETRON_Oxygen_Setup_R3.1_x64.exe
** DEWETRON_DMDReader_R3.0.zip

* Requirements:
** 3.x Software License required! (120 day Evaluation time-limit is removed)
** OS: Windows 7 64bit, Windows 10 64bit
** CPU: Intel i5 3rd gen. or better
** RAM: 8 GB
** DAQ Hardware:
    * DEWETRON TRION (DEWETRON TRION Software R3.1.0)
    * DEWETRON ORION DAQ (ORION DAQ Driver V2.1.0.0)
    * DEWETRON ORION DSA (ORION DSA Driver V4.1.0.0)

* Installation procedure:
***TRION:
** Uninstall previous Oxygen version
** Uninstall any previous TRION version via system uninstall (control panel).
** Reboot system
** Install TRION applications
** Reboot system
** Start Dewe2Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
** Power-cycle TRION boards (Power down system, then restart)
** Install Oxygen
** Verify HW settings in system menu on first startup

* New Features Oxygen:
** TRION-VGPS-V3 HW support
** GPS quality instrument
** Bitmap map overlay for GPS position instrument
** Math Offline: calculate formula channels in replay mode
** Power advanced: Flicker dc, dmax, td channels according to IEC61000-4-15 available

* New Features Oxygen NET: [optional, license required]
-

* HW Support:
***TRION - all supported modules	(Supported Measurement mode):
** TRION-1620-ACC-6-BNC			(Voltage, SW Current, IEPE, Simple CNT)
** TRION-1620-LV-6-BNC			(Voltage, SW Current)
** TRION-1620-LV-6-L1B			(Voltage, Current)
** TRION-1603-LV-6-BNC			(Voltage, SW Current)
** TRION-1603-LV-6-L1B			(Voltage, SW Current)
** TRION-1603-LV-6-D25			(Voltage, SW Current)
** TRION-2402-MULTI-4-D			(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE, CAN, MSI(%))
** TRION-2402-MULTI-8-L0B		(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE, CAN, MSI(%))
** TRION-2402-dSTG-6-L1B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-D			(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-L0B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-RJ			(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2400-dSTG-8-L0B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dACC-6-BNC		(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-dACC-8-SMB		(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-dACC-8-MD			(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-V-4-B			(Voltage, SW Current)
** TRION-2402-V-8-B			(Voltage, SW Current)
** TRION-CNT-6-L1B			(Simple CNT, Frequency)
** TRION-BASE				(IRIG B DC synchronization, PPS sync, Simple CNT, Frequency, DI, DO)
** TRION-TIMING				(IRIG A AC or DC, IRIG B AC or DC, PPS sync, GPS time sync + position, DI, DO)
** TRION-TIMING-V2			(IRIG A AC or DC, IRIG B AC or DC, PPS sync, GPS time sync + position, DI, DO)
** TRION-VGPS-x				(PPS sync, GPS time sync + position, Simple CNT, Frequency, DI, DO)
** TRION-CAN-4				(CAN)
** TRION-CAN-2				(CAN)
** TRION-DI48				(DI)
** TRION-1802				(Voltage, SW Current)	[incl. RS-485 + DAQP support]
** TRION-1600				(Voltage, SW Current)	[incl. RS-485 + DAQP support]
** TRION-1820-POWER-4			(Voltage, Current($))
(%) MSI-BR-TH-x, MSI-BR-CH-x

($) Current module required for Current mode:
* SUB-dLV-1				(Current)
* SUB-CUR-20A-1				(Current)


***EPAD - all supported modules		(Supported Measurement mode):
** EPAD2-TH8-x				(Temperature, Voltage)
** EPAD2-TH8-UNIVERSAL			(Temperature, Voltage)
** EPAD2-V8				(Voltage)
** EPAD2-RTD8				(Temperature, Resistance)
** EPAD2-TH8-P				(Temperature(�), Voltage)
** EPAD2-LA8				(Current)
** EPAD -V8				(Voltage)
** EPAD -TH8-P				(Temperature(�), Voltage)

***PAD - all supported modules		(Supported Measurement mode):
** PAD-TH8-P				(Temperature(�), Voltage)
** PAD-V8-P				(Voltage)
** PAD-DO7				(DO)

(�) Connector block required for Temperature mode:
* PAD-CB8-x-P2				(Temperature)
* PAD-CB8-x-M				(Temperature)
* PAD-CB8-RTD-S3			(Temperature)


***ORION - all supported boards		(Supported Input type):
*  ORION DAQ Series (16 bit):
** ORION-0816-10M(%)			(Analog in, CAN)
** ORION-0816-5M (%)			(Analog in, CAN)
** ORION-0816-1000			(Analog in, CAN)
** ORION-0816-500			(Analog in, CAN)
** ORION-1616-10x			(Analog in, CAN)
** ORION-1616-100x			(Analog in, CAN)
** ORION-3216-10x			(Analog in, CAN)
*  ORION DSA Series (24 bit):
** ORION-1624-20x			(Analog in, CAN)
(%)data storing speed depends on hardware configuration
CAN only available on CAN enabled boards


***HSI/DAQP - all supported modules	(Supported Measurement mode):
** HSI-HV				(Voltage, SW Current)
** HSI-LV				(Voltage, SW Current)
** DAQP-HV				(Voltage, SW Current)
** DAQP-LV				(Voltage, SW Current)
** DAQP-STG				(Voltage, SW Current, Resistance, Bridge)
** HSI-STG				(Voltage, SW Current, Resistance, Bridge)
** DAQP-BRIDGE-A			(Voltage, SW Current, Bridge)
** DAQP-BRIDGE-B			(Voltage, SW Current, Bridge)
** DAQP-FREQ-A				(Frequency)
** DAQP-CFB2				(Bridge, Capacitance)
** DAQP-CHARGE-B			(Charge)
** DAQP-CHARGE-A			(Charge)
** DAQP-MULTI				(Voltage, SW Current, Resistance, Bridge, Temperature)
** DAQP-THERM				(Temperature)
** DAQP-ACC-A				(IEPE)
** DAQP-LA				(Current)
** DAQP-V				(Voltage, SW Current)
** DAQP-V-A				(Voltage, SW Current)
** DAQP-V-B				(Voltage, SW Current)
!All other modules not tested!

DI = Digital in
DO = Digital out

* Known Limitations, general:
** Statistics window may be adjusted automatically, to prevent drifting on rounded values
** Offline statistics may have possible shift of 1 sample under certain conditions
** Total number of DAQP/HSI/PAD/EPAD modules on each serial port is limited to 32 (scan range 0-31)
** Slow data is used as an export option and can only be viewed in recorder instruments within Oxygen
** dejaVIEW may experience degrading performance on long slow async data recordings
** DMD recovery may lead to non perfect results, depending on filesize, sampling rate, no. of channels and channel type
** Only a reduced number of triggers is shown in recorder instruments
** PCI bus overload may lead to Oxygen fault

* Known Limitations, Oxygen NET:
** Only auto-sync settings allowed (Master: Internal (no absolute time-sync), Slaves: TRION-SYNC-bus only) 
** Triggered measurement not possible
** differing multi-samplerates between Master and Slaves may cause phase-offsets by 1 slow sample
** TRIONet: dynamic connect/disconnect not supported
** Occasionally, claiming a remote node may not work at first try

* Known Limitations with TRION:
-

* Known Limitations with ORION:
** ORION-CNT not supported
** ORION-DI, DO not supported
** DAQ AD-boards: fixed AIRef set to Sense
** DSA AD-boards: only 5V AI range available (AIRef set to GND)
                  10V range for DAQP racks not supported (but is selectable in SW)


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
Release Notice DEWETRON Oxygen R3.0 x64

* Components:
** DEWETRON Oxygen	R3.0	(3.0.0.42827) (e99e0f420b56)
** DEWETRON DMDReader	R3.0	(3.0.42798.0) (c170aa40bb9f)

* Files:
** DEWETRON_Oxygen_Setup_R3.0_x64.exe
** DEWETRON_DMDReader_R3.0.zip

* Requirements:
** 3.x Software License required!
** OS: Windows 7 64bit, Windows 10 64bit
** CPU: Intel i5 3rd gen. or better
** RAM: 8 GB
** DAQ Hardware:
    * DEWETRON TRION (DEWETRON TRION Software R3.0)
    * DEWETRON ORION DAQ (ORION DAQ Driver V2.1.0.0)
    * DEWETRON ORION DSA (ORION DSA Driver V4.1.0.0)

* Installation procedure:
***TRION:
** Uninstall previous Oxygen version
** Uninstall any previous TRION version via system uninstall (control panel).
** Reboot system
** Install TRION applications
** Reboot system
** Start Dewe2Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
** Power-cycle TRION boards (Power down system, then restart)
** Install Oxygen
** Verify HW settings in system menu on first startup

* New Features Oxygen:
** Multi-file: load multiple split data files at once
** Multi-file: split DMD files by number of recording events
** TRION-VGPS, TRION-TIMING: support for GPS position and quality data
** GPS position instrument, incl. OSM map overlay (online)
** Math Offline: calculate filter and statistics channels in replay mode
** Export MATLAB data file
** XCP data transfer (polling + daqlist) [optional, license required]

* New Features Oxygen NET: [optional, license required]
** TRION only!
** Synchronized measurement with mutliple DEWE2 devices via Ethernet, sync via TRION-SYNC-bus
Data files are only stored locally!
Slave setup must be done locally!

* HW Support:
***TRION - all supported modules	(Supported Measurement mode):
** TRION-1620-ACC-6-BNC			(Voltage, SW Current, IEPE, Simple CNT)
** TRION-1620-LV-6-BNC			(Voltage, SW Current)
** TRION-1620-LV-6-L1B			(Voltage, Current)
** TRION-1603-LV-6-BNC			(Voltage, SW Current)
** TRION-1603-LV-6-L1B			(Voltage, SW Current)
** TRION-1603-LV-6-D25			(Voltage, SW Current)
** TRION-2402-MULTI-4-D			(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE, CAN, MSI(%))
** TRION-2402-MULTI-8-L0B		(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE, CAN, MSI(%))
** TRION-2402-dSTG-6-L1B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-D			(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-L0B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-RJ			(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2400-dSTG-8-L0B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dACC-6-BNC		(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-dACC-8-SMB		(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-dACC-8-MD			(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-V-4-B			(Voltage, SW Current)
** TRION-2402-V-8-B			(Voltage, SW Current)
** TRION-CNT-6-L1B			(Simple CNT, Frequency)
** TRION-BASE				(IRIG B DC synchronization, PPS sync, Simple CNT, Frequency, DI, DO)
** TRION-TIMING				(IRIG A AC or DC, IRIG B AC or DC, PPS sync, GPS time sync + position, DI, DO)
** TRION-TIMING-V2			(IRIG A AC or DC, IRIG B AC or DC, PPS sync, GPS time sync + position, DI, DO)
** TRION-VGPS-x				(GPS time sync + position, Simple CNT, Frequency, DI, DO)
** TRION-CAN-4				(CAN)
** TRION-CAN-2				(CAN)
** TRION-DI48				(DI)
** TRION-1802				(Voltage, SW Current)	[incl. RS-485 + DAQP support]
** TRION-1600				(Voltage, SW Current)	[incl. RS-485 + DAQP support]
** TRION-1820-POWER-4			(Voltage, Current($))
(%) MSI-BR-TH-x, MSI-BR-CH-x

($) Current module required for Current mode:
* SUB-dLV-1				(Current)
* SUB-CUR-20A-1				(Current)


***EPAD - all supported modules		(Supported Measurement mode):
** EPAD2-TH8-x				(Temperature, Voltage)
** EPAD2-TH8-UNIVERSAL			(Temperature, Voltage)
** EPAD2-V8				(Voltage)
** EPAD2-RTD8				(Temperature, Resistance)
** EPAD2-TH8-P				(Temperature(�), Voltage)
** EPAD2-LA8				(Current)
** EPAD -V8				(Voltage)
** EPAD -TH8-P				(Temperature(�), Voltage)

***PAD - all supported modules		(Supported Measurement mode):
** PAD-TH8-P				(Temperature(�), Voltage)
** PAD-V8-P				(Voltage)
** PAD-DO7				(DO)

(�) Connector block required for Temperature mode:
* PAD-CB8-x-P2				(Temperature)
* PAD-CB8-x-M				(Temperature)
* PAD-CB8-RTD-S3			(Temperature)


***ORION - all supported boards		(Supported Input type):
*  ORION DAQ Series (16 bit):
** ORION-0816-10M(%)			(Analog in, CAN)
** ORION-0816-5M (%)			(Analog in, CAN)
** ORION-0816-1000			(Analog in, CAN)
** ORION-0816-500			(Analog in, CAN)
** ORION-1616-10x			(Analog in, CAN)
** ORION-1616-100x			(Analog in, CAN)
** ORION-3216-10x			(Analog in, CAN)
*  ORION DSA Series (24 bit):
** ORION-1624-20x			(Analog in, CAN)
(%)data storing speed depends on hardware configuration
CAN only available on CAN enabled boards


***HSI/DAQP - all supported modules	(Supported Measurement mode):
** HSI-HV				(Voltage, SW Current)
** HSI-LV				(Voltage, SW Current)
** DAQP-HV				(Voltage, SW Current)
** DAQP-LV				(Voltage, SW Current)
** DAQP-STG				(Voltage, SW Current, Resistance, Bridge)
** HSI-STG				(Voltage, SW Current, Resistance, Bridge)
** DAQP-BRIDGE-A			(Voltage, SW Current, Bridge)
** DAQP-BRIDGE-B			(Voltage, SW Current, Bridge)
** DAQP-FREQ-A				(Frequency)
** DAQP-CFB2				(Bridge, Capacitance)
** DAQP-CHARGE-B			(Charge)
** DAQP-CHARGE-A			(Charge)
** DAQP-MULTI				(Voltage, SW Current, Resistance, Bridge, Temperature)
** DAQP-THERM				(Temperature)
** DAQP-ACC-A				(IEPE)
** DAQP-LA				(Current)
** DAQP-V				(Voltage, SW Current)
** DAQP-V-A				(Voltage, SW Current)
** DAQP-V-B				(Voltage, SW Current)
!All other modules not tested!

DI = Digital in
DO = Digital out

* Known Limitations, general:
** Statistics window may be adjusted automatically, to prevent drifting on rounded values
** Offline statistics may have possible shift of 1 sample under certain conditions
** Total number of DAQP/HSI/PAD/EPAD modules on each serial port is limited to 32 (scan range 0-31)
** Slow data is used as an export option and can only be viewed in recorder instruments within Oxygen
** dejaVIEW may experience degrading performance on long slow async data recordings
** DMD recovery may lead to non perfect results, depending on filesize, sampling rate, no. of channels and channel type
** Only a reduced number of triggers is shown in recorder instruments
** PCI bus overload may lead to Oxygen fault
FIXED ** Power module: possible gap of a few milliseconds in live-data stream on pause-resume (recorded data is gapless)

* Known Limitations, Oxygen NET:
** Only auto-sync settings allowed (Master: Internal (no absolute time-sync), Slaves: TRION-SYNC-bus only) 
** Triggered measurement not possible
** differing multi-samplerates between Master and Slaves may cause phase-offsets by 1 slow sample
** TRIONet: dynamic connect/disconnect not supported
** Occasionally, claiming a remote node may not work at first try

* Known Limitations with TRION:
-

* Known Limitations with ORION:
** ORION-CNT not supported
** ORION-DI, DO not supported
** DAQ AD-boards: fixed AIRef set to Sense
** DSA AD-boards: only 5V AI range available (AIRef set to GND)
                  10V range for DAQP racks not supported (but is selectable in SW)


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
Release Notice DEWETRON Oxygen R2.6 x64

* Components:
** DEWETRON Oxygen	R2.6	(2.6.0.39283) (5746f2341677)
** DEWETRON DMDReader	R2.6	(2.6.40075.0) (36438e5d6caa)

* Files:
** DEWETRON_Oxygen_Setup_R2.6_x64.exe
** DEWETRON_DMDReader_R2.6.zip

* Requirements:
** OS: Windows 7 64bit, Windows 10 64bit
** CPU: Intel i5 3rd gen. or better
** RAM: 8 GB
** DAQ Hardware:
    * DEWETRON TRION (DEWETRON TRION Software R2.6)
    * DEWETRON ORION DAQ (ORION DAQ Driver V2.1.0.0)
    * DEWETRON ORION DSA (ORION DSA Driver V4.1.0.0)

* Installation procedure:
***TRION:
** Uninstall previous Oxygen version
** Uninstall any previous TRION version via system uninstall (control panel).
** Reboot system
** Install TRION applications
** Reboot system
** Start Dewe2Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
** Power-cycle TRION boards (Power down system, then restart)
** Install Oxygen
** Verify HW settings in system menu on first startup

* New Features Oxygen:
** Multi-file support: split DMD files by relative time
** Encoder: resampled RPM/Angle output, new sensor support: Tacho, CDM + Trigger, Quadrature/Linear Encoder
** Math formula: ecnt, hold, ...
** IIR Filter: LP/HP Butterworth or Bessel characteristic, Order 2-10
** Integrator/Differentiator: based on IIR filter

* HW Support:
***TRION - all supported modules	(Supported Measurement mode):
** TRION-1620-ACC-6-BNC			(Voltage, SW Current, IEPE, Simple CNT)
** TRION-1620-LV-6-BNC			(Voltage, SW Current)
** TRION-1620-LV-6-L1B			(Voltage, Current)
** TRION-1603-LV-6-BNC			(Voltage, SW Current)
** TRION-1603-LV-6-L1B			(Voltage, SW Current)
** TRION-1603-LV-6-D25			(Voltage, SW Current)
** TRION-2402-MULTI-4-D			(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE, CAN, MSI(%))
** TRION-2402-MULTI-8-L0B		(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE, CAN, MSI(%))
** TRION-2402-dSTG-6-L1B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-D			(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-L0B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-RJ			(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2400-dSTG-8-L0B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dACC-6-BNC		(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-dACC-8-SMB		(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-dACC-8-MD			(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-V-4-B			(Voltage, SW Current)
** TRION-2402-V-8-B			(Voltage, SW Current)
** TRION-CNT-6-L1B			(Simple CNT, Frequency)
** TRION-BASE				(IRIG B DC synchronization, Simple CNT, Frequency, DI, DO)
** TRION-TIMING				(IRIG A AC or DC, IRIG B AC or DC, GPS time sync, DI, DO)
** TRION-TIMING-V2			(IRIG A AC or DC, IRIG B AC or DC, GPS time sync, DI, DO)
** TRION-VGPS-x				(GPS time sync,Simple CNT, Frequency, DI, DO)
** TRION-CAN-4				(CAN)
** TRION-CAN-2				(CAN)
** TRION-DI48				(DI)
** TRION-1802				(Voltage, SW Current)	[incl. RS-485 + DAQP support]
** TRION-1600				(Voltage, SW Current)	[incl. RS-485 + DAQP support]
** TRION-1820-POWER-4			(Voltage, Current($))
(%) MSI-BR-TH-x, MSI-BR-CH-x
!CAN not available on TrendCorder enclosures!

($) Current module required for Current mode:
* SUB-dLV-1				(Current)
* SUB-CUR-20A-1				(Current)


***EPAD - all supported modules		(Supported Measurement mode):
** EPAD2-TH8-x				(Temperature, Voltage)
** EPAD2-TH8-UNIVERSAL			(Temperature, Voltage)
** EPAD2-V8				(Voltage)
** EPAD2-RTD8				(Temperature, Resistance)
** EPAD2-TH8-P				(Temperature(�), Voltage)
** EPAD2-LA8				(Current)
** EPAD -V8				(Voltage)
** EPAD -TH8-P				(Temperature(�), Voltage)

***PAD - all supported modules		(Supported Measurement mode):
** PAD-TH8-P				(Temperature(�), Voltage)
** PAD-V8-P				(Voltage)
** PAD-DO7				(DO)

(�) Connector block required for Temperature mode:
* PAD-CB8-x-P2				(Temperature)
* PAD-CB8-x-M				(Temperature)
* PAD-CB8-RTD-S3			(Temperature)


***ORION - all supported boards	(Supported Input type):
*  ORION DAQ Series (16 bit):
** ORION-0816-10M(%)			(Analog in, CAN)
** ORION-0816-5M (%)			(Analog in, CAN)
** ORION-0816-1000			(Analog in, CAN)
** ORION-0816-500			(Analog in, CAN)
** ORION-1616-10x			(Analog in, CAN)
** ORION-3216-10x			(Analog in, CAN)
*  ORION DSA Series (24 bit):
** ORION-1624-20x			(Analog in, CAN)
(%)data storing speed depends on hardware configuration
CAN only available on CAN enabled boards


***HSI/DAQP - all supported modules	(Supported Measurement mode):
** HSI-HV				(Voltage, SW Current)
** HSI-LV				(Voltage, SW Current)
** DAQP-HV				(Voltage, SW Current)
** DAQP-LV				(Voltage, SW Current)
** DAQP-STG				(Voltage, SW Current, Resistance, Bridge)
** HSI-STG				(Voltage, SW Current, Resistance, Bridge)
** DAQP-BRIDGE-A			(Voltage, SW Current, Bridge)
** DAQP-BRIDGE-B			(Voltage, SW Current, Bridge)
** DAQP-FREQ-A				(Frequency)
** DAQP-CFB2				(Bridge, Capacitance)
** DAQP-CHARGE-B			(Charge)
** DAQP-CHARGE-A			(Charge)
** DAQP-MULTI				(Voltage, SW Current, Resistance, Bridge, Temperature)
** DAQP-THERM				(Temperature)
** DAQP-ACC-A				(IEPE)
** DAQP-LA				(Current)
** DAQP-V				(Voltage, SW Current)
** DAQP-V-A				(Voltage, SW Current)
** DAQP-V-B				(Voltage, SW Current)
!All other modules not tested!

DI = Digital in
DO = Digital out

* Known Limitations, general:
FIXED ** When experiencing OpenGL graphic driver issues (white screen, cropped view or a touch area offset), use Oxygen (Safe Mode) shortcut in program folder to start Oxygen
** Total number of DAQP/HSI/PAD/EPAD modules on each serial port is limited to 32 (scan range 0-31)
** Each enclosure must have a unique serial number, else Oxygen will not start
** Slow data is used as an export option and can only be viewed in recorder instruments within Oxygen
** dejaVIEW may experience degrading performance on long slow async data recordings
** DMD recovery may lead to non perfect results, depending on filesize, sampling rate, no. of channels and channel type
** Only a reduced number of triggers is shown in recorder instruments
** PCI bus overload may lead to Oxygen fault
FIXED ** Power Group: Interval Mode working only up to 1000ms, above all values are NaN
** Power module: possible gap of a few milliseconds in live-data stream on pause-resume (recorded data is gapless)

* Known Limitations with TRION:
-

* Known Limitations with ORION:
** ORION-CNT not supported
** ORION-DI, DO not supported
** DAQ AD-boards: fixed AIRef set to Sense
** DSA AD-boards: only 5V AI range available (AIRef set to GND)
                  10V range for DAQP racks not supported (but is selectable in SW)


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
Release Notice DEWETRON Oxygen R2.5.1 x64

* Components:
** DEWETRON Oxygen	R2.5.1	(2.5.1.37269) (40f66a7d8662)
** DEWETRON DMDReader	R2.5	(2.5.36094.0) (caa5dc28489b)

* Files:
** DEWETRON_Oxygen_Setup_R2.5.1_x64.exe
** DEWETRON_DMDReader_R2.5.zip

* New Features Oxygen:
** ASAM MDF4 / MDF4.1 data export
** Power: 2-Wattmeter calculation

* Additional HW Support:
***EPAD - newly supported modules	(Supported Measurement mode):
** EPAD2-TH8-P				(Temperature(�), Voltage)
** EPAD -TH8-P				(Temperature(�), Voltage)

***PAD - newly supported modules	(Supported Measurement mode):
** PAD-TH8-P				(Temperature(�), Voltage)

(�) Connector block required for Temperature mode:
* PAD-CB8-x-P2				(Temperature)
* PAD-CB8-x-M				(Temperature)
* PAD-CB8-RTD-S3			(Temperature)


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +

Release Notice DEWETRON Oxygen R2.5 x64

* Components:
** DEWETRON Oxygen	R2.5	(2.5.0.36457) (e22ec4dbd2e7)
** DEWETRON DMDReader	R2.5	(2.5.36094.0) (caa5dc28489b)

* Files:
** DEWETRON_Oxygen_Setup_R2.5_x64.exe
** DEWETRON_DMDReader_R2.5.zip

* Requirements:
** OS: Windows 7 64bit, Windows 10 64bit
** CPU: Intel i5 3rd gen. or better
** RAM: 8 GB
** DAQ Hardware:
    * DEWETRON TRION (DEWETRON TRION Software R2.5)
    * DEWETRON ORION DAQ (ORION DAQ Driver V2.1.0.0)
    * DEWETRON ORION DSA (ORION DSA Driver V4.1.0.0)

* Installation procedure:
***TRION:
** Uninstall previous Oxygen version
** Uninstall any previous TRION version via system uninstall (control panel).
** Reboot system
** Install TRION applications
** Reboot system
** Start Dewe2Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
** Power-cycle TRION boards (Power down system, then restart)
** Install Oxygen
** Verify HW settings in system menu on first startup

* New Features Oxygen:
** TRION-1802/1600 HW support, incl. RS-485 and DAQP module auto-mapping
** Power: Harmonics up to 1000th order
** Power: up to 9 phases per Power Group
** Power: Line-Line RMS calculation (3 phase)
** Remote Control Interface (SCPI over Ethernet)

* New Features DMDReader:
** Absolute time in nanoseconds

* HW Support:
***TRION - all supported modules	(Supported Measurement mode):
** TRION-1620-ACC-6-BNC			(Voltage, SW Current, IEPE, Simple CNT)
** TRION-1620-LV-6-BNC			(Voltage, SW Current)
** TRION-1620-LV-6-L1B			(Voltage, Current)
** TRION-1603-LV-6-BNC			(Voltage, SW Current)
** TRION-1603-LV-6-L1B			(Voltage, SW Current)
** TRION-1603-LV-6-D25			(Voltage, SW Current)
** TRION-2402-MULTI-4-D			(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE, CAN, MSI(%))
** TRION-2402-MULTI-8-L0B		(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE, CAN, MSI(%))
** TRION-2402-dSTG-6-L1B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-D			(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-L0B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-RJ			(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2400-dSTG-8-L0B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dACC-6-BNC		(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-dACC-8-SMB		(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-dACC-8-MD			(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-V-4-B			(Voltage, SW Current)
** TRION-2402-V-8-B			(Voltage, SW Current)
** TRION-CNT-6-L1B			(Simple CNT, Frequency)
** TRION-BASE				(IRIG B DC synchronization, Simple CNT, Frequency, DI, DO)
** TRION-TIMING				(IRIG A AC or DC, IRIG B AC or DC, GPS time sync, DI, DO)
** TRION-TIMING-V2			(IRIG A AC or DC, IRIG B AC or DC, GPS time sync, DI, DO)
** TRION-VGPS-x				(GPS time sync,Simple CNT, Frequency, DI, DO)
** TRION-CAN-4				(CAN)
** TRION-CAN-2				(CAN)
** TRION-DI48				(DI)
** TRION-1802				(Voltage, SW Current)	[incl. RS-485 + DAQP support]
** TRION-1600				(Voltage, SW Current)	[incl. RS-485 + DAQP support]
(%) MSI-BR-TH-x, MSI-BR-CH-x
!CAN not available on TrendCorder enclosures!

***EPAD - all supported modules		(Supported Measurement mode):
** EPAD2-TH8-x				(Temperature, Voltage)
** EPAD2-TH8-UNIVERSAL			(Temperature, Voltage)
** EPAD2-V8				(Voltage)
** EPAD2-RTD8				(Temperature, Resistance)
** EPAD2-TH8-P				(Temperature, Voltage)
** EPAD2-LA8				(Current)
** EPAD -V8				(Voltage)
** EPAD -TH8-P-x			(Temperature)

***PAD - all supported modules		(Supported Measurement mode):
** PAD-TH8-P				(Temperature, Voltage)
** PAD-V8-P				(Voltage)
** PAD-DO7				(DO)

***ORION - all supported boards	(Supported Input type):
*  ORION DAQ Series (16 bit):
** ORION-0816-10M(%)			(Analog in, CAN)
** ORION-0816-5M (%)			(Analog in, CAN)
** ORION-0816-1000			(Analog in, CAN)
** ORION-0816-500			(Analog in, CAN)
** ORION-1616-10x			(Analog in, CAN)
** ORION-3216-10x			(Analog in, CAN)
*  ORION DSA Series (24 bit):
** ORION-1624-20x			(Analog in, CAN)
(%)data storing speed depends on hardware configuration
CAN only available on CAN enabled boards

***HSI/DAQP - all supported modules	(Supported Measurement mode):
** HSI-HV				(Voltage, SW Current)
** HSI-LV				(Voltage, SW Current)
** DAQP-HV				(Voltage, SW Current)
** DAQP-LV				(Voltage, SW Current)
** DAQP-STG				(Voltage, SW Current, Resistance, Bridge)
** HSI-STG				(Voltage, SW Current, Resistance, Bridge)
** DAQP-BRIDGE-A			(Voltage, SW Current, Bridge)
** DAQP-BRIDGE-B			(Voltage, SW Current, Bridge)
** DAQP-FREQ-A				(Frequency)
** DAQP-CFB2				(Bridge, Capacitance)
** DAQP-CHARGE-B			(Charge)
** DAQP-CHARGE-A			(Charge)
** DAQP-MULTI				(Voltage, SW Current, Resistance, Bridge, Temperature)
** DAQP-THERM				(Temperature)
** DAQP-ACC-A				(IEPE)
** DAQP-LA				(Current)
** DAQP-V				(Voltage, SW Current)
** DAQP-V-A				(Voltage, SW Current)
** DAQP-V-B				(Voltage, SW Current)
!All other modules not tested!

DI = Digital in
DO = Digital out

* Known Limitations, general:
** When experiencing OpenGL graphic driver issues (white screen, cropped view or a touch area offset), use Oxygen (Safe Mode) shortcut in program folder to start Oxygen
** Total number of DAQP/HSI/PAD/EPAD modules on each serial port is limited to 32 (scan range 0-31)
** Each enclosure must have a unique serial number, else Oxygen will not start
** Slow data is used as an export option and can only be viewed in recorder instruments within Oxygen
** dejaVIEW may experience degrading performance on long slow async data recordings
** DMD recovery may lead to non perfect results, depending on filesize, sampling rate, no. of channels and channel type
** Only a reduced number of triggers is shown in recorder instruments
** PCI bus overload may lead to Oxygen fault
** Power Group: Interval Mode working only up to 1000ms, above all values are NaN

* Known Limitations with TRION:
-

* Known Limitations with ORION:
** ORION-CNT not supported
** ORION-DI, DO not supported
** DAQ AD-boards: fixed AIRef set to Sense
** DSA AD-boards: - only 5V AI range available (AIRef set to GND)
                  - 10V range for DAQP racks not supported (but is selectable in SW)


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
Release Notice DEWETRON Oxygen R2.4.1 x64

* Components:
** DEWETRON Oxygen	R2.4.1	(2.4.1.34258) (07e24636c40a)
** DEWETRON DMDReader	R2.4	(2.4.33931.0) (6c6192c8f67e)

* Files:
** DEWETRON_Oxygen_Setup_R2.4.1_x64.exe
** DEWETRON_DMDReader_R2.4.zip

* Bugfixes:

FIXED	Power calculation
FIXED	Keyboard focus
FIXED	Scope trigger (fast signals)
FIXED	FFT replay, load data
FIXED	FFT, line resolution fix
FIXED	fixed DWModules (EPAD bug)


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
Release Notice DEWETRON Oxygen R2.4 x64

* Components:
** DEWETRON Oxygen	R2.4	(2.4.0.33520) (f092c8c5fcd3)
** DEWETRON DMDReader	R2.4	(2.4.33931.0) (6c6192c8f67e)

* Files:
** DEWETRON_Oxygen_Setup_R2.4_x64.exe
** DEWETRON_DMDReader_R2.4.zip

* Requirements:
** OS: Windows 7 64bit, Windows 10 64bit
** CPU: Intel i5 3rd gen. or better
** RAM: 8 GB
** DAQ Hardware:
    * DEWETRON TRION (DEWETRON TRION Software R2.4.4)
    * DEWETRON ORION DAQ (ORION DAQ Driver V2.1.0.0)
    * DEWETRON ORION DSA (ORION DSA Driver V4.1.0.0)

* Installation procedure:
***TRION:
** Uninstall previous Oxygen version
** Uninstall any previous TRION version via system uninstall (control panel).
** Reboot system
** Install TRION applications
** Reboot system
** Start Dewe2Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
** Power-cycle TRION boards (Power down system, then restart)
** Install Oxygen
** Verify HW settings in system menu on first startup

* New Features Oxygen:
** Power: Assisted Power configuration
** Power: Flicker Emission
** Alarm out/Events triggering + GUI update
** XY instrument
** GigE AVT (Allied Vision Technologies) camera support, incl. synchronized Video
** FFT averaging, log axes, additional spectra
** WYSIWYG Reporting

* New Features DMDReader:
-

* HW Support:
***TRION - all supported modules	(Supported Measurement mode):
** TRION-1620-ACC-6-BNC			(Voltage, SW Current, IEPE, Simple CNT)
** TRION-1620-LV-6-BNC			(Voltage, SW Current)
** TRION-1620-LV-6-L1B			(Voltage, Current)
** TRION-1603-LV-6-BNC			(Voltage, SW Current)
** TRION-1603-LV-6-L1B			(Voltage, SW Current)
** TRION-2402-MULTI-4-D			(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE, CAN, MSI(%))
** TRION-2402-MULTI-8-L0B		(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE, CAN, MSI(%))
** TRION-2402-dSTG-6-L1B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-D			(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-L0B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-RJ			(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2400-dSTG-8-L0B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dACC-6-BNC		(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-dACC-8-SMB		(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-dACC-8-MD			(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-V-4-B			(Voltage, SW Current)
** TRION-2402-V-8-B			(Voltage, SW Current)
** TRION-CNT-6-L1B			(Simple CNT, Frequency)
** TRION-BASE				(IRIG B DC synchronization, Simple CNT, Frequency, DI, DO)
** TRION-TIMING				(IRIG A AC or DC, IRIG B AC or DC, GPS time sync, DI, DO)
** TRION-VGPS-x				(GPS time sync,Simple CNT, Frequency, DI, DO)
** TRION-CAN-4				(CAN)
** TRION-CAN-2				(CAN)
** TRION-DI48				(DI)
(%) MSI-BR-TH-x, MSI-BR-CH-x
!CAN not available on TrendCorder enclosures!

***EPAD - all supported modules		(Supported Measurement mode):
** EPAD2-TH8-x				(Temperature, Voltage)
** EPAD2-TH8-UNIVERSAL			(Temperature, Voltage)
** EPAD2-V8				(Voltage)
** EPAD2-RTD8				(Temperature, Resistance)
** EPAD2-TH8-P				(Temperature, Voltage)
** EPAD2-LA8				(Current)
** EPAD-V8				(Voltage)
** EPAD-TH8-P-x				(Temperature)

***ORION - all supported boards	(Supported Input type):
*  ORION DAQ Series (16 bit):
** ORION-0816-10M(%)			(Analog in, CAN)
** ORION-0816-5M (%)			(Analog in, CAN)
** ORION-0816-1000			(Analog in, CAN)
** ORION-0816-500			(Analog in, CAN)
** ORION-1616-10x			(Analog in, CAN)
** ORION-3216-10x			(Analog in, CAN)
*  ORION DSA Series (24 bit):
** ORION-1624-20x			(Analog in, CAN)
(%)data storing speed depends on hardware configuration
CAN only available on CAN enabled boards

***HSI/DAQP - all supported modules	(Supported Measurement mode):
** HSI-HV				(Voltage, SW Current)
** HSI-LV				(Voltage, SW Current)
** DAQP-HV				(Voltage, SW Current)
** DAQP-LV				(Voltage, SW Current)
** DAQP-STG				(Voltage, SW Current, Resistance, Bridge, Temperature)
** HSI-STG				(Voltage, SW Current, Resistance, Bridge, Temperature)
** DAQP-BRIDGE-A			(Voltage, SW Current, Bridge)
** DAQP-BRIDGE-B			(Voltage, SW Current, Bridge)
** DAQP-FREQ-A				(Frequency)
** DAQP-CFB2				(Bridge, Capacitance)
** DAQP-CHARGE-B			(Charge)
!All other modules not tested!

***PAD - all supported modules		(Supported Measurement mode):
** PAD-TH8-P				(Temperature, Voltage)
** PAD-V8-P				(Voltage)
** PAD-DO7				(DO)

DI = Digital in
DO = Digital out

* Known Limitations, general:
** When experiencing OpenGL graphic driver issues (white screen), use Oxygen (Safe Mode) shortcut in program folder to start Oxygen
** Slow data is used as an export option and can only be viewed in recorder instruments
** dejaVIEW may experience degrading performance on long slow async data recordings
** DMD recovery may lead to non perfect results, depending on filesize, sampling rate, no. of channels and channel type
** Only a reduced number of triggers is shown in recorder instruments
** PCI bus overload may lead to Oxygen fault

* Known Limitations with TRION:
-

* Known Limitations with ORION:
** ORION-onboard RS485 communication only supported for one board
** ORION-CNT not supported
** ORION-DI, DO not supported
** DAQ AD-boards: only 5V AI range available (AIRef set to Sense)
** DSA AD-boards: only 5V AI range available (AIRef set to GND)
** Total number of DAQP/HSI modules limited to 32 (on one serial port)


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
Release Notice DEWETRON Oxygen R2.3.2 x64

* Components:
** DEWETRON Oxygen	R2.3.2	(2.3.2.30754)
** DEWETRON DMDReader	R2.3	(2.3.28633.0)

* Files:
** DEWETRON_Oxygen_Setup_R2.3.2_x64.exe
** DEWETRON_DMDReader_R2.3.zip

* Requirements:
** OS: Windows 7 64bit, Windows 10 64bit
** CPU: Intel i5 3rd gen. or better
** RAM: 8 GB
** DAQ Hardware:
    * DEWETRON TRION (DEWETRON TRION Software R2.4.1)
    * DEWETRON ORION DAQ (ORION DAQ Driver V2.1.0.0)
    * DEWETRON ORION DSA (ORION DSA Driver V4.1.0.0)

* Installation procedure:
***TRION:
** Uninstall previous Oxygen version
** Uninstall any previous TRION version via system uninstall (control panel).
** Reboot system
** Install TRION applications
** Reboot system
** Start Dewe2Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
** Power-cycle TRION boards (Power down system, then restart)
** Install Oxygen
** Verify HW settings in system menu on first startup

* New Features Oxygen:
-

* New Features DMDReader:
-

* Bugfixes:
FIXED	Triggered export -> not all data exported
FIXED	No trigger, under rare circumstances
FIXED	DI channels on multiple TRION enclosures not assigned correctly


* HW Support:
***TRION - all supported modules	(Supported Measurement mode):
** TRION-1620-ACC-6-BNC			(Voltage, SW Current, IEPE, Simple CNT)
** TRION-1620-LV-6-BNC			(Voltage, SW Current)
** TRION-1620-LV-6-L1B			(Voltage, Current)
** TRION-1603-LV-6-BNC			(Voltage, SW Current)
** TRION-1603-LV-6-L1B			(Voltage, SW Current)
** TRION-2402-MULTI-4-D			(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE, CAN, MSI(%))
** TRION-2402-MULTI-8-L0B		(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE, CAN, MSI(%))
** TRION-2402-dSTG-6-L1B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-D			(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-L0B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-RJ			(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2400-dSTG-8-L0B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dACC-6-BNC		(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-dACC-8-SMB		(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-dACC-8-MD			(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-V-4-B			(Voltage, SW Current)
** TRION-2402-V-8-B			(Voltage, SW Current)
** TRION-CNT-6-L1B			(Simple CNT, Frequency)
** TRION-BASE				(IRIG B DC synchronization, Simple CNT, Frequency, DI)
** TRION-TIMING				(IRIG A AC or DC, IRIG B AC or DC, GPS time sync, DI)
** TRION-VGPS-x				(GPS time sync)
** TRION-CAN-4				(CAN)
** TRION-CAN-2				(CAN)
** TRION-DI48				(DI)
(%) MSI-BR-TH-x, MSI-BR-CH-x
!CAN not available on TrendCorder enclosures!

***EPAD - all supported modules		(Supported Measurement mode):
** EPAD2-TH8-x				(Temperature, Voltage)
** EPAD2-TH8-UNIVERSAL			(Temperature, Voltage)
** EPAD2-V8				(Voltage)
** EPAD2-RTD8				(Temperature, Resistance)
** EPAD2-TH8-P				(Temperature, Voltage)
** EPAD2-LA8				(Current)
** EPAD-V8				(Voltage)
** EPAD-TH8-P-x				(Temperature)

***ORION - all supported boards	(Supported Input type):
*  ORION DAQ Series (16 bit):
** ORION-0816-10M(%)			(Analog in, CAN)
** ORION-0816-5M (%)			(Analog in, CAN)
** ORION-0816-1000			(Analog in, CAN)
** ORION-0816-500			(Analog in, CAN)
** ORION-1616-10x			(Analog in, CAN)
** ORION-3216-10x			(Analog in, CAN)
*  ORION DSA Series (24 bit):
** ORION-1624-20x			(Analog in, CAN)
(%)data storing speed depends on hardware configuration
CAN only available on CAN enabled boards

***HSI/DAQP - all supported modules	(Supported Measurement mode):
** HSI-HV				(Voltage, SW Current)
** HSI-LV				(Voltage, SW Current)
** DAQP-HV				(Voltage, SW Current)
** DAQP-LV				(Voltage, SW Current)
** DAQP-STG				(Voltage, SW Current, Resistance, Bridge, Temperature)
** HSI-STG				(Voltage, SW Current, Resistance, Bridge, Temperature)
** DAQP-BRIDGE-A			(Voltage, SW Current, Bridge)
** DAQP-BRIDGE-B			(Voltage, SW Current, Bridge)
** DAQP-FREQ-A				(Frequency)
** DAQP-CFB2				(Bridge, Capacitance)
** DAQP-CHARGE-B			(Charge)
!All other modules not tested!

***PAD - all supported modules		(Supported Measurement mode):
** PAD-TH8-P				(Temperature, Voltage)
** PAD-V8-P				(Voltage)
** PAD-DO7(%)				(Digital Out)
(%)cannot be used yet, alarm triggers missing

* Known Limitations, general:
** When experiencing OpenGL graphic driver issues (white screen), use Oxygen (Safe Mode) shortcut in program folder to start Oxygen
** Slow data is used as an export option and can only be viewed in recorder instruments
** dejaVIEW may experience degrading performance on long slow async data recordings
** DMD recovery may lead to non perfect results, depending on filesize, sampling rate, no. of channels and channel type
** Only a reduced number of triggers is shown in recorder instruments
** PCI bus overload may lead to Oxygen fault

* Known Limitations with TRION:
-

* Known Limitations with ORION:
** ORION-onboard RS485 communication only supported for one board
** ORION-CNT not supported
** ORION-DI not supported
** DAQ AD-boards: only 5V AI range available (AIRef set to Sense)
** DSA AD-boards: only 5V AI range available (AIRef set to GND)
** Total number of DAQP/HSI modules limited to 32 (on one serial port)


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + ++ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
Release Notice DEWETRON Oxygen R2.3.1 x64

* Components:
** DEWETRON Oxygen	R2.3.1	(2.3.1.30189)
** DEWETRON DMDReader	R2.3	(2.3.28633.0)

* Files:
** DEWETRON_Oxygen_Setup_R2.3.1_x64.exe
** DEWETRON_DMDReader_R2.3.zip

* Requirements:
** OS: Windows 7 64bit, Windows 10 64bit
** CPU: Intel i5 3rd gen. or better
** RAM: 8 GB
** DAQ Hardware:
    * DEWETRON TRION (DEWETRON TRION Software R2.4.1)
    * DEWETRON ORION DAQ (ORION DAQ Driver V2.1.0.0)
    * DEWETRON ORION DSA (ORION DSA Driver V4.1.0.0)

* Installation procedure:
***TRION:
** Uninstall previous Oxygen version
** Uninstall any previous TRION version via system uninstall (control panel).
** Reboot system
** Install TRION applications
** Reboot system
** Start Dewe2Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
** Power-cycle TRION boards (Power down system, then restart)
** Install Oxygen
** Verify HW settings in system menu on first startup

* New Features Oxygen:
** HW support: DAQP-CFB2, DAQP-CHARGE-B, PAD-DO7(cannot be used yet, alarm triggers missing)
** FFT: additional scaling (dB RMS etc.), draggable markers, copy-paste data
** GUI: sync indicator and status improvement, day of year added in absolute time mode
** Math Statistics: ACRMS calculation added
** Localisation: French, Polish, Chinese added
** Setup: can now be loaded onto physically different hardware (different serial no. or enclosure)

* New Features DMDReader:
-


* HW Support:
***TRION - all supported modules	(Supported Measurement mode):
** TRION-1620-ACC-6-BNC			(Voltage, SW Current, IEPE, Simple CNT)
** TRION-1620-LV-6-BNC			(Voltage, SW Current)
** TRION-1620-LV-6-L1B			(Voltage, Current)
** TRION-1603-LV-6-BNC			(Voltage, SW Current)
** TRION-1603-LV-6-L1B			(Voltage, SW Current)
** TRION-2402-MULTI-4-D			(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE, CAN, MSI�)
** TRION-2402-MULTI-8-L0B		(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE, CAN, MSI�)
** TRION-2402-dSTG-6-L1B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-D			(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-L0B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-RJ			(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2400-dSTG-8-L0B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dACC-6-BNC		(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-dACC-8-SMB		(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-dACC-8-MD			(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-V-4-B			(Voltage, SW Current)
** TRION-2402-V-8-B			(Voltage, SW Current)
** TRION-CNT-6-L1B			(Simple CNT, Frequency)
** TRION-BASE				(IRIG B DC synchronization, Simple CNT, Frequency,  DI)
** TRION-TIMING				(IRIG A AC or DC, IRIG B AC or DC, GPS time sync, DI)
** TRION-VGPS-x				(GPS time sync)
** TRION-CAN-4				(CAN)
** TRION-CAN-2				(CAN)
** TRION-DI48				(DI)
�MSI-BR-TH-x, MSI-BR-CH-x
!CAN not available on TrendCorder enclosures!

***EPAD - all supported modules		(Supported Measurement mode):
** EPAD2-TH8-x				(Temperature, Voltage)
** EPAD2-TH8-UNIVERSAL			(Temperature, Voltage)
** EPAD2-V8				(Voltage)
** EPAD2-RTD8				(Temperature, Resistance)
** EPAD2-TH8-P				(Temperature, Voltage)
** EPAD2-LA8				(Current)
** EPAD-V8				(Voltage)
** EPAD-TH8-P-x				(Temperature)

***ORION - all supported boards	(Supported Input type):
*  ORION DAQ Series (16 bit):
** ORION-0816-10M(%)			(Analog in, CAN)
** ORION-0816-5M (%)			(Analog in, CAN)
** ORION-0816-1000			(Analog in, CAN)
** ORION-0816-500			(Analog in, CAN)
** ORION-1616-10x			(Analog in, CAN)
** ORION-3216-10x			(Analog in, CAN)
*  ORION DSA Series (24 bit):
** ORION-1624-20x			(Analog in, CAN)
(%)data storing speed depends on hardware configuration
CAN only available on CAN enabled boards

***HSI/DAQP - all supported modules	(Supported Measurement mode):
** HSI-HV				(Voltage, SW Current)
** HSI-LV				(Voltage, SW Current)
** DAQP-HV				(Voltage, SW Current)
** DAQP-LV				(Voltage, SW Current)
** DAQP-STG				(Voltage, SW Current, Resistance, Bridge, Temperature)
** HSI-STG				(Voltage, SW Current, Resistance, Bridge, Temperature)
** DAQP-BRIDGE-A			(Voltage, SW Current, Bridge)
** DAQP-BRIDGE-B			(Voltage, SW Current, Bridge)
** DAQP-FREQ-A				(Frequency)
** DAQP-CFB2				(Bridge, Capacitance)
** DAQP-CHARGE-B			(Charge)
!All other modules not tested!

***PAD - all supported modules		(Supported Measurement mode):
** PAD-TH8-P				(Temperature, Voltage)
** PAD-V8-P				(Voltage)
** PAD-DO7(%)				(Digital Out)
(%)cannot be used yet, alarm triggers missing

* Known Limitations, general:
** When experiencing OpenGL graphic driver issues (white screen), use Oxygen (Safe Mode) shortcut in program folder to start Oxygen
** Slow data is used as an export option and can only be viewed in recorder instruments
** dejaVIEW may experience degrading performance on long slow async data recordings
** DMD recovery may lead to non perfect results, depending on filesize, sampling rate, no. of channels and channel type
** Only a reduced number of triggers is shown in recorder instruments
** PCI bus overload may lead to Oxygen fault

* Known Limitations with TRION:
-

* Known Limitations with ORION:
** ORION-onboard RS485 communication only supported for one board
** ORION-CNT not supported
** ORION-DI not supported
** DAQ AD-boards: only 5V AI range available (AIRef set to Sense)
** DSA AD-boards: only 5V AI range available (AIRef set to GND)
** Total number of DAQP/HSI modules limited to 32 (on one serial port)


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
Release Notice DEWETRON Oxygen R2.3 x64

* Components:
** DEWETRON Oxygen	R2.3	(2.3.0.28658)
** DEWETRON DMDReader	R2.3	(2.3.28633.0)

* Files:
** DEWETRON_Oxygen_Setup_R2.3_x64.exe
** DEWETRON_DMDReader_R2.3.zip

* Requirements:
** OS: Windows 7 64bit, Windows 10 64bit
** CPU: Intel i5 3rd gen. or better
** RAM: 8 GB
** DAQ Hardware:
    * DEWETRON TRION (DEWETRON TRION Software R2.4)
    * DEWETRON ORION DAQ (ORION DAQ Driver V2.1.0.0)
    * DEWETRON ORION DSA (ORION DSA Driver V4.1.0.0)

* Installation procedure:
***TRION:
** Uninstall previous Oxygen version
** Uninstall any previous TRION version via system uninstall (control panel).
** Reboot system
** Install TRION applications
** Reboot system
** Start Dewe2Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
** Power-cycle TRION boards (Power down system, then restart)
** Install Oxygen
** Verify HW settings in system menu on first startup

* New Features Oxygen:
** Windows 10 64bit support
** HW support: TRION DI, ORION CAN, DAQP-BRIDGE-A, DAQP-BRIDGE-B, DAQP-FREQ-A
** DEWE2(A, M) + TRIONet synchronized measurement
** DEWE2(A, M) + DEWE2(F) synchronized measurement
** Advanced Power: Harmonic calculation + Instrument, Voltage Flicker
** USB Video
** Localisation (German)

* New Features DMDReader:
** Array channel support
** PowerGroup channel prefix


* HW Support:
***TRION - all supported modules	(Supported Measurement mode):
** TRION-1620-ACC-6-BNC			(Voltage, SW Current, IEPE, Simple CNT)
** TRION-1620-LV-6-BNC			(Voltage, SW Current)
** TRION-1620-LV-6-L1B			(Voltage, Current)
** TRION-1603-LV-6-BNC			(Voltage, SW Current)
** TRION-1603-LV-6-L1B			(Voltage, SW Current)
** TRION-2402-MULTI-4-D			(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE, CAN, MSI)
** TRION-2402-MULTI-8-L0B		(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE, CAN, MSI)
** TRION-2402-dSTG-6-L1B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-D			(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-L0B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-RJ			(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2400-dSTG-8-L0B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dACC-6-BNC		(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-dACC-8-SMB		(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-dACC-8-MD			(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-V-4-B			(Voltage, SW Current)
** TRION-2402-V-8-B			(Voltage, SW Current)
** TRION-CNT-6-L1B			(Simple CNT, Frequency)
** TRION-BASE				(IRIG B DC synchronization, Simple CNT, Frequency,  DI)
** TRION-TIMING				(IRIG A AC or DC, IRIG B AC or DC, GPS time sync, DI)
** TRION-VGPS-x				(GPS time sync)
** TRION-CAN-4				(CAN)
** TRION-CAN-2				(CAN)
** TRION-DI48				(DI)
!CAN not available on TrendCorder enclosures!

***EPAD - all supported modules		(Supported Measurement mode):
** EPAD2-TH8-x				(Temperature, Voltage)
** EPAD2-TH8-UNIVERSAL			(Temperature, Voltage)
** EPAD2-V8				(Voltage)
** EPAD2-RTD8				(Temperature, Resistance)
** EPAD2-TH8-P				(Temperature, Voltage)
** EPAD2-LA8				(Current)
** EPAD-V8				(Voltage)
** EPAD-TH8-P-x				(Temperature)

***ORION - all supported boards	(Supported Input type):
*  ORION DAQ Series (16 bit):
** ORION-0816-10M(%)			(Analog in, CAN)
** ORION-0816-5M (%)			(Analog in, CAN)
** ORION-0816-1000			(Analog in, CAN)
** ORION-0816-500			(Analog in, CAN)
** ORION-1616-10x			(Analog in, CAN)
** ORION-3216-10x			(Analog in, CAN)
*  ORION DSA Series (24 bit):
** ORION-1624-20x			(Analog in, CAN)
(%)data storing speed depends on hardware configuration
CAN only available on CAN enabled boards

***HSI/DAQP - all supported modules	(Supported Measurement mode):
** HSI-HV				(Voltage, SW Current)
** HSI-LV				(Voltage, SW Current)
** DAQP-HV				(Voltage, SW Current)
** DAQP-LV				(Voltage, SW Current)
** DAQP-STG				(Voltage, SW Current, Resistance, Bridge, Temperature)
** HSI-STG				(Voltage, SW Current, Resistance, Bridge, Temperature)
** DAQP-BRIDGE-A			(Voltage, SW Current, Bridge)
** DAQP-BRIDGE-B			(Voltage, SW Current, Bridge)
** DAQP-FREQ-A				(Frequency)
!All other modules not tested!

***PAD - all supported modules		(Supported Measurement mode):
** PAD-TH8-P				(Temperature, Voltage)
** PAD-V8-P				(Voltage)


* Known Limitations, general:
** When experiencing OpenGL graphic driver issues (white screen), use Oxygen (Safe Mode) shortcut in program folder to start Oxygen
** Slow data is used as an export option and can only be viewed in recorder instruments
** dejaVIEW may experience degrading performance on long slow async data recordings
** DMD recovery may lead to non perfect results, depending on filesize, sampling rate, no. of channels and channel type
** Only a reduced number of triggers is shown in recorder instruments
** PCI bus overload may lead to Oxygen fault

* Known Limitations, TRION:
-

* Known Limitations, ORION:
** ORION-onboard RS485 communication only supported for one board
** ORION-CNT not supported
** ORION-DI not supported
** DAQ AD-boards: only 5V AI range available (AIRef set to Sense)
** DSA AD-boards: only 5V AI range available (AIRef set to GND)
** Total number of DAQP/HSI modules limited to 16


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
Release Notice DEWETRON Oxygen R2.2 x64

* Components:
** DEWETRON Oxygen	R2.2	(2.2.0.25355)
** DEWETRON DMDReader	R2.1	(2.1.22493.0)

* Files:
** DEWETRON_Oxygen_Setup_R2.2_x64.exe
** DEWETRON_DMDReader_R2.1.zip

* Requirements:
** OS: Windows 7 64bit
** CPU: Intel i5 3rd gen. or better
** RAM: 8 GB
** DAQ Hardware:
    * DEWETRON TRION (DEWETRON TRION Software R2.3.2)
    * DEWETRON ORION DAQ (ORION DAQ Driver V2.0.0.9)
    * DEWETRON ORION DSA (ORION DSA Driver V4.0.0.3)

* Installation procedure:
***TRION:
** Uninstall previous Oxygen version
** Uninstall any previous TRION version via system uninstall (control panel).
** Reboot system
** Install TRION applications
** Reboot system
** Start Dewe2Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
** Power-cycle TRION boards (Power down system, then restart)
** Install Oxygen
** Verify HW settings in system menu on first startup

* New Features Oxygen:
** Basic Statistics
** MSI TRION
** FFT instrument
** Scope instrument
** Licensing / Evaluation version
** Basic Power option

* HW Support:
***TRION - all supported modules	(Supported Measurement mode)
** TRION-1620-ACC-6-BNC			(Voltage, SW Current, IEPE, Simple CNT)
** TRION-1620-LV-6-BNC			(Voltage, SW Current)
** TRION-1620-LV-6-L1B			(Voltage, Current)
** TRION-1603-LV-6-BNC			(Voltage, SW Current)
** TRION-1603-LV-6-L1B			(Voltage, SW Current)
** TRION-2402-MULTI-4-D			(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE, CAN, MSI)
** TRION-2402-MULTI-8-L0B		(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE, CAN, MSI)
** TRION-2402-dSTG-6-L1B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-D			(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-L0B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-RJ			(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2400-dSTG-8-L0B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dACC-6-BNC		(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-dACC-8-SMB		(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-dACC-8-MD			(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-V-4-B			(Voltage, SW Current)
** TRION-2402-V-8-B			(Voltage, SW Current)
** TRION-CNT-6-L1B			(Simple CNT, Frequency)
** TRION-BASE				(IRIG B DC synchronization, Simple CNT)
** TRION-TIMING				(IRIG A AC or DC, IRIG B AC or DC, GPS time synchronization)
** TRION-VGPS-x				(GPS time synchronization)
** TRION-CAN-4				(CAN)
** TRION-CAN-2				(CAN)
!CAN not available on TrendCorder enclosures!

***EPAD - all supported modules		(Supported Measurement mode)
** EPAD2-TH8-x                     	(Temperature, Voltage)
** EPAD2-TH8-UNIVERSAL                  (Temperature, Voltage)
** EPAD2-V8                             (Voltage)
** EPAD2-RTD8                           (Temperature, Resistance)
** EPAD2-TH8-P				(Temperature, Voltage)
** EPAD2-LA8				(Current)
** EPAD-V8				(Voltage)
** EPAD-TH8-P-x				(Temperature)

***ORION - all supported boards		(Supported Input type)
*  ORION DAQ Series (16 bit):
** ORION-0816-10M(%)			(Analog in)
** ORION-0816-5M (%)			(Analog in)
** ORION-0816-1000			(Analog in)
** ORION-0816-500			(Analog in)
** ORION-1616-10x			(Analog in)
** ORION-3216-10x			(Analog in)
*  ORION DSA Series (24 bit):
** ORION-1624-20x			(Analog in)
** ORION-1622-10x			(Analog in)
(%)data storing speed depends on hardware configuration

***HSI/DAQP - all supported modules	(Supported Measurement mode)
** HSI -HV				(Voltage, SW Current)
** HSI -LV				(Voltage, SW Current)
** DAQP-HV				(Voltage, SW Current)
** DAQP-LV				(Voltage, SW Current)
** DAQP-STG				(Voltage, SW Current, Resistance, Bridge, Temperature)
** HSI -STG				(Voltage, SW Current, Resistance, Bridge, Temperature)
!All other modules not tested!

* Known Limitations, general:
** Slow data is used as an export option and can only be viewed in recorder instruments
** dejaVIEW may experience degrading performance on long slow async data recordings
** DMD recovery may lead to non perfect results, depending on filesize, sampling rate, no. of channels and channel type
** Only a reduced number of triggers is shown in recorder instruments
** PCI bus overload may lead to Oxygen fault

* Known Limitations, TRION:
** TRIONet may not be used together with a local TRION system (e.g DEWE2-A4 + TRIONet)

* Known Limitations, ORION:
** ORION-onboard RS485 communication only supported for one board
** ORION-CAN not supported
** ORION-CNT not supported
** ORION-DI not supported
** DAQ AD-boards: only 5V AI range available (AIRef set to Sense)
** DSA AD-boards: only 5V AI range available (AIRef set to GND)
** Total number of DAQP/HSI modules limited to 16


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
Release Notice DEWETRON Oxygen R2.1.1 x64

* Components:
** DEWETRON Oxygen	R2.1.1	(2.1.0.24029)
** DEWETRON DMDReader	R2.1	(2.1.22493.0)

* Files:
** DEWETRON_Oxygen_Setup_R2.1.1_x64.exe
** DEWETRON_DMDReader_R2.1.zip

* Requirements:
** OS: Windows 7 64bit
** CPU: Intel i5 3rd gen. or better
** RAM: 8 GB
** DAQ Hardware:
    * DEWETRON TRION (DEWETRON TRION Software R2.3.2)
    * DEWETRON ORION DAQ (ORION DAQ Driver V2.0.0.9)
    * DEWETRON ORION DSA (ORION DSA Driver V4.0.0.3)

* Installation procedure:
***TRION:
** Uninstall previous Oxygen version
** Uninstall any previous TRION version via system uninstall (control panel).
** Reboot system
** Install TRION applications
** Reboot system
** Start Dewe2Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
** Power-cycle TRION boards (Power down system, then restart)
** Install Oxygen
** Verify HW settings in system menu on first startup

* New Features Oxygen:
** ORION DSA support
** DAQP/HSI-STG support

* HW Support:
***TRION - all supported modules	(Supported Measurement mode)
** TRION-1620-ACC-6-BNC			(Voltage, SW Current, IEPE, Simple CNT)
** TRION-1620-LV-6-BNC			(Voltage, SW Current)
** TRION-1620-LV-6-L1B			(Voltage, Current)
** TRION-1603-LV-6-BNC			(Voltage, SW Current)
** TRION-1603-LV-6-L1B			(Voltage, SW Current)
** TRION-2402-MULTI-4-D			(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE, CAN)
** TRION-2402-MULTI-8-L0B		(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE, CAN)
** TRION-2402-dSTG-6-L1B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-D			(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-L0B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-RJ			(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2400-dSTG-8-L0B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dACC-6-BNC		(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-dACC-8-SMB		(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-dACC-8-MD			(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-V-4-B			(Voltage, SW Current)
** TRION-2402-V-8-B			(Voltage, SW Current)
** TRION-CNT-6-L1B			(Simple CNT, Frequency)
** TRION-BASE				(IRIG B DC synchronization, Simple CNT)
** TRION-TIMING				(IRIG A AC or DC, IRIG B AC or DC, GPS time synchronization)
** TRION-VGPS-x				(GPS time synchronization)
** TRION-CAN-4				(CAN)
** TRION-CAN-2				(CAN)
!CAN not available on TrendCorder enclosures!

***EPAD - all supported modules		(Supported Measurement mode)
** EPAD2-TH8-x                     	(Temperature, Voltage)
** EPAD2-TH8-UNIVERSAL                  (Temperature, Voltage)
** EPAD2-V8                             (Voltage)
** EPAD2-RTD8                           (Temperature, Resistance)
** EPAD2-TH8-P				(Temperature, Voltage)
** EPAD2-LA8				(Current)
** EPAD-V8				(Voltage)
** EPAD-TH8-P-x				(Temperature)

***ORION - all supported boards		(Supported Input type)
*  ORION DAQ Series (16 bit):
** ORION-0816-10M(%)			(Analog in)
** ORION-0816-5M (%)			(Analog in)
** ORION-0816-1000			(Analog in)
** ORION-0816-500			(Analog in)
** ORION-1616-10x			(Analog in)
** ORION-3216-10x			(Analog in)
*  ORION DSA Series (24 bit):
** ORION-1624-20x			(Analog in)
** ORION-1622-10x			(Analog in)
(%)data storing speed depends on hardware configuration

***HSI/DAQP - all supported modules	(Supported Measurement mode)
** HSI -HV				(Voltage, SW Current)
** HSI -LV				(Voltage, SW Current)
** DAQP-HV				(Voltage, SW Current)
** DAQP-LV				(Voltage, SW Current)
** DAQP-STG				(Voltage, SW Current, Resistance, Bridge, Temperature)
** HSI -STG				(Voltage, SW Current, Resistance, Bridge, Temperature)
!All other modules not tested!

* Known Limitations, general:
** Slow data is used as an export option and can only be viewed in recorder instruments
** TRION-MULTI MSI not supported
** dejaVIEW may experience degrading performance on long slow async data recordings
** DMD recovery may lead to non perfect results, depending on filesize, sampling rate, no. of channels and channel type
** Only a reduced number of triggers is shown in recorder instruments
** PCI bus overload may lead to Oxygen fault

* Known Limitations, TRION:
** TRIONet may not be used together with a local TRION system (e.g DEWE2-A4 + TRIONet)

* Known Limitations, ORION:
** ORION-onboard RS485 communication only supported for one board
** ORION-CAN not supported
** ORION-CNT not supported
** ORION-DI not supported
** DAQ AD-boards: only 5V AI range available (AIRef set to Sense)
** DSA AD-boards: only 5V AI range available (AIRef set to GND)
** Total number of DAQP/HSI modules limited to 16


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
Release Notice DEWETRON Oxygen R2.1 x64

* Components:
** DEWETRON Oxygen	R2.1	(2.1.0.22505)
** DEWETRON DMDReader	R2.1	(2.1.22493.0)

* Files:
** DEWETRON_Oxygen_Setup_R2.1_x64.exe
** DEWETRON_DMDReader_R2.1.zip

* Requirements:
** OS: Windows 7 64bit
** CPU: Intel i5 3rd gen. or better
** RAM: 8 GB
** DAQ Hardware:
    * DEWETRON TRION (DEWETRON TRION 2.3.22662.00)
    * DEWETRON ORION DAQ (Orion DAQ Drivers V2.0.0.9)

* Installation procedure:
***TRION:
** Uninstall previous Oxygen version
** Uninstall any previous TRION version via system uninstall (control panel).
** Reboot system
** Install TRION applications
** Reboot system
** Start Dewe2Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
** Power-cycle TRION boards (Power down system, then restart)
** Install Oxygen
** Verify HW settings in system menu on first startup

* New Features Oxygen:
** TRIONet HW support
** TRION-CAN HW support
** CNT input, Frequency measurement mode (used for RPM)
** TRION 100Hz sampling rate
** Strain gage setup (incl. Bridge scaling mode)

* HW Support:
***TRION - all supported modules	(Supported Measurement mode)
** TRION-1620-ACC-6-BNC			(Voltage, SW Current, IEPE, Simple CNT)
** TRION-1620-LV-6-BNC			(Voltage, SW Current)
** TRION-1620-LV-6-L1B			(Voltage, Current)
** TRION-1603-LV-6-BNC			(Voltage, SW Current)
** TRION-1603-LV-6-L1B			(Voltage, SW Current)
** TRION-2402-MULTI-4-D			(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE, CAN)
** TRION-2402-MULTI-8-L0B		(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE, CAN)
** TRION-2402-dSTG-6-L1B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-D			(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-L0B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-RJ			(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2400-dSTG-8-L0B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dACC-6-BNC		(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-dACC-8-SMB		(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-dACC-8-MD			(Voltage, SW Current, IEPE, Simple CNT, Frequency)
** TRION-2402-V-4-B			(Voltage, SW Current)
** TRION-2402-V-8-B			(Voltage, SW Current)
** TRION-CNT-6-L1B			(Simple CNT, Frequency)
** TRION-BASE				(IRIG B DC synchronization, Simple CNT)
** TRION-TIMING				(IRIG A AC or DC, IRIG B AC or DC, GPS time synchronization)
** TRION-VGPS-x				(GPS time synchronization)
** TRION-CAN-4				(CAN)
** TRION-CAN-2				(CAN)
!CAN not available on TrendCorder enclosures!

***EPAD - all supported modules		(Supported Measurement mode)
** EPAD2-TH8-x                     	(Temperature, Voltage)
** EPAD2-TH8-UNIVERSAL                  (Temperature, Voltage)
** EPAD2-V8                             (Voltage)
** EPAD2-RTD8                           (Temperature, Resistance)
** EPAD2-TH8-P				(Temperature, Voltage)
** EPAD2-LA8				(Current)
** EPAD-V8				(Voltage)
** EPAD-TH8-P-x				(Temperature)

***ORION - all supported boards		(Supported Input type)
** ORION DAQ Series (16 bit):
** ORION-0816-10M(%)			(Analog in)
** ORION-0816-5M (%)			(Analog in)
** ORION-0816-1000			(Analog in)
** ORION-0816-500			(Analog in)
** ORION-1616-10x			(Analog in)
** ORION-3216-10x			(Analog in)
(%)data storing speed depends on hardware configuration

***HSI/DAQP - all supported modules	(Supported Measurement mode)
** HSI-HV				(Voltage, SW Current)
** HSI-LV				(Voltage, SW Current)
** DAQP-HV				(Voltage, SW Current)
** DAQP-LV				(Voltage, SW Current)
!All other modules not tested!

* Known Limitations, general:
** Slow data is used as an export option and can only be viewed in recorder instruments
** TRION-MULTI MSI not supported
** dejaVIEW may experience degrading performance on long slow async data recordings
** DMD recovery may lead to non perfect results, depending on filesize, sampling rate, no. of channels and channel type
** Only a reduced number of triggers is shown in recorder instruments
** PCI bus overload may lead to Oxygen fault

* Known Limitations, TRION:
** TRIONet may not be used together with a local TRION system (e.g DEWE2-A4 + TRIONet)

* Known Limitations, ORION:
** ORION-onboard RS485 communication only supported for one board
** ORION-CAN not supported
** ORION-CNT not supported
** ORION-DI not supported
** DAQ AD-boards: only 5V AI range available (AIRef set to Sense)
** Total number of DAQP/HSI modules limited to 16


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
Release Notice DEWETRON Oxygen / TrendCorder Oxygen Software Bundle R2.0.2 x64

* Components:
** DEWETRON Oxygen			R2.0.2	(2.0.2.19128)
** DEWETRON TRION Software 		R2.2.1	(2.2.17086.00)

* Files:
** DEWETRON_Oxygen_Setup_R2.0.2_x64.exe
** DEWETRON_TRION_Applications_R2.2.1_x64.exe

* Fixes:
** External time synchronization (IRIG, GPS)
** TRION 24bit modules, 16bit mode
** Minor issues


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
Release Notice DEWETRON Oxygen / TrendCorder Oxygen Software Bundle R2.0 x64

* Components:
** DEWETRON Oxygen			R2.0	(2.0.0.17715)
** DEWETRON TRION Software 		R2.2.1	(2.2.17086.00)

* Files:
** DEWETRON_Oxygen_Setup_R2.0_x64.exe
** DEWETRON_TRION_Applications_R2.2.1_x64.exe

* HW Requirements:
** OS: Windows 7 64bit
** CPU: Intel i5 3rd gen. or better
** RAM: 8 GB
** DAQ: DEWETRON TRION or ORION DAQ measurement hardware

* Installation procedure:
** Uninstall previous Oxygen version
** Uninstall any previous TRION version via system uninstall (control panel).
** Reboot system
** Install TRION applications
** Reboot system
** Start Dewe2Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
** Power-cycle TRION boards (Power down system, then restart)
** Install Oxygen
** Verify HW settings in system menu on first startup

* New Features Oxygen:
** DMD 2.0 data file format (no backwards compatibility!)
** Software Current mode
** Math formula online calculation
** ORION DAQ A/D board support (08xx, 16xx series)
** HSI/DAQP modules signal conditioning support
** User interface optimizations for desktop/mouse operation

* New Features TRION:
** TRION Module IIR-Filter: lower cut-off frequency changed from 10Hz to 1Hz, exception: TRION-1620-LV/ACC

***TRION - all supported modules	(Supported Measurement mode)
** TRION-1620-ACC-6-BNC			(Voltage, SW Current, IEPE, Simple CNT)
** TRION-1620-LV-6-BNC			(Voltage, SW Current)
** TRION-1620-LV-6-L1B			(Voltage, Current)
** TRION-1603-LV-6-BNC			(Voltage, SW Current)
** TRION-1603-LV-6-L1B			(Voltage, SW Current)
** TRION-2402-MULTI-4-D			(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE)
** TRION-2402-MULTI-8-L0B		(Voltage, SW Current, Resistance, Bridge, Temperature, Potentiometer, IEPE)
** TRION-2402-dSTG-6-L1B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-D			(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-L0B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-RJ			(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2400-dSTG-8-L0B		(Voltage, SW Current, Resistance, IEPE, Bridge)
** TRION-2402-dACC-6-BNC		(Voltage, SW Current, IEPE, Simple CNT)
** TRION-2402-dACC-8-SMB		(Voltage, SW Current, IEPE, Simple CNT)
** TRION-2402-dACC-8-MD			(Voltage, SW Current, IEPE, Simple CNT)
** TRION-2402-V-4-B			(Voltage, SW Current)
** TRION-2402-V-8-B			(Voltage, SW Current)
** TRION-CNT-6-L1B			(Simple CNT)
** TRION-BASE				(IRIG B DC synchronization, Simple CNT)
** TRION-TIMING				(IRIG A AC or DC, IRIG B AC or DC, GPS time synchronization)
** TRION-VGPS-x				(GPS time synchronization)

***EPAD - all supported modules		(Supported Measurement mode)
** EPAD2-TH8-x                     	(Temperature, Voltage)
** EPAD2-TH8-UNIVERSAL                  (Temperature, VOltage)
** EPAD2-V8                             (Voltage)
** EPAD2-RTD8                           (Temperature, Resistance)
** EPAD2-TH8-P				(Temperature, Voltage)
** EPAD2-LA8				(Current)
** EPAD-V8				(Voltage)
** EPAD-TH8-P-x				(Temperature)

***ORION - all supported boards		(Supported Input type)
** ORION-0816-10M(%)			(Analog in)
** ORION-0816-5M (%)			(Analog in)
** ORION-0816-1000			(Analog in)
** ORION-0816-500			(Analog in)
** ORION-1616-10x			(Analog in)
** ORION-3216-10x			(Analog in)
(%)data storing speed depends on hardware configuration

***HSI/DAQP - all supported modules	(Supported Measurement mode)
** HSI-HV				(Voltage, SW Current)
** HSI-LV				(Voltage, SW Current)
** DAQP-HV				(Voltage, SW Current)
** DAQP-LV				(Voltage, SW Current)
** all other modules not tested!

* Known Limitations Oxygen:
** Slow data is used as an export option and can only be viewed in recorder instruments
** TRION-MULTI MSI not supported
** dejaVIEW may experience degrading performance on long slow async data recordings
** DMD recovery may lead to non perfect results, depending on filesize, sampling rate, no. of channels and channel type
** Only a reduced number of triggers is shown in recorder instruments
** PCI bus overload may lead to Oxygen fault
** Async channels only show actual (ACT) values

* Known Limitations TRION:
** Previous TRION versions must be uninstalled via system uninstall (control panel) prior to installing new version
** System reboot required after driver installation
** All TRION board firmware must be updated to latest version
** Please refer to DEWETRON TRION Release Notice for further details

* Known Limitations ORION/DAQP:
** ORION-onboard RS485 communication only supported for one board
** ORION-CAN not supported
** ORION-CNT not supported
** ORION-DI not supported
** DAQ AD-boards: only 5V AI range available (AIRef set to Sense)
** Number of DAQP/HSI modules limited to 16


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
Release Notice DEWETRON TrendCorder Oxygen Software Bundle R1.2.3 x64

* Components:
** DEWETRON Oxygen			1.2.3.16106
** Bundled TRION Driver/API package	2.2.15013.0 (TrendCorder ONLY)

* Files:
** DEWETRON_Oxygen_Setup_R1.2.3_x64.exe
** DEWETRON_TRION_Applications_R2.2_x64.exe

* HW Requirements:
** TrendCorder hardware
** Windows 7 64bit OS

* Installation procedure:
** Uninstall Oxygen
** Uninstall any previous TRION version via system uninstall (control panel).
** Reboot system
** Install TRION bundle
** Reboot system
** Start Dewe2Explorer and update all TRION board firmware to latest version (right-click enclosure name)
** Power-cycle TRION boards (Power down system, then restart)
** Install Oxygen

* New Features Oxygen:
-

* New Features TRION:
-

* All supported TRION Modules		(Supported Measurement mode)
** TRION-1620-ACC-6-BNC			(Voltage, IEPE, Simple CNT)
** TRION-1620-LV-6-BNC			(Voltage, Current)
** TRION-1620-LV-6-L1B			(Voltage, Current)
** TRION-1603-LV-6-BNC			(Voltage, Current)
** TRION-1603-LV-6-L1B			(Voltage, Current)
** TRION-2402-MULTI-4-D			(Voltage, Resistance, Bridge, Temperature, Potentiometer, IEPE)
** TRION-2402-MULTI-8-L0B		(Voltage, Resistance, Bridge, Temperature, Potentiometer, IEPE)
** TRION-2402-dSTG-6-L1B		(Voltage, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-D			(Voltage, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-L0B		(Voltage, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-RJ			(Voltage, Resistance, IEPE, Bridge)
** TRION-2402-dACC-6-BNC		(Voltage, IEPE, Simple CNT)
** TRION-2402-dACC-8-SMB		(Voltage, IEPE, Simple CNT)
** TRION-2402-dACC-8-MD			(Voltage, IEPE, Simple CNT)
** TRION-2402-V-4-B			(Voltage)
** TRION-2402-V-8-B			(Voltage)
** TRION-BASE				(IRIG B DC synchronization, Simple CNT)
** TRION-TIMING				(IRIG A AC or DC, IRIG B AC or DC, GPS time synchronization)
** TRION-VGPS-x				(GPS time synchronization)
** TRION-CNT-6-L1B			(Simple CNT)

* All supported EPAD Modules		(Supported Measurement mode)
** EPAD2-TH8-x                     	(Temperature, Voltage)
** EPAD2-TH8-UNIVERSAL                  (Temperature, VOltage)
** EPAD2-V8                             (Voltage)
** EPAD2-RTD8                           (Temperature)
** EPAD2-TH8-P				(Temperature, Voltage)		(new)
** EPAD2-LA8				(Current)
** EPAD-V8				(Voltage)			(new)
** EPAD-TH8-P-x				(Temperature)			(new)

* Known Limitations Oxygen:
** Simulated TRION-CAN module may cause problems in Oxygen
** Some minor display issues in ch list and ch details, concerning excitation value in new modes (Current, resistance)
** dejaVIEW may experience degrading performance on long slow async data recordings
** DMD recovery may lead to non perfect results, depending on filesize, sampling rate, no. of channels and channel type
** Only a reduced number of triggers is shown in recorder instruments
** PCI bus overload may lead to Oxygen fault
** Async channels only show actual (ACT) values

* Known Limitations TRION Bundle:
** Previous TRION versions must be uninstalled via system uninstall (control panel) prior to installing new version
** System reboot required after driver installation
** All TRION board firmware must be updated to latest version


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
Release Notice DEWETRON TrendCorder Oxygen Software Bundle R1.2.2 x64

* Components:
** DEWETRON Oxygen			1.2.2.15945
** Bundled TRION Driver/API package	2.2.15013.0 (TrendCorder ONLY)

* Files:
** DEWETRON_Oxygen_Setup_R1.2.2_x64.exe
** DEWETRON_TRION_Applications_R2.2_x64.exe

* HW Requirements:
** TrendCorder hardware
** Windows 7 64bit OS

* Installation procedure:
** Uninstall Oxygen
** Uninstall any previous TRION version via system uninstall (control panel).
** Reboot system
** Install TRION bundle
** Reboot system
** Start Dewe2Explorer and update all TRION board firmware to latest version (right-click enclosure name)
** Power-cycle TRION boards (Power down system, then restart)
** Install Oxygen

* New Features Oxygen:
-

* Additionally supported Modules	(Supported Measurement mode):
** EPAD2-LA8				(Current)

* New Features TRION:
-

* Known Limitations Oxygen:
** Simulated TRION-CAN module may cause problems in Oxygen
** Some minor display issues in ch list and ch details, concerning excitation value in new modes (Current, resistance)
** dejaVIEW may experience degrading performance on long slow async data recordings
** DMD recovery may lead to non perfect results, depending on filesize, sampling rate, no. of channels and channel type
** Only a reduced number of triggers is shown in recorder instruments
** PCI bus overload may lead to Oxygen fault
** Async channels only show actual (ACT) values

* Known Limitations TRION Bundle:
** Previous TRION versions must be uninstalled via system uninstall (control panel) prior to installing new version
** System reboot required after driver installation
** All TRION board firmware must be updated to latest version


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
Release Notice DEWETRON TrendCorder Oxygen Software Bundle R1.2.1 x64

* Components:
** DEWETRON Oxygen			1.2.1.15853
** Bundled TRION Driver/API package	2.2.15013.0 (TrendCorder ONLY)

* Files:
** DEWETRON_Oxygen_Setup_R1.2.1_x64.exe
** DEWETRON_TRION_Applications_R2.2_x64.exe

* HW Requirements:
** TrendCorder hardware
** Windows 7 64bit OS

* Installation procedure:
** Uninstall Oxygen
** Uninstall any previous TRION version via system uninstall (control panel).
** Reboot system
** Install TRION bundle
** Reboot system
** Start Dewe2Explorer and update all TRION board firmware to latest version (right-click enclosure name)
** Power-cycle TRION boards (Power down system, then restart)
** Install Oxygen

* New Features Oxygen:
** CSV slow data export (statistical data)
** GPS time synchronization (TRION-TIMING or TRION-VGPS module required in star slot)

* Additionally supported Modules	(Supported Measurement mode):
** TRION-TIMING				(IRIG A AC or DC, IRIG B AC or DC, GPS time synchronization)
** TRION-VGPS-x				(GPS time synchronization)

* New Features TRION:
-

* Known Limitations Oxygen:
** Simulated TRION-CAN module may cause problems in Oxygen
** Some minor display issues in ch list and ch details, concerning excitation value in new modes (Current, resistance)
** dejaVIEW may experience degrading performance on long slow async data recordings
** DMD recovery may lead to non perfect results, depending on filesize, sampling rate, no. of channels and channel type
** Only a reduced number of triggers is shown in recorder instruments
** PCI bus overload may lead to Oxygen fault
** Async channels only show actual (ACT) values

* Known Limitations TRION Bundle:
** Previous TRION versions must be uninstalled via system uninstall (control panel) prior to installing new version
** System reboot required after driver installation
** All TRION board firmware must be updated to latest version


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
Release Notice DEWETRON TrendCorder Oxygen Software Bundle R1.2 x64

* Components:
** DEWETRON Oxygen			1.2.0.15131
** Bundled TRION Driver/API package	2.2.15013.0 (TrendCorder ONLY)

* Files:
** DEWETRON_Oxygen_Setup_R1.2_x64.exe
** DEWETRON_TRION_Applications_R2.2_x64.exe

* HW Requirements:
** TrendCorder hardware
** Windows 7 64bit OS

* Installation procedure:
** Uninstall Oxygen
** Uninstall any previous TRION version via system uninstall (control panel).
** Reboot system
** Install TRION bundle
** Reboot system
** Start Dewe2Explorer and update all TRION board firmware to latest version (right-click enclosure name)
** Power-cycle TRION boards (Power down system, then restart)
** Install Oxygen

* New Features Oxygen:
** IRIG time synchronization (TRION-BASE or TRION-TIMING module required in star slot)
** Absolute time display:
    - System status (lower left corner)
    - Recorder instruments
    - Cursor measurement
    - CSV Export
** Editable Header fields in System Settings sidebar

* Additionally supported Modules	(Supported Measurement mode):
** TRION-2402-MULTI-4-D			(Voltage, Resistance, Bridge, Temperature, Potentiometer, IEPE)
** TRION-2402-MULTI-8-L0B		(Voltage, Resistance, Bridge, Temperature, Potentiometer, IEPE)
** TRION-1603-LV-6-L1B			(Voltage, Current)
** TRION-1620-LV-6-L1B			(Voltage, Current)
** TRION-2402-dSTG-6-L1B		(Voltage, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-D			(Voltage, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-L0B		(Voltage, Resistance, IEPE, Bridge)
** TRION-2402-dSTG-8-RJ			(Voltage, Resistance, IEPE, Bridge)
** TRION-BASE				(IRIG B DC synchronization, Simple CNT)
** TRION-TIMING				(IRIG A AC or DC, IRIG B AC or DC synchronization)

* New Features TRION:
** TRION-2402-MULTI-xx support
** TRION-16xx-xx-L1B support

* Known Limitations Oxygen:
** Simulated TRION-CAN module may cause problems in Oxygen
** Some minor display issues in ch list and ch details, concerning excitation value in new modes (Current, resistance)
** dejaVIEW may experience degrading performance on long slow async data recordings
** DMD recovery may lead to non perfect results, depending on filesize, sampling rate, no. of channels and channel type
** Only a reduced number of triggers is shown in recorder instruments
** PCI bus overload may lead to Oxygen fault
** Async channels only show actual (ACT) values

* Known Limitations TRION Bundle:
** Previous TRION versions must be uninstalled via system uninstall (control panel) prior to installing new version
** System reboot required after driver installation
** All TRION board firmware must be updated to latest version


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
Release Notice DEWETRON TrendCorder Oxygen Software Bundle R1.1 x64

* Components:
** DEWETRON Oxygen			1.1.0.12703
** Bundled TRION Driver/API package	2.1.12689.0 (TrendCorder ONLY)

* Files:
** DEWETRON_Oxygen_Setup_R1.1_x64.exe
** DEWETRON_TRION_Applications_R2.1.1_x64.exe

* HW Requirements:
** TrendCorder hardware
** Windows 7 64bit OS

* Installation procedure:
** Uninstall Oxygen
** Uninstall any previous TRION version via system uninstall (control panel).
** Reboot system
** Install TRION R2.1.1 bundle
** Reboot system
** Start Dewe2Explorer and update all TRION board firmware to latest version (right-click enclosure name)
** Power-cycle TRION boards (Power down system, then restart)
** Install Oxygen R1.1

* New Features Oxygen:
** New storing modes:
    - Continuous Slow
    - Triggered Slow/Fast
** Additional Trigger types:
    - Hysteresis
    - Window
** EPAD address assignment within Oxygen

* Additionally supported Modules	(Supported Measurement mode):
** EPAD2-V8				(Voltage)
** EPAD2-RTD8				(Temperature)

* New Features TRION:
** TRION-2402-V board now has onboard IIR LP filter capability

* Known Limitations Oxygen:
** Slow data for async (EPAD) channels is not calculated at the moment, therefore storing modes �Continuous slow� and �Triggered Slow/Fast� only contain data for TRION channels, async (EPAD) is empty.
** dejaVIEW may experience degrading performance on long slow async data recordings
** DMD recovery may lead to non perfect results, depending on filesize, sampling rate, no. of channels and channel type
** Start of multiple software instances not prevented, may cause errors
** Only a reduced number of triggers is shown in recorder instruments
** PCI bus overload may lead to Oxygen fault
** Async channels only show actual (ACT) values

* Known Limitations TRION Bundle:
** Previous TRION versions must be uninstalled via system uninstall (control panel) prior to installing new version
** System reboot required after driver installation
** All TRION board firmware must be updated to latest version
** Limited self test functionality in DEWE2Explorer (unreliable test results)


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
Release Notice DEWETRON Oxygen Software R1.0.1 x64

* Components:
** DEWETRON Oxygen			1.0.1.10651
** Bundled TRION Driver/API package	2.0.1 (TrendCorder)  {9C37FEAF-2B33-424F-AFFF-272F96747A60}

* Files:
** DEWETRON Oxygen Setup R1.0.1-x64.exe
** DEWETRON-TRION-Setup-x64_2.0.1.msi

* Requirements:
** TrendCorder hardware
** Windows 7 64bit OS

* New Features Oxygen:
** Additional Trigger functionality:
    - Pre-Trigger up to 10s
    - Stop recording after certain time

*Fixes TRION:
** Optimized HW setup communication, increased stability in multi-board system

* Known Limitations Oxygen:
** Start of multiple software instances not prevented, may cause errors
** Fileopen problem with many marker events (~5000)
** Cursor Measurement: on rare occasions A/B cursors cannot be moved any more
** EPAD scan may sometimes abort after 1s
** PCI bus overload may lead to Oxygen fault
** Async channels only show actual (ACT) values
** EPAD address assignment is not supported

* Known Limitations TRION Bundle:
** System reboot required after driver installation
** Only TrendCorder chassis supported (BridgeFilter driver not included)
** Dewe2Explorer not included
** No TRION async data (CAN) support


+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
Release Notice DEWETRON Oxygen Software R1.0 x64

* Components:
** DEWETRON Oxygen			1.0.0.9667
** Bundled TRION Driver/API package	2.0 (TrendCorder)	{a6c3834fb70eca576d2b45a303511a4eea5ea8bb}

* Files:
** DEWETRON Oxygen Setup R1.0-x64.exe
** DEWETRON-TRION-Setup-x64.msi

* Requirements:
** TrendCorder hardware
** Windows 7 64bit OS

* Supported Modules 		(Supported Measurement mode):
** TRION-1603-LV.6.BN 		(Voltage)
** TRION-1620-LV.6.BN 		(Voltage)
** TRION-1620-ACC.6.BN		(Voltage, IEPE, Simple CNT)
** TRION-2402-dACC.6.BN		(Voltage, IEPE, Simple CNT)
** TRION-2402-dACC.8A.MD	(Voltage, IEPE, Simple CNT)
** TRION-2402-dACC.8A.SB	(Voltage, IEPE, Simple CNT)
** TRION-2402-dSTG.4.DB		(Voltage, IEPE, Bridge)
** TRION-2402-dSTG.6.LE		(Voltage, IEPE, Bridge)
** TRION-2402-dSTG.8.DB		(Voltage, IEPE, Bridge)
** TRION-2402-dSTG.8.RJ		(Voltage, IEPE, Bridge)
** TRION-2402-dSTG.8A.LE	(Voltage, IEPE, Bridge)
** TRION-2402-V.4.BA		(Voltage)
** TRION-2402-V.8.BA		(Voltage)
** EPAD2-TH8-UNIV		(Temperature)
** EPAD2-TH8-K			(Temperature)

* Known Limitations Oxygen:
** Start of multiple software instances not prevented, may cause errors
** Fileopen problem with many marker events (~5000)
** Cursor Measurement: on rare occasions A/B cursors cannot be moved any more
** EPAD scan may sometimes abort after 1s
** PCI bus overload may lead to Oxygen fault
** Async channels only show actual (ACT) values
** EPAD address assignment is not supported

* Known Limitations TRION Bundle:
** System reboot required after driver installation
** Only TrendCorder chassis supported (BridgeFilter driver not included)
** Dewe2Explorer not included
** No TRION async data (CAN) support

