+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2021-06-30 Release Notice DEWETRON TRIONet Firmware R5.6.0

* Version: 	5.6.0.58864 (947373dfd06c45bfd05507bfd6cbd8e057d5227f)

* Components:
** TRIONet Firmware                5.6.0

* Files:
** TRIONet remote update:          update-image-trionet-5.6.0.58864.swu
** TRIONet USB stick image:        trionet_update_stick_image_5.6.0.58864.zip

* TRIONet node info:
** OS:                             Yocto warrior-21.0.3
** Server:                         5.6.0.58864
** Firmware:                       4.1.7 (500932eed5a6e2ba78ec0bbd2d3caf1783148de0)
** TRION API:                      5.6.0.58864
** TRION DRV:                      5.6.0.58864

* Requirements:
** All TRIONet devices used with OXYGEN must be updated to the image included in this release

* New Features and most important bugfixes:
  - TRION-AO Digital-Out-channels are now labled "DO" in Oxygen channellist (Oxy + API)
  - Dewetron Explorer: failed SRAM-Test during selftests now highlighted in red with correct text
  - Increased reliablity when scanning for TEDS-devices on systems with high data-load
  - TRION-CAN-channels default to "one-shot-mode". So messages that are not acknoledged by any listener will not be retried to be sent autonomously by the transceifer. This is done to decrease latency for CAN-Out and minimizing the risk of message-collisions on bus.
  - Oversampling Configuration Item corrected

* Known Limitations:
** None

* HW Support TRION modules:
** TRION-1620-ACC-6-BNC         FW: x0031
** TRION-1620-ACC-6-L1B         FW: x0031
** TRION-1620-LV-6-BNC          FW: x0031
** TRION-1620-LV-6-L1B          FW: x0031
** TRION-1603-LV-6-BNC          FW: x0A15
** TRION-1603-LV-6-L1B          FW: x0A15
** TRION-1603-LV-6-D25          FW: x0A15
** TRION-1600-dLV-16-D          FW: x1892
** TRION-1600-dLV-16-D-CAN      FW: x1892
** TRION-1600-dLV-32-D          FW: x1892
** TRION-1600-dLV-32-D-CAN      FW: x1892
** TRION-1802-dLV-16-D          FW: x1892
** TRION-1802-dLV-16-D-CAN      FW: x1892
** TRION-1802-dLV-32-D          FW: x1892
** TRION-1802-dLV-32-D-CAN      FW: x1892
** TRION-1810-HV-4              FW: x0063
** TRION-1810-HV-8              FW: x0063
** TRION-1820-POWER-4           FW: x0063
** TRION-1810M-POWER-4          FW: x0063
** TRION-1820-MULTI-4-D         FW: x0029
** TRION-2402-MULTI-4-D         FW: x0B18
** TRION-2402-MULTI-8-L0B       FW: x0A24
** TRION-2402-MULTI-S1          FW: x0034
** TRION-2402-dSTG-6-L1B        FW: x1120
** TRION-2402-dSTG-6-L1B-S1     FW: x1120
** TRION-2402-dSTG-8-D          FW: x1120
** TRION-2402-dSTG-8-L0B        FW: x1120
** TRION-2402-dSTG-8-RJ         FW: x1120
** TRION-2400-dSTG-8-L0B        FW: x1120
** TRION-2400-dSTG-OEM          FW: x1120
** TRION-2402-dACC-6-BNC        FW: x1119
** TRION-2402-dACC-8-SMB        FW: x1119
** TRION-2402-dACC-8-MD         FW: x1119
** TRION-2402-V-4-B             FW: x1017
** TRION-2402-V-8-B             FW: x1017
** TRION-CNT-6-L1B              FW: x1119
** TRION-BASE                   FW: x1145
** TRION-TIMING                 FW: x1145
** TRION-TIMING-V2              FW: x0004
** TRION-TIMING-V3              FW: xF016   MCU: x00020095
** TRION-VGPS-20                FW: x1145
** TRION-VGPS-20-V3             FW: xF016   MCU: x00020095
** TRION-VGPS-100               FW: x1145
** TRION-VGPS-100-V3            FW: xF016   MCU: x00020095
** TRION-CAN-4                  FW: x1122
** TRION-CAN-2                  FW: x1122
** TRION-DI-48                  FW: x1119
** TRION-DI-64-S1               FW: x0009
