+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2021-06-30 Release Notice DEWETRON Oxygen R5.6.0 x64

* Components:
** DEWETRON Oxygen      R5.6.0   (5.6.0.58865)   (4663542f6937dc4e564c56962ca6020fc595c639)

* Files:
** DEWETRON_Oxygen_Setup_R5.6.0_x64.exe
** DEWETRON_DMDReader_R5.6.0.zip

* Requirements:
** 5.x Software License required!
** OS: Windows 10 64bit
** CPU: Intel i5 3rd gen. or better
** RAM: 8 GB
** DAQ Hardware:
    * DEWETRON TRION and TRION3 (DEWETRON TRION Software R5.6.0)
    * DEWETRON ORION DAQ (ORION DAQ Driver V2.3.1.0)
    * DEWETRON ORION DSA (ORION DSA Driver V5.0.1.0)

* Installation procedure:
** TRION:
   - Install TRION applications
   - Reboot system (if requested by the installer)
   - Start DEWETRON Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
   - Power-cycle TRION boards (Power down system, then restart)
   - Start DEWETRON Explorer and check for a successful firmware upgrade
** OXYGEN:
   - Install Oxygen
   - Verify HW settings in system menu on first startup

* New Features Oxygen:
** TEDS Support:
   - Detection of IEEE 1451.4 compatible sensors (selection)
   - Apply of scaling and mode of measurement input
   - Tested and working on TRION(3)-18xx-MULTI, TRION-2402-MULTI and TRION-2402-dACC
** CPAD Decoder Plugin:
   - Native Support of CPAD2/3 Modules
** ARXML support for CAN:
   - Support of ARMXL 4.2 for decoding of CAN Messages
** TRIONet manual claiming:
   - Enable the user to manually select the TRIONet for measurement
   - Use multiple measurements in one Ethernet System
** Header Data as Formula Constant:
   - Use Numeric Header data in Formula
   - Can be adjusted also via SCPI in Testbed Environment
** Enable Voltage and Current Excitation Monitor:
   - Check actual set Voltage and Current Excitation of selected Boards
** BirdsEye adaptions:
   - Kml-track data can be used  as
center, left or right boundary of lane
** Additional Improvements:
   - New Storing Option: Stop measurement after... additional to Pause
   - Increase Pre-Time and Freeze time up to 60 seconds
   - Manual (Recording)-Trigger via GUI or SCPI
   - File Name pattern, user defined counter offset
   - Formula Channels can now be also grouped
   - Navigate thru channel list with CTRL+PAGE UP/DOWN
   - Increased sensitivity of power flicker emission calculation

* Fixes:
   - Update of Graphic Framework to avoid screen flickering on intel graphics
   - CAN-OUT, wrong data @ high speed, new Option "Autonomous Resend" (disabled by default to avoid the issue)
   - Error Message regarding Oversampling @ Setup loading
   - Problem with ACQ-Start with no channel Enabled on first DAQ Board

* Known Limitations:
  - CPAD Baudrate Setting function is limited
