## 2022-05-02 Release Notice DEWETRON Oxygen R6.1.1 x64

### Version: 6.1.1.61822
Revision: 80a07470c3ce5169ceb344dbd3f3e17c0b0185fa

Components                      | Version
--------------------------------|--------------------------
DEWETRON Oxygen                 | 6.1.1.61822

## Requirements
* 6.x Software License required!
* OS: Windows 10 64bit or better
* CPU: Intel i5 3rd gen. or better
* Minimum RAM: 8 GB
* Recommended RAM: 16 GB (for high sample rates and channel counts)
* DAQ Hardware:
  - DEWETRON TRION and TRION3 (DEWETRON TRION Software R6.1.1)
  - DEWETRON ORION DAQ (ORION DAQ Driver V2.3.1.0)
  - DEWETRON ORION DSA (ORION DSA Driver V5.0.1.0)

## Installation procedure
  - TRION:
    - Install TRION applications
    - Reboot system (if requested by the installer)
    - Start DEWETRON Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
    - Power-cycle TRION boards (Power down system, then restart)
    - Start DEWETRON Explorer and check for a successful firmware upgrade
  - OXYGEN:
    - Install Oxygen
    - Verify HW settings in system menu on first startup

## Fixes
  - Fixed wrong white on white rendering with Oxygen classic style
  - Installation using SYSTEM account fixed
  - Snapshot fixed an issue when the set interval was not applied correctly
  - Order Analysis performance improvement
  - Stability
    - Frequency Measurement: Fixed Oxygen crash on >2MS boards
    - Fix crash due to channel without timebase in audio player instrument
    - Fix crash with Stop measurement trigger
    - Fix crash when using spectrum analyzer and multiple file open
    - Fix spurious crash when opening splitted DMD files
    
