## 2022-07-15 Release Notice DEWETRON Oxygen R6.2.1 x64
Revision: 9fc52c1f65b49de1b08c5bdb8e08ac6a98189ae0

Components                      | Version
--------------------------------|--------------------------
DEWETRON Oxygen                 | 6.2.1.62584

## Files
DEWETRON_Oxygen_Setup_R6.2.1_x64.exe
DEWETRON_Oxygen_Setup_R6.2.1_x64_cvss.exe (no Python scripting)

## Requirements
* 6.x Software License required!
* OS: Windows 10 64bit or better
* CPU: Intel i3 3rd gen. or better
* Minimum RAM: 8 GB
* Recommended RAM: 16 GB (for high sample rates and channel counts)
* DAQ Hardware:
  - DEWETRON TRION and TRION3 (DEWETRON TRION Software R6.2.1)
  - DEWETRON ORION DAQ (ORION DAQ Driver V2.3.1.0)
  - DEWETRON ORION DSA (ORION DSA Driver V5.0.1.0)

## Installation procedure
  - TRION:
    - Install TRION applications
    - Reboot system (if requested by the installer)
    - Start DEWETRON Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
    - Power-cycle TRION boards (Power down system, then restart)
    - Start DEWETRON Explorer and check for a successful firmware upgrade
  - OXYGEN:
    - Install Oxygen
    - Verify HW settings in system menu on first startup

## New Features
  - Data Navigation
    - Import CSV files in analysis
    - "Save As" allows to remove channel data from DMD files
  - Advanced Statistics
    - Triggered Statistics - calculate on trigger events
    - Running Statistics - running statistics on given window for sync channels
  - Hardware: XR Series
    - Support for RS485 and CAN Mode
    - Export DBC file in CAN Mode
  - NetCDF Export
    - Network Common Data Form support (NetCDF3, NetCDF4, NetCDF5)
  - CVSS installer without embedded Python

## Improvements
  - Power:
    -  Accumulate current signals for capacity computation
  - User Experience
    - Added error list
    - "Selection" header type support
    - Recorder allows up to 40 channels
    - Multi select instruments to edit properties
    - Hardware mismatch dialog can be forced
  - XY Chart
    - Multiple traces with shared X-Y axis
  - DMD Reader
    - Added functions to read measurement setup (xml)
  - FFT
    - Added FFT Averaging
  - Enum Scaling
    - Available for formular channels
  - Exports
    - Added align to trigger

## Fixes
  - Fixed memory leak in split file video recording with h.264 on Intel hardware
  - Memory consumption reduced for long-time recordings
  - Power: flicker emission is computed more accurately
  - TEDS: Fixed issue with accelerometer sensor
  - Frequency measurement: Fixed crash with high sample rates (>2MS)
  - ARXML: Fixed issue showing channels as other channels
  - Excel Export: 
    - Fixed missing reduced samples
    - Fixed user reduced channel names in
  - CVS Import: Fixed handling of unicode paths



## 2022-07-04 Release Notice DEWETRON Oxygen R6.2.0 x64
Revision: 4e948c29615a94058afbc48c41609269f3b45105

Components                      | Version
--------------------------------|--------------------------
DEWETRON Oxygen                 | 6.2.0.62422

## Files
DEWETRON_Oxygen_Setup_R6.2.0_x64.exe
DEWETRON_Oxygen_Setup_R6.2.0_x64_cvss.exe

## Requirements
* 6.x Software License required!
* OS: Windows 10 64bit or better
* CPU: Intel i3 3rd gen. or better
* Minimum RAM: 8 GB
* Recommended RAM: 16 GB (for high sample rates and channel counts)
* DAQ Hardware:
  - DEWETRON TRION and TRION3 (DEWETRON TRION Software R6.2.0)
  - DEWETRON ORION DAQ (ORION DAQ Driver V2.3.1.0)
  - DEWETRON ORION DSA (ORION DSA Driver V5.0.1.0)

## Installation procedure
  - TRION:
    - Install TRION applications
    - Reboot system (if requested by the installer)
    - Start DEWETRON Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
    - Power-cycle TRION boards (Power down system, then restart)
    - Start DEWETRON Explorer and check for a successful firmware upgrade
  - OXYGEN:
    - Install Oxygen
    - Verify HW settings in system menu on first startup

## New Features
  - Data Navigation
    - Import CSV files in analysis
    - "Save As" allows to remove channel data from DMD files
  - Advanced Statistics
    - Triggered Statistics - calculate on trigger events
    - Running Statistics - running statistics on given window for sync channels
  - Hardware: XR Series
    - Support for RS485 and CAN Mode
    - Export DBC file in CAN Mode
  - NetCDF Export
    - Network Common Data Form support (NetCDF3, NetCDF4, NetCDF5)
  - CVSS installer without embedded Python

## Improvements
  - Power:
    -  Accumulate current signals for capacity computation
  - User Experience
    - Added error list
    - "Selection" header type support
    - Recorder allows up to 40 channels
    - Multi select instruments to edit properties
    - Hardware mismatch dialog can be forced
  - XY Chart
    - Multiple traces with shared X-Y axis
  - DMD Reader
    - Added functions to read measurement setup (xml)
  - FFT
    - Added FFT Averaging
  - Enum Scaling
    - Available for formular channels
  - Exports
    - Added align to trigger

## Fixes
  - Fixed memory leak in split file video recording with h.264 on Intel hardware
  - Memory consumption reduced for long-time recordings
  - Power: flicker emission is computed more accurately
  - TEDS: Fixed issue with accelerometer sensor
  - Frequency measurement: Fixed crash with high sample rates (>2MS)
  - ARXML: Fixed issue showing channels as other channels
  - Export: Fixed reduces sample missing in EXCEL export



## 2022-05-02 Release Notice DEWETRON Oxygen R6.1.1 x64

### Version: 6.1.1.61822
Revision: 80a07470c3ce5169ceb344dbd3f3e17c0b0185fa

Components                      | Version
--------------------------------|--------------------------
DEWETRON Oxygen                 | 6.1.1.61822

## Files
DEWETRON_Oxygen_Setup_R6.1.1_x64.exe

## Requirements
* 6.x Software License required!
* OS: Windows 10 64bit or better
* CPU: Intel i5 3rd gen. or better
* Minimum RAM: 8 GB
* Recommended RAM: 16 GB (for high sample rates and channel counts)
* DAQ Hardware:
  - DEWETRON TRION and TRION3 (DEWETRON TRION Software R6.1.1)
  - DEWETRON ORION DAQ (ORION DAQ Driver V2.3.1.0)
  - DEWETRON ORION DSA (ORION DSA Driver V5.0.1.0)

## Installation procedure
  - TRION:
    - Install TRION applications
    - Reboot system (if requested by the installer)
    - Start DEWETRON Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
    - Power-cycle TRION boards (Power down system, then restart)
    - Start DEWETRON Explorer and check for a successful firmware upgrade
  - OXYGEN:
    - Install Oxygen
    - Verify HW settings in system menu on first startup

## Fixes
  - Fixed wrong white on white rendering with Oxygen classic style
  - Installation using SYSTEM account fixed
  - Snapshot fixed an issue when the set interval was not applied correctly
  - Order Analysis performance improvement
  - Stability
    - Frequency Measurement: Fixed Oxygen crash on >2MS boards
    - Fix crash due to channel without timebase in audio player instrument
    - Fix crash with Stop measurement trigger
    - Fix crash when using spectrum analyzer and multiple file open
    - Fix spurious crash when opening splitted DMD files
    
