+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2025-04-02 Release Notice dewetron_gmbh_lib_dewetron_drivers-0.0.0.23.zip

* Files:
** dewetron_gmbh_lib_dewetron_drivers-0.0.0.23.zip

* Version: 0.0.0.23

* Requirements:
** Windows 10 64-Bit or Windows 11 64-Bit
** NI LabVIEW 2018 or higher (32 bit and 64 bit)
** DEWETRON-TRION-Applications-7.4.2.7598 or higher

* Installation procedure
** Can be installed by using LabVIEW Package Manager

* Description
** Native LabVIEW driver for TRION & TRION3 modules
** Documentation included in the source code
** Dedicated functions included in separate VIs for hardware configuration
** Programming examples for different use cases included
** Supports TRION & TRION3 modules in DEWE2 (incl. TRIONet(3)) & DEWE3 chassis
** Supports one or several NEX[DAQ] connected via USB or Ethernet
** Synchronization via internal DEWE2/DEWE3 chassis clock
** Synchronization of several DEWE2/DEWE3 (CC-V1 & CC-V2) chassis via TRION Sync I/O
** Synchronization of several NEXD[DAQ] via PTP
** Supported Channel types:
*** Analog inputs (AI)
*** Analog outputs (AO)
*** Digital inputs (DI)
*** Digital outputs (DO)
*** Counter inputs (CNT)
*** CAN message receive
*** CAN message decode (for LabVIEW 32 bit)
*** Recognition of MSIs & SUB modules

* Known Limitations
** External Synchronization signals not supported
** Maximum tested data rate: 200 MB/s (corresponds to 48 AI á 1 MS/s á 24 bit)
** NEX[DAQ] limitation in daisy-chain wiring: 100 MB/s max. data rate
** CAN-FD on NEX[DAQ]
** CAN message decode (for LabVIEW 64 bit due to missing LabVIEW library)
** CAN output

* Changes from v0.0.0.14 to v0.0.0.23
** Support and synchronization of several NEX[DAQ] via PTP
** Bugfixing for MSI support with NEX[DAQ] and TRION(3)-MULTI 

* Changes from v0.0.0.13 to v0.0.0.14
** Synchronization of several DEWE2/DEWE3 (CC-V1 & CC-V2) chassis via TRION Sync I/O added

* Changes from v0.0.0.8 to v0.0.0.13
** New supported channel types:
*** Analog outputs (AO)
*** Digital outputs (DO)
*** CAN message receive
*** CAN message decode (for LabVIEW 32 bit)
** TRIONet supported

* Changes from v0.0.0.7 to v0.0.0.8
** If-1 is entered for ShuntResistance the Parameter won't be set
** The number format has now also been set to a point as a decimal separator for the InputOffset
** Only integer values ​​can now be entered for ShuntResistance

+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2022-10-11 Release Notice dewetron_gmbh_lib_dewetron_drivers-0.0.0.14.zip

* Files:
** dewetron_gmbh_lib_dewetron_drivers-0.0.0.14.zip

* Version: 0.0.0.14

* Requirements:
** Windows 10 64-Bit
** NI LabVIEW 2018 or higher (32 bit and 64 bit)
** DEWETRON-TRION-Applications-6.3.0.63500 or higher

* Installation procedure
** Can be installed by using LabVIEW Package Manager

* Description
** Native LabVIEW driver for TRION & TRION3 modules
** Documentation included in the source code
** Dedicated functions included in separate VIs for hardware configuration
** Programming examples for different use cases included
** Supports TRION & TRION3 modules in DEWE2 (incl. TRIONet(3)) & DEWE3 chassis
** Supports one NEX[DAQ] connected via USB or Ethernet
** Synchronization via internal DEWE2/DEWE3 chassis clock
** Synchronization of several DEWE2/DEWE3 (CC-V1 & CC-V2) chassis via TRION Sync I/O
** Supported Channel types:
*** Analog inputs (AI)
*** Analog outputs (AO)
*** Digital inputs (DI)
*** Digital outputs (DO)
*** Counter inputs (CNT)
*** CAN message receive
*** CAN message decode (for LabVIEW 32 bit)
*** Recognition of MSIs & SUB modules

* Known Limitations
** External Synchronization signals not supported
** More than one NEX[DAQ] synchronized via PTP connected to one PC
** Maximum tested data rate: 200 MB/s (corresponds to 48 AI á 1 MS/s á 24 bit)
** CAN-FD on NEX[DAQ]
** CAN message decode (for LabVIEW 64 bit due to missing LabVIEW library)
** CAN output 

* Changes from v0.0.0.13 to v0.0.0.14
** Synchronization of several DEWE2/DEWE3 (CC-V1 & CC-V2) chassis via TRION Sync I/O added

* Changes from v0.0.0.8 to v0.0.0.13
** New supported channel types:
*** Analog outputs (AO)
*** Digital outputs (DO)
*** CAN message receive
*** CAN message decode (for LabVIEW 32 bit)
** TRIONet supported

* Changes from v0.0.0.7 to v0.0.0.8
** If-1 is entered for ShuntResistance the Parameter won't be set
** The number format has now also been set to a point as a decimal separator for the InputOffset
** Only integer values ​​can now be entered for ShuntResistance

+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2022-10-11 Release Notice dewetron_gmbh_lib_dewetron_drivers-0.0.0.13.zip

* Files:
** dewetron_gmbh_lib_dewetron_drivers-0.0.0.13.zip

* Version: 0.0.0.13

* Requirements:
** Windows 10 64-Bit
** NI LabVIEW 2018 or higher (32 bit and 64 bit)
** DEWETRON-TRION-Applications-6.3.0.63500 or higher

* Installation procedure
** Can be installed by using LabVIEW Package Manager

* Description
** Native LabVIEW driver for TRION & TRION3 modules
** Documentation included in the source code
** Dedicated functions included in separate VIs for hardware configuration
** Programming examples for different use cases included
** Supports TRION & TRION3 modules in DEWE2 (incl. TRIONet(3)) & DEWE3 chassis
** Supports one NEX[DAQ] connected via USB or Ethernet
** Synchronization via internal DEWE2/DEWE3 chassis clock
** Supported Channel types:
*** Analog inputs (AI)
*** Analog outputs (AO)
*** Digital inputs (DI)
*** Digital outputs (DO)
*** Counter inputs (CNT)
*** CAN message receive
*** CAN message decode (for LabVIEW 32 bit)
*** Recognition of MSIs & SUB modules

* Known Limitations
** External Synchronization signals not supported
** Synchronization of several DEWE2/DEWE3 chassis via TRION Sync I/O not supported
** More than one NEX[DAQ] synchronized via PTP connected to one PC
** Maximum tested data rate: 200 MB/s (corresponds to 48 AI á 1 MS/s á 24 bit)
** CAN-FD on NEX[DAQ]
** CAN message decode (for LabVIEW 64 bit due to missing LabVIEW library)
** CAN output 

* Changes from v0.0.0.8 to v0.0.0.13
** New supported channel types:
*** Analog outputs (AO)
*** Digital outputs (DO)
*** CAN message receive
*** CAN message decode (for LabVIEW 32 bit)
** TRIONet supported

* Changes from v0.0.0.7 to v0.0.0.8
** If-1 is entered for ShuntResistance the Parameter won't be set
** The number format has now also been set to a point as a decimal separator for the InputOffset
** Only integer values ​​can now be entered for ShuntResistance

+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2022-07-15 Release Notice dewetron_gmbh_lib_dewetron_drivers-0.0.0.8.zip

* Files:
** dewetron_gmbh_lib_dewetron_drivers-0.0.0.8.zip

* Version: 0.0.0.8

* Requirements:
** Windows 10 64-Bit
** NI LabVIEW 2018 or higher (32 bit and 64 bit)
** DEWETRON-TRION-Applications-6.2.0.62422 or higher

* Installation procedure
** Can be installed by using LabVIEW Package Manager

* Description
** Native LabVIEW driver for TRION & TRION3 modules
** Supports TRION & TRION3 modules in DEWE2 & DEWE3 chassis
** Synchronization via internal DEWE2/DEWE3 chassis clock
** Supported Channel types:
*** Analog inputs (AI)
*** Digital Inputs (DI)
*** Counter Inputs (CNT)

* Changes from v0.0.0.7 to 0.0.0.8
** If-1 is entered for ShuntResistance the Parameter won't be set
** The number format has now also been set to a point as a decimal separator for the InputOffset
** Only integer values ​​can now be entered for ShuntResistance

* Known Limitations
** TRIONet not supported
** External Synchronization signals not supported
** Synchronization of several DEWE2/DEWE3 chassis via TRION Sync I/O not supported
** MSI adapters not supported
** Maximum tested data rate: 200 MB/s (corresponds to 48 AI á 1 MS/s á 24 bit)
** Unsupported channel types:
*** CAN input and output (CAN)
*** Digital outputs (DO)
*** Analog outputs (AO)

+ + + + + + + + + + + + + + + + + + + + + + + + + + + + + + + +
2022-07-07 Release Notice dewetron_gmbh_lib_dewetron_drivers-0.0.0.7.zip

* Files:
** dewetron_gmbh_lib_dewetron_drivers-0.0.0.7.zip

* Version: 0.0.0.7

* Requirements:
** Windows 10 64-Bit
** NI LabVIEW 2018 or higher (32 bit and 64 bit)
** DEWETRON-TRION-Applications-6.2.0.62422 or higher

* Installation procedure
** Can be installed by using LabVIEW Package Manager

* Description
** Native LabVIEW driver for TRION & TRION3 modules
** Supports TRION & TRION3 modules in DEWE2 & DEWE3 chassis
** Synchronization via internal DEWE2/DEWE3 chassis clock
** Supported Channel types:
*** Analog inputs (AI)
*** Digital Inputs (DI)
*** Counter Inputs (CNT)

* Known Limitations
** TRIONet not supported
** External Synchronization signals not supported
** Synchronization of several DEWE2/DEWE3 chassis via TRION Sync I/O not supported
** MSI adapters not supported
** Maximum tested data rate: 200 MB/s (corresponds to 48 AI á 1 MS/s á 24 bit)
** Unsupported channel types:
*** CAN input and output (CAN)
*** Digital outputs (DO)
*** Analog outputs (AO)



