## 2023-02-28 Release Notice DEWETRON Oxygen R6.4.4 x64

Revision: 1c6c6944dca3e29309727a656c188b97a827993c

Components                      | Version
--------------------------------|--------------------------
DEWETRON Oxygen                 | 6.4.4.64822

## Files
DEWETRON-OXYGEN-Setup-6.4.4.64822-x64.msi
DEWETRON-OXYGEN-Setup-6.4.4.64822-x64-cvss.msi  (without Python Scripting)

## Requirements
* 6.x Software License required!
* OS: Windows 10 64bit or better
* CPU: Intel i3 3rd gen. or better
* Minimum RAM: 8 GB
* Recommended RAM: 16 GB (for high sample rates and channel counts)
* DAQ Hardware:
  - DEWETRON TRION and TRION3 (DEWETRON TRION Software R6.4.0)
  - DEWETRON ORION DAQ (ORION DAQ Driver V2.3.1.0)
  - DEWETRON ORION DSA (ORION DSA Driver V5.0.1.0)

## Installation procedure
  - TRION:
    - Install TRION applications
    - Reboot system (if requested by the installer)
    - Start DEWETRON Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
    - Power-cycle TRION boards (Power down system, then restart)
    - Start DEWETRON Explorer and check for a successful firmware upgrade
  - OXYGEN:
    - Install Oxygen
    - Verify HW settings in system menu on first startup

## Fixes
  - Fixed claiming of TRIONet in combination with Oxygen Net
  - Fixed Oxygen Net nodes will not be recognized automatically when starting a preconfigured setup on the master
  - Fixed crash when editing a DMD file
  - Fixed storing to file paths using german umlauts
  - Fixed trigger condition preview collapsing on sidebar close/open
  - Fixed support for Alvium USB3 cameras with newest firmware



## 2023-01-26 Release Notice DEWETRON Oxygen R6.4.1 x64

Revision: 60fd9dec228f7252a0d6ce5a20dc1764b28797af

Components                      | Version
--------------------------------|--------------------------
DEWETRON Oxygen                 | 6.4.1.64538

## Files
DEWETRON-OXYGEN-Setup-6.4.1.64538-x64.msi
DEWETRON-OXYGEN-Setup-6.4.1.64538-x64-cvss.msi  (without Python Scripting)

## Requirements
* 6.x Software License required!
* OS: Windows 10 64bit or better
* CPU: Intel i3 3rd gen. or better
* Minimum RAM: 8 GB
* Recommended RAM: 16 GB (for high sample rates and channel counts)
* DAQ Hardware:
  - DEWETRON TRION and TRION3 (DEWETRON TRION Software R6.4.0)
  - DEWETRON ORION DAQ (ORION DAQ Driver V2.3.1.0)
  - DEWETRON ORION DSA (ORION DSA Driver V5.0.1.0)

## Installation procedure
  - TRION:
    - Install TRION applications
    - Reboot system (if requested by the installer)
    - Start DEWETRON Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
    - Power-cycle TRION boards (Power down system, then restart)
    - Start DEWETRON Explorer and check for a successful firmware upgrade
  - OXYGEN:
    - Install Oxygen
    - Verify HW settings in system menu on first startup

## Improvements
  - XCP - Arm Measurement option
  - Vimba/GigE Camera Support for Linux

## Fixes
  - Prevent crash on recording stop
  - Fixed cancel in channel selection dialog
  - Fixed calculation of time trigger
  


## 2023-01-17 Release Notice DEWETRON Oxygen R6.4.0 x64

Revision: e22640774517d238e72900e3d9bab85e21f7795c

Components                      | Version
--------------------------------|--------------------------
DEWETRON Oxygen                 | 6.4.0.64419

## Files
DEWETRON-OXYGEN-Setup-6.4.0.64419-x64.msi
DEWETRON-OXYGEN-Setup-6.4.0.64419-x64-cvss.msi  (without Python Scripting)

## Requirements
* 6.x Software License required!
* OS: Windows 10 64bit or better
* CPU: Intel i3 3rd gen. or better
* Minimum RAM: 8 GB
* Recommended RAM: 16 GB (for high sample rates and channel counts)
* DAQ Hardware:
  - DEWETRON TRION and TRION3 (DEWETRON TRION Software R6.4.0)
  - DEWETRON ORION DAQ (ORION DAQ Driver V2.3.1.0)
  - DEWETRON ORION DSA (ORION DSA Driver V5.0.1.0)

## Installation procedure
  - TRION:
    - Install TRION applications
    - Reboot system (if requested by the installer)
    - Start DEWETRON Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
    - Power-cycle TRION boards (Power down system, then restart)
    - Start DEWETRON Explorer and check for a successful firmware upgrade
  - OXYGEN:
    - Install Oxygen
    - Verify HW settings in system menu on first startup

## New Features
  - Modifications of software channels in dmd files
    - Available for all channels and calculations
    - Batch processing supported
    - Not available for hardware channels
  - Tape Sensor Plugin
    - Calculation of mechanical speed and angle
  - Resolver Plugin
    - Calculation of mechanical speed and angle
    - Supports modulated inputs with excitation, envelope detection by software
    - Supports demodulated inputs with excitation, envelope detection by electronics
  - Sensorless DQ and rotor angle
    - Power Group option in DQ-Analysis
    - Online insight into motor control
    - Angle signal without any rotary sensor

## Improvements
  - Absolute time trigger
    - Absolute start time, trigger interval, deactivate after set time
  - Signal preview
    - For Level High&Low and Window In/Out conditions
  - Saturation display
    - Available in Live and Record mode
    - SCPI support
  - Excitation ON/OFF switch
    - Avoid sensor malfunctions during channel setup
    - SCPI support
  - Output channel instrument
    - SCPI support: Start, Pause, Stop, State
  - Ethernet Receiver
    - IPV6 support
  - Max measurement time in evaluation mode limited to 30 sec


## Fixes


## 2022-10-17 Release Notice DEWETRON Oxygen R6.3.1 x64

Revision: 926695d2f374a71af8643218197c17047849cfbf

Components                      | Version
--------------------------------|--------------------------
DEWETRON Oxygen                 | 6.3.1.63640

## Files
DEWETRON-OXYGEN-Setup-6.3.1.63640-x64.msi
DEWETRON-OXYGEN-Setup-6.3.1.63640-x64-cvss.msi  (without Python Scripting)

## Requirements
* 6.x Software License required!
* OS: Windows 10 64bit or better
* CPU: Intel i3 3rd gen. or better
* Minimum RAM: 8 GB
* Recommended RAM: 16 GB (for high sample rates and channel counts)
* DAQ Hardware:
  - DEWETRON TRION and TRION3 (DEWETRON TRION Software R6.3.0)
  - DEWETRON ORION DAQ (ORION DAQ Driver V2.3.1.0)
  - DEWETRON ORION DSA (ORION DSA Driver V5.0.1.0)

## Installation procedure
  - TRION:
    - Install TRION applications
    - Reboot system (if requested by the installer)
    - Start DEWETRON Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
    - Power-cycle TRION boards (Power down system, then restart)
    - Start DEWETRON Explorer and check for a successful firmware upgrade
  - OXYGEN:
    - Install Oxygen
    - Verify HW settings in system menu on first startup

## Fixes
  - Fix MSI Installer packages missing OpenMP libraries
  - Fix performance issue with OpenMP after installation
  - Fix spelling errors in DE translation
  - Fix FIR showing total delay and compensable delay
  - Fix a crash caused by a missing timebase


## 2022-10-03 Release Notice DEWETRON Oxygen R6.3.0 x64

Revision: 851865410548989002881ef4ff43139e40fdb05e

Components                      | Version
--------------------------------|--------------------------
DEWETRON Oxygen                 | 6.3.0.63502

## Files
DEWETRON-OXYGEN-Setup-6.3.0.63502-x64.msi
DEWETRON-OXYGEN-Setup-6.3.0.63502-x64-cvss.msi  (without Python Scripting)

## Requirements
* 6.x Software License required!
* OS: Windows 10 64bit or better
* CPU: Intel i3 3rd gen. or better
* Minimum RAM: 8 GB
* Recommended RAM: 16 GB (for high sample rates and channel counts)
* DAQ Hardware:
  - DEWETRON TRION and TRION3 (DEWETRON TRION Software R6.3.0)
  - DEWETRON ORION DAQ (ORION DAQ Driver V2.3.1.0)
  - DEWETRON ORION DSA (ORION DSA Driver V5.0.1.0)

## Installation procedure
  - TRION:
    - Install TRION applications
    - Reboot system (if requested by the installer)
    - Start DEWETRON Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
    - Power-cycle TRION boards (Power down system, then restart)
    - Start DEWETRON Explorer and check for a successful firmware upgrade
  - OXYGEN:
    - Install Oxygen
    - Verify HW settings in system menu on first startup

## New Features
  - Multi-stage FIR filter
    - Low pass, High pass, Band pass, Band stop
  - Power
    - Vectorscope improvements: arrow length depending on signal amplitude
    - Configureable number of periods for calculation interval
  - TRION3-AOUT
    - New output channel instrument
      - Constant value, Function generator support
      - Channel replay
  - Sensor delay compensation up to 500ms
  - Export
    - datx export format
    - Usable with DSPCon software package
  - Persistant Recorder Labels
    - Available in REC and PLAY mode
    - Labels can be added by pressing the "Labels" button
  -  FFT
    - Peak hold channel 
    - Enable option in FFT_Cpx channel
  - Feature Promotion
    - Promotion of newly added options and features
    - Get a time 30-day demo license by using QR-code
  - Device Support
    - DEWE3-A4L
    - Ethernet-Frontends based on DEWE3-RMx and DEWE3-M4

## Improvements
  - Usability
    - Customizable Favorites in Add Channel
  - IIR filter
    - Frequency response preview in channel setup
  - CAN
    - dbc file export for CAN messages and signals
    - Channel list filter for CAN message IDs
  - Data Stream
    - Added triggered data stream
  - SCPI
    - Check saturation status
    - Highest and lowest timing interval
    - Control of triggered data stream
  - Digital Out
    - Configurable up to 3600s
  - Stop Measurement and quit on shutdown signal.
    - Can be used to quit OXYGEN on power failure (with an UPS)
  - Counter
    - Event counter max number of pulse increased to 2000000
    - Optional reset counters at measurement start
  - Installer
    - New msi based installer

## Fixes
  - SCPI
    - Support for connection override
  - IMC2 Export
     - Fixed issue when other applications could not read the samples of frequency measurement channels.
  - Bridge scaling: Fixed unit reset when changing scaling type
  - TRIONet
    - Fixed "Auto claim USB" on systems that alter the TRIONet MAC address
  - Performance and stability improvements



## 2022-07-15 Release Notice DEWETRON Oxygen R6.2.1 x64
Revision: 9fc52c1f65b49de1b08c5bdb8e08ac6a98189ae0

Components                      | Version
--------------------------------|--------------------------
DEWETRON Oxygen                 | 6.2.1.62584

## Files
DEWETRON_Oxygen_Setup_R6.2.1_x64.exe
DEWETRON_Oxygen_Setup_R6.2.1_x64_cvss.exe (no Python scripting)

## Requirements
* 6.x Software License required!
* OS: Windows 10 64bit or better
* CPU: Intel i3 3rd gen. or better
* Minimum RAM: 8 GB
* Recommended RAM: 16 GB (for high sample rates and channel counts)
* DAQ Hardware:
  - DEWETRON TRION and TRION3 (DEWETRON TRION Software R6.2.1)
  - DEWETRON ORION DAQ (ORION DAQ Driver V2.3.1.0)
  - DEWETRON ORION DSA (ORION DSA Driver V5.0.1.0)

## Installation procedure
  - TRION:
    - Install TRION applications
    - Reboot system (if requested by the installer)
    - Start DEWETRON Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
    - Power-cycle TRION boards (Power down system, then restart)
    - Start DEWETRON Explorer and check for a successful firmware upgrade
  - OXYGEN:
    - Install Oxygen
    - Verify HW settings in system menu on first startup

## New Features
  - Data Navigation
    - Import CSV files in analysis
    - "Save As" allows to remove channel data from DMD files
  - Advanced Statistics
    - Triggered Statistics - calculate on trigger events
    - Running Statistics - running statistics on given window for sync channels
  - Hardware: XR Series
    - Support for RS485 and CAN Mode
    - Export DBC file in CAN Mode
  - NetCDF Export
    - Network Common Data Form support (NetCDF3, NetCDF4, NetCDF5)
  - CVSS installer without embedded Python

## Improvements
  - Power:
    -  Accumulate current signals for capacity computation
  - User Experience
    - Added error list
    - "Selection" header type support
    - Recorder allows up to 40 channels
    - Multi select instruments to edit properties
    - Hardware mismatch dialog can be forced
  - XY Chart
    - Multiple traces with shared X-Y axis
  - DMD Reader
    - Added functions to read measurement setup (xml)
  - FFT
    - Added FFT Averaging
  - Enum Scaling
    - Available for formular channels
  - Exports
    - Added align to trigger

## Fixes
  - Fixed memory leak in split file video recording with h.264 on Intel hardware
  - Memory consumption reduced for long-time recordings
  - Power: flicker emission is computed more accurately
  - TEDS: Fixed issue with accelerometer sensor
  - Frequency measurement: Fixed crash with high sample rates (>2MS)
  - ARXML: Fixed issue showing channels as other channels
  - Excel Export: 
    - Fixed missing reduced samples
    - Fixed user reduced channel names in
  - CVS Import: Fixed handling of unicode paths



## 2022-07-04 Release Notice DEWETRON Oxygen R6.2.0 x64
Revision: 4e948c29615a94058afbc48c41609269f3b45105

Components                      | Version
--------------------------------|--------------------------
DEWETRON Oxygen                 | 6.2.0.62422

## Files
DEWETRON_Oxygen_Setup_R6.2.0_x64.exe
DEWETRON_Oxygen_Setup_R6.2.0_x64_cvss.exe

## Requirements
* 6.x Software License required!
* OS: Windows 10 64bit or better
* CPU: Intel i3 3rd gen. or better
* Minimum RAM: 8 GB
* Recommended RAM: 16 GB (for high sample rates and channel counts)
* DAQ Hardware:
  - DEWETRON TRION and TRION3 (DEWETRON TRION Software R6.2.0)
  - DEWETRON ORION DAQ (ORION DAQ Driver V2.3.1.0)
  - DEWETRON ORION DSA (ORION DSA Driver V5.0.1.0)

## Installation procedure
  - TRION:
    - Install TRION applications
    - Reboot system (if requested by the installer)
    - Start DEWETRON Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
    - Power-cycle TRION boards (Power down system, then restart)
    - Start DEWETRON Explorer and check for a successful firmware upgrade
  - OXYGEN:
    - Install Oxygen
    - Verify HW settings in system menu on first startup

## New Features
  - Data Navigation
    - Import CSV files in analysis
    - "Save As" allows to remove channel data from DMD files
  - Advanced Statistics
    - Triggered Statistics - calculate on trigger events
    - Running Statistics - running statistics on given window for sync channels
  - Hardware: XR Series
    - Support for RS485 and CAN Mode
    - Export DBC file in CAN Mode
  - NetCDF Export
    - Network Common Data Form support (NetCDF3, NetCDF4, NetCDF5)
  - CVSS installer without embedded Python

## Improvements
  - Power:
    -  Accumulate current signals for capacity computation
  - User Experience
    - Added error list
    - "Selection" header type support
    - Recorder allows up to 40 channels
    - Multi select instruments to edit properties
    - Hardware mismatch dialog can be forced
  - XY Chart
    - Multiple traces with shared X-Y axis
  - DMD Reader
    - Added functions to read measurement setup (xml)
  - FFT
    - Added FFT Averaging
  - Enum Scaling
    - Available for formular channels
  - Exports
    - Added align to trigger

## Fixes
  - Fixed memory leak in split file video recording with h.264 on Intel hardware
  - Memory consumption reduced for long-time recordings
  - Power: flicker emission is computed more accurately
  - TEDS: Fixed issue with accelerometer sensor
  - Frequency measurement: Fixed crash with high sample rates (>2MS)
  - ARXML: Fixed issue showing channels as other channels
  - Export: Fixed reduces sample missing in EXCEL export



## 2022-05-02 Release Notice DEWETRON Oxygen R6.1.1 x64

### Version: 6.1.1.61822
Revision: 80a07470c3ce5169ceb344dbd3f3e17c0b0185fa

Components                      | Version
--------------------------------|--------------------------
DEWETRON Oxygen                 | 6.1.1.61822

## Files
DEWETRON_Oxygen_Setup_R6.1.1_x64.exe

## Requirements
* 6.x Software License required!
* OS: Windows 10 64bit or better
* CPU: Intel i5 3rd gen. or better
* Minimum RAM: 8 GB
* Recommended RAM: 16 GB (for high sample rates and channel counts)
* DAQ Hardware:
  - DEWETRON TRION and TRION3 (DEWETRON TRION Software R6.1.1)
  - DEWETRON ORION DAQ (ORION DAQ Driver V2.3.1.0)
  - DEWETRON ORION DSA (ORION DSA Driver V5.0.1.0)

## Installation procedure
  - TRION:
    - Install TRION applications
    - Reboot system (if requested by the installer)
    - Start DEWETRON Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
    - Power-cycle TRION boards (Power down system, then restart)
    - Start DEWETRON Explorer and check for a successful firmware upgrade
  - OXYGEN:
    - Install Oxygen
    - Verify HW settings in system menu on first startup

## Fixes
  - Fixed wrong white on white rendering with Oxygen classic style
  - Installation using SYSTEM account fixed
  - Snapshot fixed an issue when the set interval was not applied correctly
  - Order Analysis performance improvement
  - Stability
    - Frequency Measurement: Fixed Oxygen crash on >2MS boards
    - Fix crash due to channel without timebase in audio player instrument
    - Fix crash with Stop measurement trigger
    - Fix crash when using spectrum analyzer and multiple file open
    - Fix spurious crash when opening splitted DMD files
    
