## 2025-02-17 Release Notice DEWETRON TRION API R7.4.1

Revision: 57b8f7de701145d7610724e638c3dfbe599f66cf

Components                      | Version
--------------------------------|--------------------------
DEWETRON Explorer               | 7.4.1.7232
DEWETRON TRION API              | 7.4.1.7232
DEWETRON TRION driver           | 7.4.1.7232
DEWETRON DEWE2 driver           | 7.4.1.7232

## Files
DEWETRON-TRION-Applications-7.4.1.7232.exe

## Requirements
* Update all TRION modules to the latest firmware included in this release
* Use OXYGEN R7.4.1 or higher
* Windows 10 64-Bit or better

## Installation procedure
* Install TRION applications
* Reboot system (if requested by the installer)
* Start DEWETRON Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
* Power-cycle TRION boards (Power down system, then restart)
* Start DEWETRON Explorer and check for a successful firmware upgrade

## Fixes and Changes
 * New firmware for 18XX-MULTI fixing spikes in the signal when using CAN OUT

## New Firmwares

HW Support TRION3 modules       | Firmware
--------------------------------|-----------
TRION3-1801-MULTI-8-L0B         | FW: 0053
TRION3-1802-MULTI-8-L0B         | FW: 0053
TRION3-1810-MULTI-8-L0B         | FW: 0053
TRION3-1820-MULTI-4-D           | FW: 0053
TRION3-1820-MULTI-8-L0B         | FW: 0053
TRION3-1850-MULTI-4-D           | FW: 0053
TRION3-1850-MULTI-8-L0B         | FW: 0053

HW Support TRION modules        | Firmware
--------------------------------|-----------
TRION-1820-MULTI-4-D            | FW: 0053
TRION-1850-MULTI-4-D            | FW: 0053



## 2025-02-05 Release Notice DEWETRON TRION API R7.4.0

Revision: 472a361fb6ed138b9c7c376bd22d947f74fefa14

Components                      | Version
--------------------------------|--------------------------
DEWETRON Explorer               | 7.4.0.7046
DEWETRON TRION API              | 7.4.0.7046
DEWETRON TRION driver           | 7.4.0.7046
DEWETRON DEWE2 driver           | 7.4.0.7046

## Files
DEWETRON-TRION-Applications-7.4.0.7046.exe

## Requirements
* Update all TRION modules to the latest firmware included in this release
* Use OXYGEN R7.4.0 or higher
* Windows 10 64-Bit or better

## Installation procedure
* Install TRION applications
* Reboot system (if requested by the installer)
* Start DEWETRON Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
* Power-cycle TRION boards (Power down system, then restart)
* Start DEWETRON Explorer and check for a successful firmware upgrade

## New Features
* DEWETRON Explorer: "View/Log" displaying application log
* TRIONet: ICMP/Ping extension for systems blocking UDP broadcasts

## Fixes and Changes
* TRION API: Fix 3Wire RTD/Res settings and gain for 18XX-MULTI boards
* TRION-POWER: Fix for spikes in measured samples when using SUB-XV module
* Removed 32bit driver for TRION and DEWE2
* Removed TRION-SDK from installer. Please use github instead.


## 2024-11-20 Release Notice DEWETRON TRION API R7.3.2

Revision: f6f8bf5b1b38b78b8d8a67761130412adeb7e977

Components                      | Version
--------------------------------|--------------------------
DEWETRON Explorer               | 7.3.2.6198
DEWETRON TRION API              | 7.3.2.6198
DEWETRON TRION driver           | 7.3.2.6198
DEWETRON DEWE2 driver           | 7.3.2.6198

## Files
DEWETRON-TRION-Applications-7.3.2.6198.exe

## Requirements
* Update all TRION modules to the latest firmware included in this release
* Use OXYGEN R7.3.2 or higher
* Windows 10 64-Bit or better

## Installation procedure
* Install TRION applications
* Reboot system (if requested by the installer)
* Start DEWETRON Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
* Power-cycle TRION boards (Power down system, then restart)
* Start DEWETRON Explorer and check for a successful firmware upgrade

## Fixes
* Fix for semaphore handling of date and time changes.


## 2024-11-14 Release Notice DEWETRON TRION API R7.3.0

Revision: e0677c9d3d0752715941d97bcaca3b4db9ec909f

Components                      | Version
--------------------------------|--------------------------
DEWETRON Explorer               | 7.3.0.6146
DEWETRON TRION API              | 7.3.0.6146
DEWETRON TRION driver           | 7.3.0.6146
DEWETRON DEWE2 driver           | 7.3.0.6146

## Files
DEWETRON-TRION-Applications-7.3.0.6146.exe

## Requirements
* Update all TRION modules to the latest firmware included in this release
* Use OXYGEN R7.3.0 or higher
* Windows 10 64-Bit or better

## Installation procedure
* Install TRION applications
* Reboot system (if requested by the installer)
* Start DEWETRON Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
* Power-cycle TRION boards (Power down system, then restart)
* Start DEWETRON Explorer and check for a successful firmware upgrade

## New Features
* Performance and stability improvements

## Fixes
* TRION3-18XX-MULTI: Fix for spurious CAN error during calibration
* TRION-CONTROLLER: New firmware fixing glitches when using CAN OUT
* NEXDAQ: New firmware supporting 89MHz FMC clock

## New Firmwares

HW Support TRION3 modules       | Firmware
--------------------------------|-----------
TRION3-1801-MULTI-8-L0B         | FW: 0052
TRION3-1802-MULTI-8-L0B         | FW: 0052
TRION3-1810-MULTI-8-L0B         | FW: 0052
TRION3-1820-MULTI-4-D           | FW: 0052
TRION3-1820-MULTI-8-L0B         | FW: 0052
TRION3-1850-MULTI-4-D           | FW: 0052
TRION3-1850-MULTI-8-L0B         | FW: 0052
TRION3-CONTROLLER               | FW: 0043   MCU: 01000122


HW Support TRION modules        | Firmware
--------------------------------|-----------
TRION-1820-MULTI-4-D            | FW: 0052
TRION-1850-MULTI-4-D            | FW: 0052


HW Support Chassis modules      | Firmware
--------------------------------|-----------
TRION3-CONTROLLER               | FW: 0043   MCU: 01000122


HW Support Nex[DAQ] modules     | Firmware
--------------------------------|-----------
NEXDAQ-1000                     | FW: 0054
NEXDAQ-200                      | FW: 0054


## 2024-08-27 Release Notice DEWETRON TRION API R7.2.1

Revision: 876a648bcaebd47fe225e89ab132256fce382190

Components                      | Version
--------------------------------|--------------------------
DEWETRON Explorer               | 7.2.1.5243
DEWETRON TRION API              | 7.2.1.5243
DEWETRON TRION driver           | 7.2.1.5243
DEWETRON DEWE2 driver           | 7.2.1.5243

## Files
DEWETRON-TRION-Applications-7.2.1.5243.exe

## Requirements
* Update all TRION modules to the latest firmware included in this release
* Use OXYGEN R7.2.0 or higher
* Windows 10 64-Bit or better

## Installation procedure
* Install TRION applications
* Reboot system (if requested by the installer)
* Start DEWETRON Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
* Power-cycle TRION boards (Power down system, then restart)
* Start DEWETRON Explorer and check for a successful firmware upgrade

## Fixes
* NEX[DAQ]-1000 simulation sample rate divider support fixed.


## 2024-08-13 Release Notice DEWETRON TRION API R7.2.0

Revision: c59cfa726b9840bdf89643b3e6641672483dbc36

Components                      | Version
--------------------------------|--------------------------
DEWETRON Explorer               | 7.2.0.5178
DEWETRON TRION API              | 7.2.0.5178
DEWETRON TRION driver           | 7.2.0.5178
DEWETRON DEWE2 driver           | 7.2.0.5178

## Files
DEWETRON-TRION-Applications-7.2.0.5178.exe

## Requirements
* Update all TRION modules to the latest firmware included in this release
* Use OXYGEN R7.2.0 or higher
* Windows 10 64-Bit or better

## Installation procedure
* Install TRION applications
* Reboot system (if requested by the installer)
* Start DEWETRON Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
* Power-cycle TRION boards (Power down system, then restart)
* Start DEWETRON Explorer and check for a successful firmware upgrade

## New Features
* Chassis Controller Feature Upgrade
* PPS-Output via Chassis Controller

## Fixes
* ID003 TRION3-1810M-POWER: Phase mismatch at low Samplerate
* ID004 Phase mismatch of TRION-POWER-SUB-dLV
* CAN Selftest for Chassis Controller

## Known Limitations
* NEX[DAQ]-1000 simulation does not support sample rate divider

## New Firmwares

HW Support TRION3 modules       | Firmware
--------------------------------|-----------
TRION3-1600-dLV-16-D            | FW: 1902
TRION3-1600-dLV-16-D-CAN        | FW: 1902
TRION3-1600-dLV-32-D            | FW: 1902
TRION3-1600-dLV-32-D-CAN        | FW: 1902
TRION3-1801-MULTI-8-L0B         | FW: 0046
TRION3-1802-MULTI-8-L0B         | FW: 0046
TRION3-1802-dLV-16-D            | FW: 1902
TRION3-1802-dLV-16-D-CAN        | FW: 1902
TRION3-1802-dLV-32-D            | FW: 1902
TRION3-1802-dLV-32-D-CAN        | FW: 1902
TRION3-1810-HV-8                | FW: 0078
TRION3-1810-MULTI-8-L0B         | FW: 0046
TRION3-1810M-POWER-4            | FW: 0078
TRION3-1820-MULTI-4-D           | FW: 0046
TRION3-1820-MULTI-8-L0B         | FW: 0046
TRION3-1820-POWER-4             | FW: 0078
TRION3-1850-MULTI-4-D           | FW: 0046
TRION3-1850-MULTI-8-L0B         | FW: 0046
TRION3-CONTROLLER               | FW: 0042   MCU: 01000122


HW Support TRION modules        | Firmware
--------------------------------|-----------
TRION-1600-dLV-16-D             | FW: 1902
TRION-1600-dLV-16-D-CAN         | FW: 1902
TRION-1600-dLV-32-D             | FW: 1902
TRION-1600-dLV-32-D-CAN         | FW: 1902
TRION-1802-dLV-16-D             | FW: 1902
TRION-1802-dLV-16-D-CAN         | FW: 1902
TRION-1802-dLV-32-D             | FW: 1902
TRION-1802-dLV-32-D-CAN         | FW: 1902
TRION-1810-HV-4                 | FW: 0078
TRION-1810-HV-8                 | FW: 0078
TRION-1810M-POWER-4             | FW: 0078
TRION-1820-MULTI-4-D            | FW: 0046
TRION-1820-POWER-4              | FW: 0078
TRION-1850-MULTI-4-D            | FW: 0046


HW Support Chassis modules      | Firmware
--------------------------------|-----------
TRION3-CONTROLLER               | FW: 0042   MCU: 01000122

HW Support LITE[PA] modules     | Firmware
--------------------------------|-----------
LITEPA-4                        | FW: 0078


HW Support PUREC modules        | Firmware
--------------------------------|-----------
PUREC-200                       | FW: 1902
PUREC-200-CAN                   | FW: 1902
PUREC-50                        | FW: 1902
PUREC-50-CAN                    | FW: 1902


## 2024-05-27 Release Notice DEWETRON TRION API R7.1.1

Revision: 26c98ba4677bc1a19d7e0590475122b6c54e05d3

Components                      | Version
--------------------------------|--------------------------
DEWETRON Explorer               | 7.1.1.4060
DEWETRON TRION API              | 7.1.1.4060
DEWETRON TRION driver           | 7.1.1.4060
DEWETRON DEWE2 driver           | 7.1.1.4060

## Files
DEWETRON-TRION-Applications-7.1.1.4060.exe

## Requirements
* Update all TRION modules to the latest firmware included in this release
* Use OXYGEN R7.1.1 or higher
* Windows 10 64-Bit or better

## Installation procedure
* Install TRION applications
* Reboot system (if requested by the installer)
* Start DEWETRON Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
* Power-cycle TRION boards (Power down system, then restart)
* Start DEWETRON Explorer and check for a successful firmware upgrade

## Fixes
* TRION3-1820-ACC-8-MD fixed firmware showing correct channel status in voltage mode

## Known Limitations
* NEX[DAQ]-1000 simulation does not support sample rate divider

## New Firmwares

HW Support TRION3 modules       | Firmware
--------------------------------|-----------
TRION3-1820-ACC-8-MD            | FW: 0050


## 2024-05-13 Release Notice DEWETRON TRION API R7.1.0

Revision: 140127caaf216ce90ed800340f5e43758fd297f5

Components                      | Version
--------------------------------|--------------------------
DEWETRON Explorer               | 7.1.0.4012
DEWETRON TRION API              | 7.1.0.4012
DEWETRON TRION driver           | 7.1.0.4012
DEWETRON DEWE2 driver           | 7.1.0.4012

## Files
DEWETRON-TRION-Applications-7.1.0.4012.exe

## Requirements
* Update all TRION modules to the latest firmware included in this release
* Use OXYGEN R7.1.0 or higher
* Windows 10 64-Bit or better

## Installation procedure
* Install TRION applications
* Reboot system (if requested by the installer)
* Start DEWETRON Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
* Power-cycle TRION boards (Power down system, then restart)
* Start DEWETRON Explorer and check for a successful firmware upgrade

## New Features
* TRION3-1820-ACC-8-MD support added
* TRION3-AOUT-8: New mode "Channel Sum" (see New Firmwares)
  * Possibility to create linear equation with all AI and output the result via AO channel
* PTP-Out option for TRION-TIMING-V3 and TRION-VGPS-V3
* LITE[PA] support added
* TRION-SUB-CT current transducer support added
* NEX[DAQ]-1000 support added
  * AI sample rate max 1MS
  * CNT sample rate max 200kS
* Individual CAN(-FD) baudrate selection supported

## Fixes
* Fix for wrong AC coupling on MSI2-CH with TRION-MULTI-2402 displaying 0.08Hz instead of 0.14Hz
* Fix for duplicate boards shown in DEWETRON Explorer

## Known Limitations
* NEX[DAQ]-1000 simulation does not support sample rate divider

## New Firmwares

HW Support TRION3 modules       | Firmware
--------------------------------|-----------
TRION3-1820-ACC-8-MD            | FW: 0049
TRION3-AOUT-8                   | FW: 0040

HW Support TRION modules        | Firmware
--------------------------------|-----------
TRION-TIMING-V3                 | FW: F021   MCU: 01000121
TRION-VGPS-100-V3               | FW: F021   MCU: 01000121
TRION-VGPS-20-V3                | FW: F021   MCU: 01000121

HW Support Nex[DAQ] modules     | Firmware
--------------------------------|-----------
NEXDAQ-1000                     | FW: 0051
NEXDAQ-200                      | FW: 0051

HW Support LITE[PA] modules     | Firmware
--------------------------------|-----------
LITEPA-CONTROLLER               | FW: 0038


## 2024-03-08 Release Notice DEWETRON TRION API R7.0.1

Revision: b1c725da774ed2596fc9e59c111e53bd3f5cf5a1

Components                      | Version
--------------------------------|--------------------------
DEWETRON Explorer               | 7.0.1.3193
DEWETRON TRION API              | 7.0.1.3193
DEWETRON TRION driver           | 7.0.1.3193
DEWETRON DEWE2 driver           | 7.0.1.3193

## Files
DEWETRON-TRION-Applications-7.0.1.3193.exe

## Requirements
* Update all TRION modules to the latest firmware included in this release
* Use OXYGEN R7.0.0 or higher
* Windows 10 64-Bit or better

## Installation procedure
* Install TRION applications
* Reboot system (if requested by the installer)
* Start DEWETRON Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
* Power-cycle TRION boards (Power down system, then restart)
* Start DEWETRON Explorer and check for a successful firmware upgrade

## New Features and most important bugfixes
* Fix: MSI2-CH-100 with TRION3-18XX-Multi not working


## 2024-03-08 Release Notice DEWETRON TRION API R6.7.4

Revision: 5bfa00ce7c0d900ebe46b42d7ee420c3e28c8f2d

Components                      | Version
--------------------------------|--------------------------
DEWETRON Explorer               | 6.7.4.3192
DEWETRON TRION API              | 6.7.4.3192
DEWETRON TRION driver           | 6.7.4.3192
DEWETRON DEWE2 driver           | 6.7.4.3192

## Files
DEWETRON-TRION-Applications-6.7.4.3192.exe

## Requirements
* Update all TRION modules to the latest firmware included in this release
* Use OXYGEN R6.7.3 or higher
* Windows 10 64-Bit or better

## Installation procedure
* Install TRION applications
* Reboot system (if requested by the installer)
* Start DEWETRON Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
* Power-cycle TRION boards (Power down system, then restart)
* Start DEWETRON Explorer and check for a successful firmware upgrade

## New Features and most important bugfixes
* Fix: MSI2-CH-100 with TRION3-18XX-Multi not working


## 2024-02-01 Release Notice DEWETRON TRION API R7.0.0

Revision: c8730c64bd0f421a4b0a87b70977e5b072fa9e1e

Components                      | Version
--------------------------------|--------------------------
DEWETRON Explorer               | 7.0.0.2733
DEWETRON TRION API              | 7.0.0.2733
DEWETRON TRION driver           | 7.0.0.2733
DEWETRON DEWE2 driver           | 7.0.0.2733

## Files
DEWETRON-TRION-Applications-7.0.0.2733.exe

## Requirements
* Update all TRION modules to the latest firmware included in this release
* Use OXYGEN R7.0.0 or higher
* Windows 10 64-Bit or better

## Installation procedure
* Install TRION applications
* Reboot system (if requested by the installer)
* Start DEWETRON Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
* Power-cycle TRION boards (Power down system, then restart)
* Start DEWETRON Explorer and check for a successful firmware upgrade

## New Features and most important bugfixes
* Dewetron Explorer
  * New X icon, better dark mode, splashscreen
  * Improved network configuration
    * Added set to default (default static, default dhcp)
    * Allow configuration even if ip seetings do not match (TRIONet, NEXDAQ)
* CAN-FD bittiming added
* Fix: ID001 - TRION(3)-18xx-MULTI Highpass Filters (0.16Hz - 100Hz) show 64% overshoot and higher cutoff frequencies than expected
* Fix: ID002 - TRION(3)-18xx-MULTI Highpass Filters (0.16Hz - 100Hz) is distorting the input signal


## Known Limitations

## New Firmwares

HW Support TRION modules        | Firmware
--------------------------------|-----------
TRION3-1820-MULTI-4-D           | FW: x0043
TRION3-1820-MULTI-8-L0B         | FW: x0043
TRION3-1850-MULTI-4-D           | FW: x0043
TRION3-1850-MULTI-8-L0B         | FW: x0043
TRION3-1801-MULTI-8-L0B         | FW: x0043
TRION-1820-MULTI-4-D            | FW: x0043

HW Support DEWE3 chassis        | Firmware
--------------------------------|-----------
DEWE3-A4                        | FW: x0038   MCU: 0x01000109
DEWE3-M4                        | FW: x0038   MCU: 0x01000109


## 2024-02-14 Release Notice DEWETRON TRION API R6.7.3

Revision: 7aa6f0e1381c890da5d0df82d545e1a3cac015d7

Components                      | Version
--------------------------------|--------------------------
DEWETRON Explorer               | 6.7.3.2897
DEWETRON TRION API              | 6.7.3.2897
DEWETRON TRION driver           | 6.7.3.2897
DEWETRON DEWE2 driver           | 6.7.3.2897

## Files
DEWETRON-TRION-Applications-6.7.3.2897.exe

## Requirements
* Update all TRION modules to the latest firmware included in this release
* Use OXYGEN R6.7.3 or higher
* Windows 10 64-Bit or better

## Installation procedure
* Install TRION applications
* Reboot system (if requested by the installer)
* Start DEWETRON Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
* Power-cycle TRION boards (Power down system, then restart)
* Start DEWETRON Explorer and check for a successful firmware upgrade

## New Features and most important bugfixes
* Fix: ID001 - TRION(3)-18xx-MULTI Highpass Filters (0.16Hz - 100Hz) show 64% overshoot and higher cutoff frequencies than expected
* Fix: ID002 - TRION(3)-18xx-MULTI Highpass Filters (0.16Hz - 100Hz) is distorting the input signal

## New Firmwares

HW Support TRION modules        | Firmware
--------------------------------|-----------
TRION3-1820-MULTI-4-D           | FW: x0043
TRION3-1820-MULTI-8-L0B         | FW: x0043
TRION3-1850-MULTI-4-D           | FW: x0043
TRION3-1850-MULTI-8-L0B         | FW: x0043
TRION3-1801-MULTI-8-L0B         | FW: x0043
TRION-1820-MULTI-4-D            | FW: x0043

HW Support DEWE3 chassis        | Firmware
--------------------------------|-----------
DEWE3-A4                        | FW: x0038   MCU: 0x01000109
DEWE3-M4                        | FW: x0038   MCU: 0x01000109


## 2023-12-04 Release Notice DEWETRON TRION API R6.7.2

Revision: 6e29cade2bda4c122e6674a6263aeb6b6bb16c2c

Components                      | Version
--------------------------------|--------------------------
DEWETRON Explorer               | 6.7.2.2175
DEWETRON TRION API              | 6.7.2.2175
DEWETRON TRION driver           | 6.7.2.2175
DEWETRON DEWE2 driver           | 6.7.2.2175

## Files
DEWETRON-TRION-Applications-6.7.2.2175.exe

## Requirements
* Update all TRION modules to the latest firmware included in this release
* Use OXYGEN R6.7.1 or higher
* Windows 10 64-Bit or better

## Installation procedure
* Install TRION applications
* Reboot system (if requested by the installer)
* Start DEWETRON Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
* Power-cycle TRION boards (Power down system, then restart)
* Start DEWETRON Explorer and check for a successful firmware upgrade

## New Features and most important bugfixes
* TRION(3)-18xx-MULTI Highpass Filters (0.16Hz - 100Hz) is distorting the input signal
* TrionCal: TRION-18XX-MULTI, allow AUTO and 0Hz for HP-Filter in XML
* CHASSIS-CONTROLLER-V2: Fixed an issue with spikes when using CAN OUT (new fw)

## Known Limitations
* ID001 - TRION(3)-18xx-MULTI Highpass Filters (0.16Hz - 100Hz) show 64% overshoot and higher cutoff frequencies than expected

## New Firmwares

HW Support DEWE3 chassis        | Firmware
--------------------------------|-----------
DEWE3-A4                        | FW: x0038   MCU: 0x01000109
DEWE3-M4                        | FW: x0038   MCU: 0x01000109


## 2023-10-23 Release Notice DEWETRON TRION API R6.7.1

Revision: 1ee33ea7162d4418af9de534a019b5426b815472

Components                      | Version
--------------------------------|--------------------------
DEWETRON Explorer               | 6.7.1.1582
DEWETRON TRION API              | 6.7.1.1582
DEWETRON TRION driver           | 6.7.1.1582
DEWETRON DEWE2 driver           | 6.7.1.1582

## Files
DEWETRON-TRION-Applications-6.7.1.1582.exe

## Requirements
* Update all TRION modules to the latest firmware included in this release
* Use OXYGEN R6.7.1 or higher
* Windows 10 64-Bit or better

## Installation procedure
* Install TRION applications
* Reboot system (if requested by the installer)
* Start DEWETRON Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
* Power-cycle TRION boards (Power down system, then restart)
* Start DEWETRON Explorer and check for a successful firmware upgrade

## New Features and most important bugfixes
* TRION driver fix for last 32bit addressable page (Debian Linux OS)

## Known Limitations
* None


## 2023-10-06 Release Notice DEWETRON TRION API R6.7.0

Revision: 39c8e85197f9ff266a891bc4d1ba5f67ffc503df

Components                      | Version
--------------------------------|--------------------------
DEWETRON Explorer               | 6.7.0.1448
DEWETRON TRION API              | 6.7.0.1448
DEWETRON TRION driver           | 6.7.0.1448
DEWETRON DEWE2 driver           | 6.7.0.1448

## Files
DEWETRON-TRION-Applications-6.7.0.1448.exe

## Requirements
* Update all TRION modules to the latest firmware included in this release
* Use OXYGEN R6.7.0 or higher
* Windows 10 64-Bit or better

## Installation procedure
* Install TRION applications
* Reboot system (if requested by the installer)
* Start DEWETRON Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
* Power-cycle TRION boards (Power down system, then restart)
* Start DEWETRON Explorer and check for a successful firmware upgrade

## New Features and most important bugfixes
* DEWE3-M8S enclosure support added
* TRION3-1810-HV-8 support added

## Fixes
* TRIONet3 simulation allows TRION3 boards

## New Firmwares

HW Support TRION modules        | Firmware
--------------------------------|-----------
TRION3-1810M-POWER-4            | FW: x0077
TRION-1820-POWER-4              | FW: x0077
TRION-1810M-POWER-4             | FW: x0077
TRION3-1810-SUB-8               | FW: x0019

HW Support DEWE3 chassis        | Firmware
--------------------------------|-----------
DEWE3-A4                        | FW: x0036   MCU: 0x01000109
DEWE3-M4                        | FW: x0036   MCU: 0x01000109


## 2023-09-14 Release Notice DEWETRON TRION API R6.6.1

Revision: 45fadabcfe6f627121d9a4fc8a177236070b5621

Components                      | Version
--------------------------------|--------------------------
DEWETRON Explorer               | 6.6.1.1146
DEWETRON TRION API              | 6.6.1.1146
DEWETRON TRION driver           | 6.6.1.1146
DEWETRON DEWE2 driver           | 6.6.1.1146

## Files
DEWETRON-TRION-Applications-6.6.1.1146.exe

## Requirements
* Update all TRION modules to the latest firmware included in this release
* Use OXYGEN R6.6.1 or higher
* Windows 10 64-Bit or better

## Installation procedure
* Install TRION applications
* Reboot system (if requested by the installer)
* Start DEWETRON Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
* Power-cycle TRION boards (Power down system, then restart)
* Start DEWETRON Explorer and check for a successful firmware upgrade

## New Features and most important bugfixes
* NEX[DAQ]-200 device support

## Known Limitations
* None

## Firmwares


## 2023-07-24 Release Notice DEWETRON TRION API R6.6.0

Revision: 98efc4da43ef96f4b384bda3c6ae1c658a374fae

Components                      | Version
--------------------------------|--------------------------
DEWETRON Explorer               | 6.6.0.632
DEWETRON TRION API              | 6.6.0.632
DEWETRON TRION driver           | 6.6.0.632
DEWETRON DEWE2 driver           | 6.6.0.632

## Files
DEWETRON-TRION-Applications-6.6.0.632.exe

## Requirements
* Update all TRION modules to the latest firmware included in this release
* Use OXYGEN R6.6 or higher
* Windows 10 64-Bit or better

## Installation procedure
* Install TRION applications
* Reboot system (if requested by the installer)
* Start DEWETRON Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
* Power-cycle TRION boards (Power down system, then restart)
* Start DEWETRON Explorer and check for a successful firmware upgrade

## New Features and most important bugfixes
* TRION(3)-1820-MULTI:
  * Input coupling (highpass filter) overshoot fixed with 0.15Hz filter
* TRIONet3 support
* TRION(3)-Power:
  * TRION SUB-XV support
* TRION3-SUB-8:
  * TRION SUB-XV support

## Known Limitations
* None

## Firmwares

HW Support TRION modules        | Firmware
--------------------------------|-----------
TRION3-1810M-POWER-4            | FW: x0076
TRION3-1810-SUB-8               | FW: x0017
TRION3-1820-MULTI-4-D           | FW: x0035
TRION3-1820-MULTI-8-L0B         | FW: x0035
TRION3-1850-MULTI-4-D           | FW: x0035
TRION3-1850-MULTI-8-L0B         | FW: x0035
TRION3-AOUT-8                   | FW: x0035
TRION-1620-ACC-6-BNC            | FW: x0031
TRION-1620-ACC-6-L1B            | FW: x0031
TRION-1620-LV-6-BNC             | FW: x0031
TRION-1620-LV-6-L1B             | FW: x0031
TRION-1603-LV-6-BNC             | FW: x0A15
TRION-1603-LV-6-L1B             | FW: x0A15
TRION-1603-LV-6-D25             | FW: x0A15
TRION-1600-dLV-16-D             | FW: x1893
TRION-1600-dLV-16-D-CAN         | FW: x1893
TRION-1600-dLV-32-D             | FW: x1893
TRION-1600-dLV-32-D-CAN         | FW: x1893
TRION-1802-dLV-16-D             | FW: x1893
TRION-1802-dLV-16-D-CAN         | FW: x1893
TRION-1802-dLV-32-D             | FW: x1893
TRION-1802-dLV-32-D-CAN         | FW: x1893
TRION-1810-HV-4                 | FW: x0076
TRION-1810-HV-8                 | FW: x0076
TRION-1820-POWER-4              | FW: x0076
TRION-1810M-POWER-4             | FW: x0076
TRION-1820-MULTI-4-D            | FW: x0035
TRION-2402-MULTI-4-D            | FW: x0B18
TRION-2402-MULTI-8-L0B          | FW: x0A24
TRION-2402-MULTI-S1             | FW: x0034
TRION-2402-dSTG-6-L1B           | FW: x1120
TRION-2402-dSTG-6-L1B-S1        | FW: x1120
TRION-2402-dSTG-8-D             | FW: x1120
TRION-2402-dSTG-8-L0B           | FW: x1120
TRION-2402-dSTG-8-RJ            | FW: x1120
TRION-2400-dSTG-8-L0B           | FW: x1120
TRION-2400-dSTG-OEM             | FW: x1120
TRION-2402-dACC-6-BNC           | FW: x1119
TRION-2402-dACC-8-SMB           | FW: x1119
TRION-2402-dACC-8-MD            | FW: x1119
TRION-2402-V-4-B                | FW: x1017
TRION-2402-V-8-B                | FW: x1017
TRION-CNT-6-L1B                 | FW: x1119
TRION-BASE                      | FW: x1145
TRION-TIMING                    | FW: x1145
TRION-TIMING-V2                 | FW: x0004
TRION-TIMING-V3                 | FW: xF016   MCU: x00020095
TRION-VGPS-20                   | FW: x1145
TRION-VGPS-20-V3                | FW: xF016   MCU: x00020095
TRION-VGPS-100                  | FW: x1145
TRION-VGPS-100-V3               | FW: xF016   MCU: x00020095
TRION-CAN-4                     | FW: x1122
TRION-CAN-2                     | FW: x1122
TRION-DI-48                     | FW: x1119
TRION-DI-64-S1                  | FW: x0009

HW Support PUREC                | Firmware
--------------------------------|-----------
PUREC-200                       | FW: x1893
PUREC-50                        | FW: x1893

HW Support DEWE3 chassis        | Firmware
--------------------------------|-----------
DEWE3-PA8                       |
DEWE3-A4                        | FW: x0036   MCU: 0x01000108
DEWE3-A4L                       |
DEWE3-M4                        | FW: x0036   MCU: 0x01000108
DEWE3-RM4                       |
DEWE3-RM8                       |
DEWE3-RM12                      |
DEWE3-RM16                      |
TRIONet3                        |

HW Support DEWE2 chassis        | Firmware
--------------------------------|-----------
DEWE2-PA7
DEWE2-A4
DEWE2-A4L
DEWE2-A7
DEWE2-A13
DEWE2-M4
DEWE2-M4s
DEWE2-M7
DEWE2-M7s
DEWE2-M13
DEWE2-M13s
DEWE2-M18
DEWE2-F4s
DEWE2-F7s
DEWE2-F13s
DEWE2-F18
DEWE2-F4-THUNDERBOLT
DEWE2-F13-FIBRE
TRIONet
TrendCorder



## 2023-04-06 Release Notice DEWETRON TRION API R6.5.0

Revision: 945a6696167b443c4c32b869cbd3445a9d9ae37b

Components                      | Version
--------------------------------|--------------------------
DEWETRON Explorer               | 6.5.0.65368
DEWETRON TRION API              | 6.5.0.65368
DEWETRON TRION driver           | 6.5.0.65368
DEWETRON DEWE2 driver           | 6.5.0.65368

## Files
DEWETRON-TRION-Applications-6.5.0.65368.exe

## Requirements
* Update all TRION modules to the latest firmware included in this release
* Use OXYGEN R6.5 or higher
* Windows 10 64-Bit or better

## Installation procedure
* Install TRION applications
* Reboot system (if requested by the installer)
* Start DEWETRON Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
* Power-cycle TRION boards (Power down system, then restart)
* Start DEWETRON Explorer and check for a successful firmware upgrade

## New Features and most important bugfixes:
* TRION3-1802-dLV: Full support added 
* TRION3-1600-dLV: Full support added 
* Chassis Controller 2: 
  * Frequency-Out support
  * IRIG Out support

## Known Limitations
* None

## Firmwares

HW Support TRION modules        | Firmware
--------------------------------|-----------
TRION3-1810M-POWER-4            | FW: x0072
TRION3-1810-SUB-8               | FW: x0015
TRION3-1820-MULTI-4-D           | FW: x0034
TRION3-1820-MULTI-8-L0B         | FW: x0034
TRION3-1850-MULTI-4-D           | FW: x0034
TRION3-1850-MULTI-8-L0B         | FW: x0034
TRION3-AOUT-8                   | FW: x0035
TRION-1620-ACC-6-BNC            | FW: x0031
TRION-1620-ACC-6-L1B            | FW: x0031
TRION-1620-LV-6-BNC             | FW: x0031
TRION-1620-LV-6-L1B             | FW: x0031
TRION-1603-LV-6-BNC             | FW: x0A15
TRION-1603-LV-6-L1B             | FW: x0A15
TRION-1603-LV-6-D25             | FW: x0A15
TRION-1600-dLV-16-D             | FW: x1893
TRION-1600-dLV-16-D-CAN         | FW: x1893
TRION-1600-dLV-32-D             | FW: x1893
TRION-1600-dLV-32-D-CAN         | FW: x1893
TRION-1802-dLV-16-D             | FW: x1893
TRION-1802-dLV-16-D-CAN         | FW: x1893
TRION-1802-dLV-32-D             | FW: x1893
TRION-1802-dLV-32-D-CAN         | FW: x1893
TRION-1810-HV-4                 | FW: x0072
TRION-1810-HV-8                 | FW: x0072
TRION-1820-POWER-4              | FW: x0072
TRION-1810M-POWER-4             | FW: x0072
TRION-1820-MULTI-4-D            | FW: x0034
TRION-2402-MULTI-4-D            | FW: x0B18
TRION-2402-MULTI-8-L0B          | FW: x0A24
TRION-2402-MULTI-S1             | FW: x0034
TRION-2402-dSTG-6-L1B           | FW: x1120
TRION-2402-dSTG-6-L1B-S1        | FW: x1120
TRION-2402-dSTG-8-D             | FW: x1120
TRION-2402-dSTG-8-L0B           | FW: x1120
TRION-2402-dSTG-8-RJ            | FW: x1120
TRION-2400-dSTG-8-L0B           | FW: x1120
TRION-2400-dSTG-OEM             | FW: x1120
TRION-2402-dACC-6-BNC           | FW: x1119
TRION-2402-dACC-8-SMB           | FW: x1119
TRION-2402-dACC-8-MD            | FW: x1119
TRION-2402-V-4-B                | FW: x1017
TRION-2402-V-8-B                | FW: x1017
TRION-CNT-6-L1B                 | FW: x1119
TRION-BASE                      | FW: x1145
TRION-TIMING                    | FW: x1145
TRION-TIMING-V2                 | FW: x0004
TRION-TIMING-V3                 | FW: xF016   MCU: x00020095
TRION-VGPS-20                   | FW: x1145
TRION-VGPS-20-V3                | FW: xF016   MCU: x00020095
TRION-VGPS-100                  | FW: x1145
TRION-VGPS-100-V3               | FW: xF016   MCU: x00020095
TRION-CAN-4                     | FW: x1122
TRION-CAN-2                     | FW: x1122
TRION-DI-48                     | FW: x1119
TRION-DI-64-S1                  | FW: x0009

HW Support PUREC                | Firmware
--------------------------------|-----------
PUREC-200                       | FW: x1893
PUREC-50                        | FW: x1893

HW Support DEWE3 chassis        | Firmware
--------------------------------|-----------
DEWE3-PA8                       |
DEWE3-A4                        | FW: x0033   MCU: x000200E8
DEWE3-A4L                       |
DEWE3-M4                        | FW: x0033   MCU: x000200E8
DEWE3-RM4                       |
DEWE3-RM8                       |
DEWE3-RM12                      |
DEWE3-RM16                      |

HW Support DEWE2 chassis        | Firmware
--------------------------------|-----------
DEWE2-PA7
DEWE2-A4
DEWE2-A4L
DEWE2-A7
DEWE2-A13
DEWE2-M4
DEWE2-M4s
DEWE2-M7
DEWE2-M7s
DEWE2-M13
DEWE2-M13s
DEWE2-M18
DEWE2-F4s
DEWE2-F7s
DEWE2-F13s
DEWE2-F18
DEWE2-F4-THUNDERBOLT
DEWE2-F13-FIBRE
TRIONet
TrendCorder


## 2023-01-17 Release Notice DEWETRON TRION API R6.4.0

Revision: efc2fa19814687ab39ff1fa1b5285dd6a032df92

Components                      | Version
--------------------------------|--------------------------
DEWETRON Explorer               | 6.4.0.64345
DEWETRON TRION API              | 6.4.0.64345
DEWETRON TRION driver           | 6.4.0.64345
DEWETRON DEWE2 driver           | 6.4.0.64345

## Files
DEWETRON-TRION-Applications-6.4.0.64345.exe

## Requirements
* Update all TRION modules to the latest firmware included in this release
* Use OXYGEN R6.4 or higher
* Windows 10 64-Bit or better

## Installation procedure
* Install TRION applications
* Reboot system (if requested by the installer)
* Start DEWETRON Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
* Power-cycle TRION boards (Power down system, then restart)
* Start DEWETRON Explorer and check for a successful firmware upgrade

## New Features and most important bugfixes:
* TRION3-18XX-MULTI, TRION-18XX-MULTI higher sensor excitation power
  - up to 1W for 24V setting

## Known Limitations
* None

## Firmwares

HW Support TRION modules        | Firmware
--------------------------------|-----------
TRION3-1810M-POWER-4            | FW: x0064
TRION3-1810-SUB-8               | FW: x0015
TRION3-1820-MULTI-4-D           | FW: x0034
TRION3-1820-MULTI-8-L0B         | FW: x0034
TRION3-1850-MULTI-4-D           | FW: x0034
TRION3-1850-MULTI-8-L0B         | FW: x0034
TRION3-AOUT-8                   | FW: x0035
TRION-1620-ACC-6-BNC            | FW: x0031
TRION-1620-ACC-6-L1B            | FW: x0031
TRION-1620-LV-6-BNC             | FW: x0031
TRION-1620-LV-6-L1B             | FW: x0031
TRION-1603-LV-6-BNC             | FW: x0A15
TRION-1603-LV-6-L1B             | FW: x0A15
TRION-1603-LV-6-D25             | FW: x0A15
TRION-1600-dLV-16-D             | FW: x1893
TRION-1600-dLV-16-D-CAN         | FW: x1893
TRION-1600-dLV-32-D             | FW: x1893
TRION-1600-dLV-32-D-CAN         | FW: x1893
TRION-1802-dLV-16-D             | FW: x1893
TRION-1802-dLV-16-D-CAN         | FW: x1893
TRION-1802-dLV-32-D             | FW: x1893
TRION-1802-dLV-32-D-CAN         | FW: x1893
TRION-1810-HV-4                 | FW: x0064
TRION-1810-HV-8                 | FW: x0064
TRION-1820-POWER-4              | FW: x0064
TRION-1810M-POWER-4             | FW: x0064
TRION-1820-MULTI-4-D            | FW: x0034
TRION-2402-MULTI-4-D            | FW: x0B18
TRION-2402-MULTI-8-L0B          | FW: x0A24
TRION-2402-MULTI-S1             | FW: x0034
TRION-2402-dSTG-6-L1B           | FW: x1120
TRION-2402-dSTG-6-L1B-S1        | FW: x1120
TRION-2402-dSTG-8-D             | FW: x1120
TRION-2402-dSTG-8-L0B           | FW: x1120
TRION-2402-dSTG-8-RJ            | FW: x1120
TRION-2400-dSTG-8-L0B           | FW: x1120
TRION-2400-dSTG-OEM             | FW: x1120
TRION-2402-dACC-6-BNC           | FW: x1119
TRION-2402-dACC-8-SMB           | FW: x1119
TRION-2402-dACC-8-MD            | FW: x1119
TRION-2402-V-4-B                | FW: x1017
TRION-2402-V-8-B                | FW: x1017
TRION-CNT-6-L1B                 | FW: x1119
TRION-BASE                      | FW: x1145
TRION-TIMING                    | FW: x1145
TRION-TIMING-V2                 | FW: x0004
TRION-TIMING-V3                 | FW: xF016   MCU: x00020095
TRION-VGPS-20                   | FW: x1145
TRION-VGPS-20-V3                | FW: xF016   MCU: x00020095
TRION-VGPS-100                  | FW: x1145
TRION-VGPS-100-V3               | FW: xF016   MCU: x00020095
TRION-CAN-4                     | FW: x1122
TRION-CAN-2                     | FW: x1122
TRION-DI-48                     | FW: x1119
TRION-DI-64-S1                  | FW: x0009

HW Support PUREC                | Firmware
--------------------------------|-----------
PUREC-200                       | FW: x1893
PUREC-50                        | FW: x1893

HW Support DEWE3 chassis        | Firmware
--------------------------------|-----------
DEWE3-PA8
DEWE3-A4
DEWE3-A4L
DEWE3-M4
DEWE3-RM4
DEWE3-RM8
DEWE3-RM12
DEWE3-RM16

HW Support DEWE2 chassis        | Firmware
--------------------------------|-----------
DEWE2-PA7
DEWE2-A4
DEWE2-A4L
DEWE2-A7
DEWE2-A13
DEWE2-M4
DEWE2-M4s
DEWE2-M7
DEWE2-M7s
DEWE2-M13
DEWE2-M13s
DEWE2-M18
DEWE2-F4s
DEWE2-F7s
DEWE2-F13s
DEWE2-F18
DEWE2-F4-THUNDERBOLT
DEWE2-F13-FIBRE
TRIONet
TrendCorder


## 2022-10-03 Release Notice DEWETRON TRION API R6.3.0

Revision: 655ab5b8196458b9086b22b58258346e0b08dc3d

Components                      | Version
--------------------------------|--------------------------
DEWETRON Explorer               | 6.3.0.63500
DEWETRON TRION API              | 6.3.0.63500
DEWETRON TRION driver           | 6.3.0.63500
DEWETRON DEWE2 driver           | 6.3.0.63500

## Files
DEWETRON-TRION-Applications-6.3.0.63500.exe

## Requirements
* Update all TRION modules to the latest firmware included in this release
* Use OXYGEN R6.3 or higher
* Windows 10 64-Bit or better

## Installation procedure
* Install TRION applications
* Reboot system (if requested by the installer)
* Start DEWETRON Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
* Power-cycle TRION boards (Power down system, then restart)
* Start DEWETRON Explorer and check for a successful firmware upgrade

## New Features and most important bugfixes:
* New chassis: DEWE3-A4L
* TRION3-1820-MULTI, TRION3-1850-MULTI
  - Current mode: 2mA range support added
* TRION-1820-MULTI
  - Current mode: 2mA range support added

## Known Limitations
* None

## Firmwares

HW Support TRION modules        | Firmware
--------------------------------|-----------
TRION3-1810M-POWER-4            | FW: x0072
TRION3-1810-SUB-8               | FW: x0015
TRION3-1820-MULTI-4-D           | FW: x0034
TRION3-1820-MULTI-8-L0B         | FW: x0034
TRION3-1850-MULTI-4-D           | FW: x0034
TRION3-1850-MULTI-8-L0B         | FW: x0034
TRION3-AOUT-8                   | FW: x0035
TRION-1620-ACC-6-BNC            | FW: x0031
TRION-1620-ACC-6-L1B            | FW: x0031
TRION-1620-LV-6-BNC             | FW: x0031
TRION-1620-LV-6-L1B             | FW: x0031
TRION-1603-LV-6-BNC             | FW: x0A15
TRION-1603-LV-6-L1B             | FW: x0A15
TRION-1603-LV-6-D25             | FW: x0A15
TRION-1600-dLV-16-D             | FW: x1893
TRION-1600-dLV-16-D-CAN         | FW: x1893
TRION-1600-dLV-32-D             | FW: x1893
TRION-1600-dLV-32-D-CAN         | FW: x1893
TRION-1802-dLV-16-D             | FW: x1893
TRION-1802-dLV-16-D-CAN         | FW: x1893
TRION-1802-dLV-32-D             | FW: x1893
TRION-1802-dLV-32-D-CAN         | FW: x1893
TRION-1810-HV-4                 | FW: x0072
TRION-1810-HV-8                 | FW: x0072
TRION-1820-POWER-4              | FW: x0072
TRION-1810M-POWER-4             | FW: x0072
TRION-1820-MULTI-4-D            | FW: x0034
TRION-2402-MULTI-4-D            | FW: x0B18
TRION-2402-MULTI-8-L0B          | FW: x0A24
TRION-2402-MULTI-S1             | FW: x0034
TRION-2402-dSTG-6-L1B           | FW: x1120
TRION-2402-dSTG-6-L1B-S1        | FW: x1120
TRION-2402-dSTG-8-D             | FW: x1120
TRION-2402-dSTG-8-L0B           | FW: x1120
TRION-2402-dSTG-8-RJ            | FW: x1120
TRION-2400-dSTG-8-L0B           | FW: x1120
TRION-2400-dSTG-OEM             | FW: x1120
TRION-2402-dACC-6-BNC           | FW: x1119
TRION-2402-dACC-8-SMB           | FW: x1119
TRION-2402-dACC-8-MD            | FW: x1119
TRION-2402-V-4-B                | FW: x1017
TRION-2402-V-8-B                | FW: x1017
TRION-CNT-6-L1B                 | FW: x1119
TRION-BASE                      | FW: x1145
TRION-TIMING                    | FW: x1145
TRION-TIMING-V2                 | FW: x0004
TRION-TIMING-V3                 | FW: xF016   MCU: x00020095
TRION-VGPS-20                   | FW: x1145
TRION-VGPS-20-V3                | FW: xF016   MCU: x00020095
TRION-VGPS-100                  | FW: x1145
TRION-VGPS-100-V3               | FW: xF016   MCU: x00020095
TRION-CAN-4                     | FW: x1122
TRION-CAN-2                     | FW: x1122
TRION-DI-48                     | FW: x1119
TRION-DI-64-S1                  | FW: x0009

HW Support PUREC                | Firmware
--------------------------------|-----------
PUREC-200                       | FW: x1893
PUREC-50                        | FW: x1893

HW Support DEWE3 chassis        | Firmware
--------------------------------|-----------
DEWE3-PA8
DEWE3-A4
DEWE3-A4L
DEWE3-M4
DEWE3-RM4
DEWE3-RM8
DEWE3-RM12
DEWE3-RM16

HW Support DEWE2 chassis        | Firmware
--------------------------------|-----------
DEWE2-PA7
DEWE2-A4
DEWE2-A4L
DEWE2-A7
DEWE2-A13
DEWE2-M4
DEWE2-M4s
DEWE2-M7
DEWE2-M7s
DEWE2-M13
DEWE2-M13s
DEWE2-M18
DEWE2-F4s
DEWE2-F7s
DEWE2-F13s
DEWE2-F18
DEWE2-F4-THUNDERBOLT
DEWE2-F13-FIBRE
TRIONet
TrendCorder



## 2022-07-15 Release Notice DEWETRON TRION API R6.2.1
Revision: 9fc52c1f65b49de1b08c5bdb8e08ac6a98189ae0

Components                      | Version
--------------------------------|--------------------------
DEWETRON Explorer               | 6.2.1.62584
DEWETRON TRION API              | 6.2.1.62584
DEWETRON TRION driver           | 6.2.1.62584
DEWETRON DEWE2 driver           | 6.2.1.62584
DEWE-TRION board information    | 1657802236
DEWE enclosure information      | 1657802236
DEWE-TRION firmware revisions   | 1657802236
DEWE-TRION TEDS default data    | 1657802236

## Files
DEWETRON-TRION-Applications-6.2.1.62584.exe

## Requirements
* Update all TRION modules to the latest firmware included in this release
* Use OXYGEN R6.2 or higher
* Windows 10 64-Bit or better

## Installation procedure
* Install TRION applications
* Reboot system (if requested by the installer)
* Start DEWETRON Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
* Power-cycle TRION boards (Power down system, then restart)
* Start DEWETRON Explorer and check for a successful firmware upgrade

## New Features and most important bugfixes:
* TRION3-18XX-POWER, TRION-18XX-POWER
  - Fixed phase error with current delay settings on 1MS ADCs.

## Known Limitations
* None

## Firmwares

HW Support TRION modules        | Firmware
--------------------------------|-----------
TRION3-1810M-POWER-4            | FW: x0070
TRION3-1810-SUB-8               | FW: x0015
TRION3-1820-MULTI-4-D           | FW: x0034
TRION3-1820-MULTI-8-L0B         | FW: x0034
TRION3-1850-MULTI-4-D           | FW: x0034
TRION3-1850-MULTI-8-L0B         | FW: x0034
TRION3-AOUT-8                   | FW: x0035
TRION-1620-ACC-6-BNC            | FW: x0031
TRION-1620-ACC-6-L1B            | FW: x0031
TRION-1620-LV-6-BNC             | FW: x0031
TRION-1620-LV-6-L1B             | FW: x0031
TRION-1603-LV-6-BNC             | FW: x0A15
TRION-1603-LV-6-L1B             | FW: x0A15
TRION-1603-LV-6-D25             | FW: x0A15
TRION-1600-dLV-16-D             | FW: x1893
TRION-1600-dLV-16-D-CAN         | FW: x1893
TRION-1600-dLV-32-D             | FW: x1893
TRION-1600-dLV-32-D-CAN         | FW: x1893
TRION-1802-dLV-16-D             | FW: x1893
TRION-1802-dLV-16-D-CAN         | FW: x1893
TRION-1802-dLV-32-D             | FW: x1893
TRION-1802-dLV-32-D-CAN         | FW: x1893
TRION-1810-HV-4                 | FW: x0070
TRION-1810-HV-8                 | FW: x0070
TRION-1820-POWER-4              | FW: x0070
TRION-1810M-POWER-4             | FW: x0070
TRION-1820-MULTI-4-D            | FW: x0034
TRION-2402-MULTI-4-D            | FW: x0B18
TRION-2402-MULTI-8-L0B          | FW: x0A24
TRION-2402-MULTI-S1             | FW: x0034
TRION-2402-dSTG-6-L1B           | FW: x1120
TRION-2402-dSTG-6-L1B-S1        | FW: x1120
TRION-2402-dSTG-8-D             | FW: x1120
TRION-2402-dSTG-8-L0B           | FW: x1120
TRION-2402-dSTG-8-RJ            | FW: x1120
TRION-2400-dSTG-8-L0B           | FW: x1120
TRION-2400-dSTG-OEM             | FW: x1120
TRION-2402-dACC-6-BNC           | FW: x1119
TRION-2402-dACC-8-SMB           | FW: x1119
TRION-2402-dACC-8-MD            | FW: x1119
TRION-2402-V-4-B                | FW: x1017
TRION-2402-V-8-B                | FW: x1017
TRION-CNT-6-L1B                 | FW: x1119
TRION-BASE                      | FW: x1145
TRION-TIMING                    | FW: x1145
TRION-TIMING-V2                 | FW: x0004
TRION-TIMING-V3                 | FW: xF016   MCU: x00020095
TRION-VGPS-20                   | FW: x1145
TRION-VGPS-20-V3                | FW: xF016   MCU: x00020095
TRION-VGPS-100                  | FW: x1145
TRION-VGPS-100-V3               | FW: xF016   MCU: x00020095
TRION-CAN-4                     | FW: x1122
TRION-CAN-2                     | FW: x1122
TRION-DI-48                     | FW: x1119
TRION-DI-64-S1                  | FW: x0009

HW Support PUREC                | Firmware
--------------------------------|-----------
PUREC-200                       | FW: x1893
PUREC-50                        | FW: x1893

HW Support DEWE3 chassis        | Firmware
--------------------------------|-----------
DEWE3-PA8
DEWE3-A4
DEWE3-M4
DEWE3-RM4
DEWE3-RM8
DEWE3-RM12
DEWE3-RM16

HW Support DEWE2 chassis        | Firmware
--------------------------------|-----------
DEWE2-PA7
DEWE2-A4
DEWE2-A4L
DEWE2-A7
DEWE2-A13
DEWE2-M4
DEWE2-M4s
DEWE2-M7
DEWE2-M7s
DEWE2-M13
DEWE2-M13s
DEWE2-M18
DEWE2-F4s
DEWE2-F7s
DEWE2-F13s
DEWE2-F18
DEWE2-F4-THUNDERBOLT
DEWE2-F13-FIBRE
TRIONet
TrendCorder


## 2022-07-04 Release Notice DEWETRON TRION API R6.2.0
Revision: 4e948c29615a94058afbc48c41609269f3b45105

Components                      | Version
--------------------------------|--------------------------
DEWETRON Explorer               | 6.2.0.62422
DEWETRON TRION API              | 6.2.0.62422
DEWETRON TRION driver           | 6.2.0.62422
DEWETRON DEWE2 driver           | 6.2.0.62422
DEWE-TRION board information    | 1656915922
DEWE enclosure information      | 1656915922
DEWE-TRION firmware revisions   | 1656915922
DEWE-TRION TEDS default data    | 1656915922

## Files
DEWETRON-TRION-Applications-6.2.0.62422.exe

## Requirements
* Update all TRION modules to the latest firmware included in this release
* Use OXYGEN R6.2 or higher
* Windows 10 64-Bit or better

## Installation procedure
* Install TRION applications
* Reboot system (if requested by the installer)
* Start DEWETRON Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
* Power-cycle TRION boards (Power down system, then restart)
* Start DEWETRON Explorer and check for a successful firmware upgrade

## New Features and most important bugfixes:
* TRION3-18XX-POWER, TRION-18XX-POWER
  - Fixed phase error with current delay settings on 1MS ADCs.

## Known Limitations
* None

## Firmwares

HW Support TRION modules        | Firmware
--------------------------------|-----------
TRION3-1810M-POWER-4            | FW: x0070
TRION3-1810-SUB-8               | FW: x0015
TRION3-1820-MULTI-4-D           | FW: x0034
TRION3-1820-MULTI-8-L0B         | FW: x0034
TRION3-1850-MULTI-4-D           | FW: x0034
TRION3-1850-MULTI-8-L0B         | FW: x0034
TRION3-AOUT-8                   | FW: x0035
TRION-1620-ACC-6-BNC            | FW: x0031
TRION-1620-ACC-6-L1B            | FW: x0031
TRION-1620-LV-6-BNC             | FW: x0031
TRION-1620-LV-6-L1B             | FW: x0031
TRION-1603-LV-6-BNC             | FW: x0A15
TRION-1603-LV-6-L1B             | FW: x0A15
TRION-1603-LV-6-D25             | FW: x0A15
TRION-1600-dLV-16-D             | FW: x1893
TRION-1600-dLV-16-D-CAN         | FW: x1893
TRION-1600-dLV-32-D             | FW: x1893
TRION-1600-dLV-32-D-CAN         | FW: x1893
TRION-1802-dLV-16-D             | FW: x1893
TRION-1802-dLV-16-D-CAN         | FW: x1893
TRION-1802-dLV-32-D             | FW: x1893
TRION-1802-dLV-32-D-CAN         | FW: x1893
TRION-1810-HV-4                 | FW: x0070
TRION-1810-HV-8                 | FW: x0070
TRION-1820-POWER-4              | FW: x0070
TRION-1810M-POWER-4             | FW: x0070
TRION-1820-MULTI-4-D            | FW: x0034
TRION-2402-MULTI-4-D            | FW: x0B18
TRION-2402-MULTI-8-L0B          | FW: x0A24
TRION-2402-MULTI-S1             | FW: x0034
TRION-2402-dSTG-6-L1B           | FW: x1120
TRION-2402-dSTG-6-L1B-S1        | FW: x1120
TRION-2402-dSTG-8-D             | FW: x1120
TRION-2402-dSTG-8-L0B           | FW: x1120
TRION-2402-dSTG-8-RJ            | FW: x1120
TRION-2400-dSTG-8-L0B           | FW: x1120
TRION-2400-dSTG-OEM             | FW: x1120
TRION-2402-dACC-6-BNC           | FW: x1119
TRION-2402-dACC-8-SMB           | FW: x1119
TRION-2402-dACC-8-MD            | FW: x1119
TRION-2402-V-4-B                | FW: x1017
TRION-2402-V-8-B                | FW: x1017
TRION-CNT-6-L1B                 | FW: x1119
TRION-BASE                      | FW: x1145
TRION-TIMING                    | FW: x1145
TRION-TIMING-V2                 | FW: x0004
TRION-TIMING-V3                 | FW: xF016   MCU: x00020095
TRION-VGPS-20                   | FW: x1145
TRION-VGPS-20-V3                | FW: xF016   MCU: x00020095
TRION-VGPS-100                  | FW: x1145
TRION-VGPS-100-V3               | FW: xF016   MCU: x00020095
TRION-CAN-4                     | FW: x1122
TRION-CAN-2                     | FW: x1122
TRION-DI-48                     | FW: x1119
TRION-DI-64-S1                  | FW: x0009

HW Support PUREC                | Firmware
--------------------------------|-----------
PUREC-200                       | FW: x1893
PUREC-50                        | FW: x1893

HW Support DEWE3 chassis        | Firmware
--------------------------------|-----------
DEWE3-PA8
DEWE3-A4
DEWE3-M4
DEWE3-RM4
DEWE3-RM8
DEWE3-RM12
DEWE3-RM16

HW Support DEWE2 chassis        | Firmware
--------------------------------|-----------
DEWE2-PA7
DEWE2-A4
DEWE2-A4L
DEWE2-A7
DEWE2-A13
DEWE2-M4
DEWE2-M4s
DEWE2-M7
DEWE2-M7s
DEWE2-M13
DEWE2-M13s
DEWE2-M18
DEWE2-F4s
DEWE2-F7s
DEWE2-F13s
DEWE2-F18
DEWE2-F4-THUNDERBOLT
DEWE2-F13-FIBRE
TRIONet
TrendCorder


## 2022-06-09 Release Notice DEWETRON TRION API R6.1.2

### Version: 6.1.2.61980
Revision: 7c5b9075153aaba5b65e886c97dcafbc832b7298

Components                      | Version
--------------------------------|--------------------------
DEWETRON Explorer               | 6.1.2.61980
DEWETRON TRION API              | 6.1.2.61980
DEWETRON TRION driver           | 6.1.2.61980
DEWETRON DEWE2 driver           | 6.1.2.61980
DEWE-TRION board information    | 1652781805
DEWE enclosure information      | 1652781805
DEWE-TRION firmware revisions   | 1652781805
DEWE-TRION TEDS default data    | 1652781805

## Files
DEWETRON-TRION-Applications-6.1.2.61980.exe

## Requirements
* Update all TRION modules to the latest firmware included in this release
* Use OXYGEN R6.1 or higher
* Windows 10 64-Bit or better

## Installation procedure
* Install TRION applications
* Reboot system (if requested by the installer)
* Start DEWETRON Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
* Power-cycle TRION boards (Power down system, then restart)
* Start DEWETRON Explorer and check for a successful firmware upgrade

## New Features and most important bugfixes:
* TRION3-18XX-POWER, TRION-18XX-POWER
  - Fixed slot 3 issues

## Known Limitations
* None

## Firmwares

HW Support TRION modules        | Firmware
--------------------------------|-----------
TRION3-1810M-POWER-4            | FW: x0069
TRION3-1810-SUB-8               | FW: x0015
TRION3-1820-MULTI-4-D           | FW: x0034
TRION3-1820-MULTI-8-L0B         | FW: x0034
TRION3-1850-MULTI-4-D           | FW: x0034
TRION3-1850-MULTI-8-L0B         | FW: x0034
TRION3-AOUT-8                   | FW: x0035
TRION-1620-ACC-6-BNC            | FW: x0031
TRION-1620-ACC-6-L1B            | FW: x0031
TRION-1620-LV-6-BNC             | FW: x0031
TRION-1620-LV-6-L1B             | FW: x0031
TRION-1603-LV-6-BNC             | FW: x0A15
TRION-1603-LV-6-L1B             | FW: x0A15
TRION-1603-LV-6-D25             | FW: x0A15
TRION-1600-dLV-16-D             | FW: x1893
TRION-1600-dLV-16-D-CAN         | FW: x1893
TRION-1600-dLV-32-D             | FW: x1893
TRION-1600-dLV-32-D-CAN         | FW: x1893
TRION-1802-dLV-16-D             | FW: x1893
TRION-1802-dLV-16-D-CAN         | FW: x1893
TRION-1802-dLV-32-D             | FW: x1893
TRION-1802-dLV-32-D-CAN         | FW: x1893
TRION-1810-HV-4                 | FW: x0069
TRION-1810-HV-8                 | FW: x0069
TRION-1820-POWER-4              | FW: x0069
TRION-1810M-POWER-4             | FW: x0069
TRION-1820-MULTI-4-D            | FW: x0034
TRION-2402-MULTI-4-D            | FW: x0B18
TRION-2402-MULTI-8-L0B          | FW: x0A24
TRION-2402-MULTI-S1             | FW: x0034
TRION-2402-dSTG-6-L1B           | FW: x1120
TRION-2402-dSTG-6-L1B-S1        | FW: x1120
TRION-2402-dSTG-8-D             | FW: x1120
TRION-2402-dSTG-8-L0B           | FW: x1120
TRION-2402-dSTG-8-RJ            | FW: x1120
TRION-2400-dSTG-8-L0B           | FW: x1120
TRION-2400-dSTG-OEM             | FW: x1120
TRION-2402-dACC-6-BNC           | FW: x1119
TRION-2402-dACC-8-SMB           | FW: x1119
TRION-2402-dACC-8-MD            | FW: x1119
TRION-2402-V-4-B                | FW: x1017
TRION-2402-V-8-B                | FW: x1017
TRION-CNT-6-L1B                 | FW: x1119
TRION-BASE                      | FW: x1145
TRION-TIMING                    | FW: x1145
TRION-TIMING-V2                 | FW: x0004
TRION-TIMING-V3                 | FW: xF016   MCU: x00020095
TRION-VGPS-20                   | FW: x1145
TRION-VGPS-20-V3                | FW: xF016   MCU: x00020095
TRION-VGPS-100                  | FW: x1145
TRION-VGPS-100-V3               | FW: xF016   MCU: x00020095
TRION-CAN-4                     | FW: x1122
TRION-CAN-2                     | FW: x1122
TRION-DI-48                     | FW: x1119
TRION-DI-64-S1                  | FW: x0009

HW Support PUREC                | Firmware
--------------------------------|-----------
PUREC-200                       | FW: x1893
PUREC-50                        | FW: x1893

HW Support DEWE3 chassis        | Firmware
--------------------------------|-----------
DEWE3-PA8
DEWE3-A4
DEWE3-M4
DEWE3-RM4
DEWE3-RM8
DEWE3-RM12
DEWE3-RM16

HW Support DEWE2 chassis        | Firmware
--------------------------------|-----------
DEWE2-PA7
DEWE2-A4
DEWE2-A4L
DEWE2-A7
DEWE2-A13
DEWE2-M4
DEWE2-M4s
DEWE2-M7
DEWE2-M7s
DEWE2-M13
DEWE2-M13s
DEWE2-M18
DEWE2-F4s
DEWE2-F7s
DEWE2-F13s
DEWE2-F18
DEWE2-F4-THUNDERBOLT
DEWE2-F13-FIBRE
TRIONet
TrendCorder


## 2022-05-02 Release Notice DEWETRON TRION API R6.1.1

### Version: 6.1.1.61787
Revision: 7d6539ff17f2b2d9902505ce46bc482f693ec7ee

Components                      | Version
--------------------------------|--------------------------
DEWETRON Explorer               | 6.1.1.61787
DEWETRON TRION API              | 6.1.1.61787
DEWETRON TRION driver           | 6.1.1.61787
DEWETRON DEWE2 driver           | 6.1.1.61787
DEWE-TRION board information    | 1651058316
DEWE enclosure information      | 1651058316
DEWE-TRION firmware revisions   | 1651058316
DEWE-TRION TEDS default data    | 1651058316

## Files
DEWETRON-TRION-Applications-6.1.1.61787.exe

## Requirements
* Update all TRION modules to the latest firmware included in this release
* Use OXYGEN R6.1 or higher
* Windows 10 64-Bit or better

## Installation procedure
* Install TRION applications
* Reboot system (if requested by the installer)
* Start DEWETRON Explorer and update each TRION board firmware to latest version (right-click on enclosure name)
* Power-cycle TRION boards (Power down system, then restart)
* Start DEWETRON Explorer and check for a successful firmware upgrade

## New Features and most important bugfixes:
* TRION3-18XX-MULTI, TRION-18XX-MULTI
  - Fix for CAN delay issue with FW 0x0033

## Known Limitations
* None

## Firmwares

HW Support TRION modules        | Firmware
--------------------------------|-----------
TRION3-1810M-POWER-4            | FW: x0068
TRION3-1810-SUB-8               | FW: x0015
TRION3-1820-MULTI-4-D           | FW: x0034
TRION3-1820-MULTI-8-L0B         | FW: x0034
TRION3-1850-MULTI-4-D           | FW: x0034
TRION3-1850-MULTI-8-L0B         | FW: x0034
TRION3-AOUT-8                   | FW: x0035
TRION-1620-ACC-6-BNC            | FW: x0031
TRION-1620-ACC-6-L1B            | FW: x0031
TRION-1620-LV-6-BNC             | FW: x0031
TRION-1620-LV-6-L1B             | FW: x0031
TRION-1603-LV-6-BNC             | FW: x0A15
TRION-1603-LV-6-L1B             | FW: x0A15
TRION-1603-LV-6-D25             | FW: x0A15
TRION-1600-dLV-16-D             | FW: x1893
TRION-1600-dLV-16-D-CAN         | FW: x1893
TRION-1600-dLV-32-D             | FW: x1893
TRION-1600-dLV-32-D-CAN         | FW: x1893
TRION-1802-dLV-16-D             | FW: x1893
TRION-1802-dLV-16-D-CAN         | FW: x1893
TRION-1802-dLV-32-D             | FW: x1893
TRION-1802-dLV-32-D-CAN         | FW: x1893
TRION-1810-HV-4                 | FW: x0068
TRION-1810-HV-8                 | FW: x0068
TRION-1820-POWER-4              | FW: x0068
TRION-1810M-POWER-4             | FW: x0068
TRION-1820-MULTI-4-D            | FW: x0034
TRION-2402-MULTI-4-D            | FW: x0B18
TRION-2402-MULTI-8-L0B          | FW: x0A24
TRION-2402-MULTI-S1             | FW: x0034
TRION-2402-dSTG-6-L1B           | FW: x1120
TRION-2402-dSTG-6-L1B-S1        | FW: x1120
TRION-2402-dSTG-8-D             | FW: x1120
TRION-2402-dSTG-8-L0B           | FW: x1120
TRION-2402-dSTG-8-RJ            | FW: x1120
TRION-2400-dSTG-8-L0B           | FW: x1120
TRION-2400-dSTG-OEM             | FW: x1120
TRION-2402-dACC-6-BNC           | FW: x1119
TRION-2402-dACC-8-SMB           | FW: x1119
TRION-2402-dACC-8-MD            | FW: x1119
TRION-2402-V-4-B                | FW: x1017
TRION-2402-V-8-B                | FW: x1017
TRION-CNT-6-L1B                 | FW: x1119
TRION-BASE                      | FW: x1145
TRION-TIMING                    | FW: x1145
TRION-TIMING-V2                 | FW: x0004
TRION-TIMING-V3                 | FW: xF016   MCU: x00020095
TRION-VGPS-20                   | FW: x1145
TRION-VGPS-20-V3                | FW: xF016   MCU: x00020095
TRION-VGPS-100                  | FW: x1145
TRION-VGPS-100-V3               | FW: xF016   MCU: x00020095
TRION-CAN-4                     | FW: x1122
TRION-CAN-2                     | FW: x1122
TRION-DI-48                     | FW: x1119
TRION-DI-64-S1                  | FW: x0009

HW Support PUREC                | Firmware
--------------------------------|-----------
PUREC-200                       | FW: x1893
PUREC-50                        | FW: x1893

HW Support DEWE3 chassis        | Firmware
--------------------------------|-----------
DEWE3-PA8
DEWE3-A4
DEWE3-M4
DEWE3-RM4
DEWE3-RM8
DEWE3-RM12
DEWE3-RM16

HW Support DEWE2 chassis        | Firmware
--------------------------------|-----------
DEWE2-PA7
DEWE2-A4
DEWE2-A4L
DEWE2-A7
DEWE2-A13
DEWE2-M4
DEWE2-M4s
DEWE2-M7
DEWE2-M7s
DEWE2-M13
DEWE2-M13s
DEWE2-M18
DEWE2-F4s
DEWE2-F7s
DEWE2-F13s
DEWE2-F18
DEWE2-F4-THUNDERBOLT
DEWE2-F13-FIBRE
TRIONet
TrendCorder
